; bhtsddr.inf, BHT Integrated MMC/SD Controller INF file
; Copyright (c) BHT Corp. 
; for Win10/Win11

[Version]
Signature   = "$Windows NT$"
Class       = SCSIAdapter
ClassGuid   = {4D36E97B-E325-11CE-BFC1-08002BE10318}
Provider    = %BayHubTech%
DriverVer = 12/22/2021,2.1.101.10550
Catalogfile = bhtsddr.cat

[SourceDisksNames]
1 = %bhtsddr.DriverDisk%

[SourceDisksFiles]
bhtsddr.sys = 1
bhtv5Icon.dll = 1

[DestinationDirs]
DefaultDestDir = 12
Copybhtv5Icon = 11
Copybhtv5Icon_WoW64 = 10, sysWoW64

[ControlFlags]
ExcludeFromSelect = *

[Manufacturer]
%BayHubTech% = bhtsddr,NTamd64.10.0...19042,NTx86.10.0...19042


[bhtsddr.NTx86.10.0...19042]
%bhtsddr.Generic_DeviceDesc% = DriverInstallx86, PCI\VEN_1217&DEV_8520		;Default for Fujin2
%bhtsddr.Generic_DeviceDesc% = DriverInstallx86, PCI\VEN_1217&DEV_8420		;Default for SDS0
%bhtsddr.Generic_DeviceDesc% = DriverInstallx86, PCI\VEN_1217&DEV_8421		;Default for SDS1
%bhtsddr.Generic_DeviceDesc% = DriverInstallx86, PCI\VEN_1217&DEV_8620		;Default for Seabird
%bhtsddr.Generic_DeviceDesc% = DriverInstallx86, PCI\VEN_1217&DEV_8621		;Default for Seabird
%bhtsddr.Generic_DeviceDesc% = DriverInstallx86, PCI\VEN_1217&DEV_8720		;Default for SeaEagle2
%bhtsddr.Generic_DeviceDesc% = DriverInstallx86, PCI\VEN_1217&DEV_8721		;Default for SeaEagle2
%bhtsddr.Generic_DeviceDesc% = DriverInstallx86, PCI\VEN_1217&DEV_8722		;Default for SeaEagle2
%bhtsddr.Generic_DeviceDesc% = DriverInstallx86, PCI\VEN_1217&DEV_8723		;Default for SeaEagle2

%bhtsddr.DeviceDesc% = DriverInstallx86_221117aa, PCI\VEN_1217&DEV_8520&SUBSYS_221117aa ;idx 1
%bhtsddr.DeviceDesc% = DriverInstallx86_504117aa, PCI\VEN_1217&DEV_8620&SUBSYS_504117aa ;idx 2,3
%bhtsddr.DeviceDesc% = DriverInstallx86_504c17aa, PCI\VEN_1217&DEV_8520&SUBSYS_504c17aa ;idx 4
%bhtsddr.DeviceDesc% = DriverInstallx86_222c17aa, PCI\VEN_1217&DEV_8621&SUBSYS_222c17aa ;idx 5
%bhtsddr.DeviceDesc% = DriverInstallx86_380017aa, PCI\VEN_1217&DEV_8620&SUBSYS_380017aa ;idx 6
%bhtsddr.DeviceDesc% = DriverInstallx86_380117aa, PCI\VEN_1217&DEV_8620&SUBSYS_380117aa ;idx 7
%bhtsddr.DeviceDesc% = DriverInstallx86_380017aa_8621, PCI\VEN_1217&DEV_8621&SUBSYS_380017aa ;idx 8
%bhtsddr.DeviceDesc% = DriverInstallx86_390317aa, PCI\VEN_1217&DEV_8621&SUBSYS_390317aa ;idx 9
%bhtsddr.DeviceDesc% = DriverInstallx86_390217aa, PCI\VEN_1217&DEV_8621&SUBSYS_390217aa   ;idx 10
%bhtsddr.DeviceDesc% = DriverInstallx86_06EF1028, PCI\VEN_1217&DEV_8520&SUBSYS_06EF1028 ;idx 13
%bhtsddr.DeviceDesc% = DriverInstallx86_380017aa_8520, PCI\VEN_1217&DEV_8520&SUBSYS_380017aa ;idx 14
%bhtsddr.DeviceDesc% = DriverInstallx86_b28219da, PCI\VEN_1217&DEV_8520&SUBSYS_b28219da ;idx 15
%bhtsddr.DeviceDesc% = DriverInstallx86_10521025, PCI\VEN_1217&DEV_8621&SUBSYS_10521025 ;idx 16
%bhtsddr.DeviceDesc% = DriverInstallx86_10631025, PCI\VEN_1217&DEV_8621&SUBSYS_10631025 ;idx 17
%bhtsddr.DeviceDesc% = DriverInstallx86_000417aa, PCI\VEN_1217&DEV_8620&SUBSYS_000417aa ;idx 18
%bhtsddr.DeviceDesc% = DriverInstallx86_505b17aa, PCI\VEN_1217&DEV_8621&SUBSYS_505b17aa ;idx 19
%bhtsddr.DeviceDesc% = DriverInstallx86_511817aa, PCI\VEN_1217&DEV_8621&SUBSYS_511817aa ;idx 20
%bhtsddr.DeviceDesc% = DriverInstallx86_505c17aa, PCI\VEN_1217&DEV_8621&SUBSYS_505c17aa ;idx 21
%bhtsddr.DeviceDesc% = DriverInstallx86_609517aa, PCI\VEN_1217&DEV_8520&SUBSYS_609517aa ;idx 22
%bhtsddr.DeviceDesc% = DriverInstallx86_607E17aa, PCI\VEN_1217&DEV_8520&SUBSYS_607E17aa ;idx 23
%bhtsddr.DeviceDesc% = DriverInstallx86_369417aa, PCI\VEN_1217&DEV_8520&SUBSYS_369417aa ;idx 24
%bhtsddr.DeviceDesc% = DriverInstallx86_505417aa, PCI\VEN_1217&DEV_8520&SUBSYS_505417aa ;idx 25
%bhtsddr.DeviceDesc% = DriverInstallx86_380317aa, PCI\VEN_1217&DEV_8620&SUBSYS_380317aa ;idx 26
%bhtsddr.DeviceDesc% = DriverInstallx86_20648086, PCI\VEN_1217&DEV_8621&SUBSYS_20648086 ;idx 27
%bhtsddr.DeviceDesc% = DriverInstallx86_380117aa_8621, PCI\VEN_1217&DEV_8621&SUBSYS_380117aa ;idx 30
%bhtsddr.DeviceDesc% = DriverInstallx86_380217aa, PCI\VEN_1217&DEV_8621&SUBSYS_380217aa ;idx 31
%bhtsddr.DeviceDesc% = DriverInstallx86_380417aa, PCI\VEN_1217&DEV_8620&SUBSYS_380417aa ;idx 32
%bhtsddr.DeviceDesc% = DriverInstallx86_60ae17aa, PCI\VEN_1217&DEV_8520&SUBSYS_60ae17aa ;idx 33
%bhtsddr.DeviceDesc% = DriverInstallx86_06251028, PCI\VEN_1217&DEV_8520&SUBSYS_06251028 ;idx 34
%bhtsddr.DeviceDesc% = DriverInstallx86_06261028, PCI\VEN_1217&DEV_8520&SUBSYS_06261028 ;idx 35
%bhtsddr.DeviceDesc% = DriverInstallx86_060f1028, PCI\VEN_1217&DEV_8520&SUBSYS_060f1028 ;idx 36
%bhtsddr.DeviceDesc% = DriverInstallx86_062f1028, PCI\VEN_1217&DEV_8520&SUBSYS_062f1028 ;idx 37
%bhtsddr.DeviceDesc% = DriverInstallx86_06101028, PCI\VEN_1217&DEV_8520&SUBSYS_06101028 ;idx 38
%bhtsddr.DeviceDesc% = DriverInstallx86_224917aa, PCI\VEN_1217&DEV_8621&SUBSYS_224917aa ;idx 39
%bhtsddr.DeviceDesc% = DriverInstallx86_224a17aa, PCI\VEN_1217&DEV_8621&SUBSYS_224a17aa ;idx 40
%bhtsddr.DeviceDesc% = DriverInstallx86_506617aa, PCI\VEN_1217&DEV_8520&SUBSYS_506617aa ;idx 41
%bhtsddr.DeviceDesc% = DriverInstallx86_381f17aa, PCI\VEN_1217&DEV_8621&SUBSYS_381f17aa ;idx 47
%bhtsddr.DeviceDesc% = DriverInstallx86_382017aa, PCI\VEN_1217&DEV_8621&SUBSYS_382017aa ;idx 48
%bhtsddr.DeviceDesc% = DriverInstallx86_388117aa, PCI\VEN_1217&DEV_8520&SUBSYS_388117aa ;idx 49
%bhtsddr.DeviceDesc% = DriverInstallx86_380317aa_8621, PCI\VEN_1217&DEV_8621&SUBSYS_380317aa ;idx 50
%bhtsddr.DeviceDesc% = DriverInstallx86_381217aa, PCI\VEN_1217&DEV_8620&SUBSYS_381217aa ;idx 51
%bhtsddr.DeviceDesc% = DriverInstallx86_740017aa, PCI\VEN_1217&DEV_8621&SUBSYS_740017aa ;idx 52
%bhtsddr.DeviceDesc% = DriverInstallx86_381c17aa, PCI\VEN_1217&DEV_8621&SUBSYS_381c17aa ;idx 53
%bhtsddr.DeviceDesc% = DriverInstallx86_11881025, PCI\VEN_1217&DEV_8621&SUBSYS_11881025 ;idx 54
%bhtsddr.DeviceDesc% = DriverInstallx86_11891025, PCI\VEN_1217&DEV_8621&SUBSYS_11891025 ;idx 55
%bhtsddr.DeviceDesc% = DriverInstallx86_506817aa, PCI\VEN_1217&DEV_8621&SUBSYS_506817aa ;idx 56
%bhtsddr.DeviceDesc% = DriverInstallx86_380517aa, PCI\VEN_1217&DEV_8621&SUBSYS_380517aa ;idx 57
%bhtsddr.DeviceDesc% = DriverInstallx86_506a17aa, PCI\VEN_1217&DEV_8621&SUBSYS_506a17aa ;idx 58
%bhtsddr.DeviceDesc% = DriverInstallx86_506f17aa, PCI\VEN_1217&DEV_8621&SUBSYS_506f17aa ;idx 59
%bhtsddr.DeviceDesc% = DriverInstallx86_60cd17aa, PCI\VEN_1217&DEV_8621&SUBSYS_60cd17aa ;idx 60
%bhtsddr.DeviceDesc% = DriverInstallx86_380717aa, PCI\VEN_1217&DEV_8621&SUBSYS_380717aa ;idx 61
%bhtsddr.DeviceDesc% = DriverInstallx86_226117aa, PCI\VEN_1217&DEV_8621&SUBSYS_226117aa ;idx 62
%bhtsddr.DeviceDesc% = DriverInstallx86_20738086, PCI\VEN_1217&DEV_8621&SUBSYS_20738086 ;idx 63
%bhtsddr.DeviceDesc_SD% = DriverInstallx86_12301025, PCI\VEN_1217&DEV_8621&SUBSYS_12301025 ;idx 64
%bhtsddr.DeviceDesc% = DriverInstallx86_380617aa, PCI\VEN_1217&DEV_8621&SUBSYS_380617aa ;idx 65
%bhtsddr.DeviceDesc% = DriverInstallx86_380417aa_8621, PCI\VEN_1217&DEV_8621&SUBSYS_380417aa ;idx 66
%bhtsddr.DeviceDesc% = DriverInstallx86_380817aa, PCI\VEN_1217&DEV_8621&SUBSYS_380817aa ;idx 67
%bhtsddr.DeviceDesc% = DriverInstallx86_384617aa, PCI\VEN_1217&DEV_8621&SUBSYS_384617aa ;idx 68
%bhtsddr.DeviceDesc% = DriverInstallx86_227317aa, PCI\VEN_1217&DEV_8621&SUBSYS_227317aa ;idx 69
%bhtsddr.DeviceDesc% = DriverInstallx86_380917aa, PCI\VEN_1217&DEV_8621&SUBSYS_380917aa ;idx 70
%bhtsddr.DeviceDesc% = DriverInstallx86_39F617aa, PCI\VEN_1217&DEV_8621&SUBSYS_39F617aa ;idx 71 for Compal EL451 EL4C1
%bhtsddr.DeviceDesc% = DriverInstallx86_381317aa, PCI\VEN_1217&DEV_8621&SUBSYS_381317aa ;idx 72 for Compal EL431 EL531 EL5C3
%bhtsddr.DeviceDesc% = DriverInstallx86_382417aa, PCI\VEN_1217&DEV_8621&SUBSYS_382417aa ;idx 73 for Compal EL452 EL4C2
%bhtsddr.DeviceDesc% = DriverInstallx86_382117aa, PCI\VEN_1217&DEV_8621&SUBSYS_382117aa ;idx 74 for Compal EL432 EL532
%bhtsddr.DeviceDesc% = DriverInstallx86_507517aa, PCI\VEN_1217&DEV_8621&SUBSYS_507517aa ;idx 75
%bhtsddr.DeviceDesc% = DriverInstallx86_383e17aa, PCI\VEN_1217&DEV_8621&SUBSYS_383e17aa ;idx 76 for Compal S740   Support Modernstandby
%bhtsddr.DeviceDesc% = DriverInstallx86_381817aa, PCI\VEN_1217&DEV_8621&SUBSYS_381817aa ;idx 77 for Lenovo
%bhtsddr.DeviceDesc% = DriverInstallx86_381417aa, PCI\VEN_1217&DEV_8621&SUBSYS_381417aa ;idx 78 for Lenovo
%bhtsddr.DeviceDesc% = DriverInstallx86_380f17aa, PCI\VEN_1217&DEV_8621&SUBSYS_380f17aa ;idx 79 for Lenovo        Support Modernstandby
%bhtsddr.DeviceDesc% = DriverInstallx86_507217aa, PCI\VEN_1217&DEV_8621&SUBSYS_507217aa ;idx 80 for Lenovo WU issue
%bhtsddr.DeviceDesc% = DriverInstallx86_383717aa, PCI\VEN_1217&DEV_8621&SUBSYS_383717aa ;idx 81 for Lenovo C340
%bhtsddr.DeviceDesc% = DriverInstallx86_3a3b17aa, PCI\VEN_1217&DEV_8621&SUBSYS_3a3b17aa ;idx 82 for Lenovo C340S340 for ICL 
%bhtsddr.DeviceDesc% = DriverInstallx86_383517aa, PCI\VEN_1217&DEV_8621&SUBSYS_383517aa ;idx 83 for Lenovo FLMS0  Support Modernstandby
%bhtsddr.DeviceDesc% = DriverInstallx86_382F17aa, PCI\VEN_1217&DEV_8621&SUBSYS_382F17aa ;idx 84 for Lenovo V340 14
%bhtsddr.DeviceDesc% = DriverInstallx86_383217aa, PCI\VEN_1217&DEV_8621&SUBSYS_383217aa ;idx 85 for Lenovo V340 15
%bhtsddr.DeviceDesc% = DriverInstallx86_385217aa, PCI\VEN_1217&DEV_8621&SUBSYS_385217aa ;idx 86 for Lenovo V340 IIL 14
%bhtsddr.DeviceDesc% = DriverInstallx86_385117aa, PCI\VEN_1217&DEV_8621&SUBSYS_385117aa ;idx 87 for Lenovo V340 IIL 15
%bhtsddr.DeviceDesc% = DriverInstallx86_507c17aa, PCI\VEN_1217&DEV_8621&SUBSYS_507c17aa ;idx 88 for Lenovo L43829A0L5A0
%bhtsddr.DeviceDesc% = DriverInstallx86_381617aa, PCI\VEN_1217&DEV_8621&SUBSYS_381617aa ;idx 89 for Lenovo C350-11
%bhtsddr.DeviceDesc% = DriverInstallx86_507e17aa, PCI\VEN_1217&DEV_8621&SUBSYS_507e17aa ;idx 90 for Lenovo Odin Thor
%bhtsddr.DeviceDesc% = DriverInstallx86_383117aa, PCI\VEN_1217&DEV_8621&SUBSYS_383117aa ;idx 91 for Lenovo FLMA0
%bhtsddr.DeviceDesc% = DriverInstallx86_381b17aa, PCI\VEN_1217&DEV_8621&SUBSYS_381b17aa ;idx 92 for Lenovo C550-14AMD
%bhtsddr.DeviceDesc% = DriverInstallx86_382517aa, PCI\VEN_1217&DEV_8621&SUBSYS_382517aa ;idx 93 for Lenovo Ideapad Duet3 D350
%bhtsddr.DeviceDesc% = DriverInstallx86_381717aa, PCI\VEN_1217&DEV_8621&SUBSYS_381717aa ;idx 94 for Lenovo C550-14Intel
%bhtsddr.DeviceDesc% = DriverInstallx86_382217aa, PCI\VEN_1217&DEV_8621&SUBSYS_382217aa ;idx 95 for Lenovo Yoga duet7 D550
%bhtsddr.DeviceDesc% = DriverInstallx86_383d17aa, PCI\VEN_1217&DEV_8621&SUBSYS_383d17aa ;idx 96 for Lenovo GLY5U
%bhtsddr.DeviceDesc% = DriverInstallx86_507b17aa, PCI\VEN_1217&DEV_8621&SUBSYS_507b17aa ;idx 97 for Lenovo LIA
%bhtsddr.DeviceDesc% = DriverInstallx86_381917aa, PCI\VEN_1217&DEV_8621&SUBSYS_381917aa ;idx 98 for Lenovo Y550
%bhtsddr.DeviceDesc% = DriverInstallx86_512417aa, PCI\VEN_1217&DEV_8621&SUBSYS_512417aa ;idx 99 for Lenovo EX95
%bhtsddr.DeviceDesc% = DriverInstallx86_383a17aa, PCI\VEN_1217&DEV_8621&SUBSYS_383a17aa ;idx 100 for Lenovo V350_Titan Intel platform
%bhtsddr.DeviceDesc% = DriverInstallx86_382717aa, PCI\VEN_1217&DEV_8621&SUBSYS_382717aa ;idx 101 for Lenovo V350_Titan AMD platform
%bhtsddr.DeviceDesc% = DriverInstallx86_380a17aa, PCI\VEN_1217&DEV_8621&SUBSYS_380a17aa ;idx 102 for Lenovo Y750S
%bhtsddr.DeviceDesc% = DriverInstallx86_383917aa, PCI\VEN_1217&DEV_8621&SUBSYS_383917aa ;idx 103 for Lenovo Compal GLMS1
%bhtsddr.DeviceDesc% = DriverInstallx86_382617aa, PCI\VEN_1217&DEV_8621&SUBSYS_382617aa ;idx 104 for Lenovo
%bhtsddr.DeviceDesc% = DriverInstallx86_382917aa, PCI\VEN_1217&DEV_8621&SUBSYS_382917aa ;idx 105 for Lenovo 100e 300e 2rd 
%bhtsddr.DeviceDesc% = DriverInstallx86_509317aa, PCI\VEN_1217&DEV_8621&SUBSYS_509317aa ;idx 106 for Lenovo Yoga Gen 6 
%bhtsddr.DeviceDesc% = DriverInstallx86_508f17aa, PCI\VEN_1217&DEV_8621&SUBSYS_508f17aa ;idx 107 for Lenovo Odin2.0 Thor2.0
%bhtsddr.DeviceDesc% = DriverInstallx86_382817aa, PCI\VEN_1217&DEV_8621&SUBSYS_382817aa ;idx 108 for Lenovo LC56-14TGL
%bhtsddr.DeviceDesc% = DriverInstallx86_382b17aa, PCI\VEN_1217&DEV_8621&SUBSYS_382b17aa ;idx 109 for Lenovo Y750A+N
%bhtsddr.DeviceDesc% = DriverInstallx86_382d17aa, PCI\VEN_1217&DEV_8621&SUBSYS_382d17aa ;idx 110 for Lenovo 300W Gen3 JPL
%bhtsddr.DeviceDesc% = DriverInstallx86_383c17aa, PCI\VEN_1217&DEV_8621&SUBSYS_383c17aa ;idx 111 for Lenovo GLI42
%bhtsddr.DeviceDesc% = DriverInstallx86_509117aa, PCI\VEN_1217&DEV_8621&SUBSYS_509117aa ;idx 112 for Lenovo Odin2.0 Thor2.0 AMD update
%bhtsddr.DeviceDesc% = DriverInstallx86_383317aa, PCI\VEN_1217&DEV_8621&SUBSYS_383317aa ;idx 113 for Lenovo D330-10IGL
%bhtsddr.DeviceDesc% = DriverInstallx86_383017aa, PCI\VEN_1217&DEV_8621&SUBSYS_383017aa ;idx 114 for Lenovo LC56 AMD
%bhtsddr.DeviceDesc% = DriverInstallx86_383b17aa, PCI\VEN_1217&DEV_8621&SUBSYS_383b17aa ;idx 115 for Lenovo V350_Titan
%bhtsddr.DeviceDesc% = DriverInstallx86_383417aa, PCI\VEN_1217&DEV_8621&SUBSYS_383417aa ;idx 116 for Lenovo S560-16 ITL 
%bhtsddr.DeviceDesc% = DriverInstallx86_383f17aa, PCI\VEN_1217&DEV_8621&SUBSYS_383f17aa ;idx 117 for Lenovo S560-16ACN
%bhtsddr.DeviceDesc% = DriverInstallx86_384017aa, PCI\VEN_1217&DEV_8621&SUBSYS_384017aa ;idx 118 for Lenovo V350_Titan 
%bhtsddr.DeviceDesc% = DriverInstallx86_384117aa, PCI\VEN_1217&DEV_8621&SUBSYS_384117aa ;idx 119 for Lenovo D760
%bhtsddr.DeviceDesc% = DriverInstallx86_384417aa, PCI\VEN_1217&DEV_8621&SUBSYS_384417aa ;idx 120 for Lenovo Thinkbook 14P
%bhtsddr.DeviceDesc% = DriverInstallx86_384517aa, PCI\VEN_1217&DEV_8621&SUBSYS_384517aa ;idx 121 for Lenovo Thinkbook 16P
%bhtsddr.DeviceDesc% = DriverInstallx86_384717aa, PCI\VEN_1217&DEV_8621&SUBSYS_384717aa ;idx 122 for Lenovo Y560ITH
%bhtsddr.DeviceDesc% = DriverInstallx86_384917aa, PCI\VEN_1217&DEV_8621&SUBSYS_384917aa ;idx 123 for Lenovo 100E/300E
%bhtsddr.DeviceDesc% = DriverInstallx86_384b17aa, PCI\VEN_1217&DEV_8621&SUBSYS_384b17aa ;idx 124 for Lenovo Y760S
%bhtsddr.DeviceDesc% = DriverInstallx86_384c17aa, PCI\VEN_1217&DEV_8621&SUBSYS_384c17aa ;idx 125 for Lenovo Y550IMH
%bhtsddr.DeviceDesc% = DriverInstallx86_50e11558, PCI\VEN_1217&DEV_8621&SUBSYS_50e11558 ;idx 126 for Clevo
%bhtsddr.DeviceDesc% = DriverInstallx86_50e21558, PCI\VEN_1217&DEV_8621&SUBSYS_50e21558 ;idx 127 for Clevo
%bhtsddr.DeviceDesc% = DriverInstallx86_50151558, PCI\VEN_1217&DEV_8621&SUBSYS_50151558 ;idx 128 for Clevo
%bhtsddr.DeviceDesc% = DriverInstallx86_50171558, PCI\VEN_1217&DEV_8621&SUBSYS_50171558 ;idx 129 for Clevo
%bhtsddr.DeviceDesc% = DriverInstallx86_866b1558, PCI\VEN_1217&DEV_8621&SUBSYS_866b1558 ;idx 130 for Clevo
%bhtsddr.DeviceDesc% = DriverInstallx86_867b1558, PCI\VEN_1217&DEV_8621&SUBSYS_867b1558 ;idx 131 for Clevo
%bhtsddr.DeviceDesc% = DriverInstallx86_00021217, PCI\VEN_1217&DEV_8621&SUBSYS_00021217 ;idx 132 for OZ711LV2 default ID update for Clevo AMD
%bhtsddr.DeviceDesc% = DriverInstallx86_85111558, PCI\VEN_1217&DEV_8621&SUBSYS_85111558 ;idx 133 for Clevo
%bhtsddr.DeviceDesc% = DriverInstallx86_87111558, PCI\VEN_1217&DEV_8621&SUBSYS_87111558 ;idx 134 for Clevo
%bhtsddr.DeviceDesc% = DriverInstallx86_50f41558, PCI\VEN_1217&DEV_8621&SUBSYS_50f41558 ;idx 135 for Clevo
%bhtsddr.DeviceDesc% = DriverInstallx86_50c51558, PCI\VEN_1217&DEV_8621&SUBSYS_50c51558 ;idx 136 for Clevo
%bhtsddr.DeviceDesc% = DriverInstallx86_51a11558, PCI\VEN_1217&DEV_8621&SUBSYS_51a11558 ;idx 137 for Clevo TGL-U
%bhtsddr.DeviceDesc% = DriverInstallx86_a5001558, PCI\VEN_1217&DEV_8621&SUBSYS_a5001558 ;idx 138 for Clevo Renoir
%bhtsddr.DeviceDesc% = DriverInstallx86_a6001558, PCI\VEN_1217&DEV_8621&SUBSYS_a6001558 ;idx 139 for Clevo Ryzen
%bhtsddr.DeviceDesc% = DriverInstallx86_40301558, PCI\VEN_1217&DEV_8621&SUBSYS_40301558 ;idx 140 for Clevo NV40Mx
%bhtsddr.DeviceDesc% = DriverInstallx86_14A11558, PCI\VEN_1217&DEV_8621&SUBSYS_14A11558 ;idx 141 for Clevo L140MU
%bhtsddr.DeviceDesc% = DriverInstallx86_384f17aa, PCI\VEN_1217&DEV_8621&SUBSYS_384f17aa ;idx 142 for Lenovo S170-Dali
%bhtsddr.DeviceDesc% = DriverInstallx86_e2071071, PCI\VEN_1217&DEV_8621&SUBSYS_e2071071 ;idx 143 for Getac F110G6
%bhtsddr.DeviceDesc% = DriverInstallx86_a1211071, PCI\VEN_1217&DEV_8621&SUBSYS_a1211071 ;idx 144 for Getac K120G2
%bhtsddr.DeviceDesc% = DriverInstallx86_40151071, PCI\VEN_1217&DEV_8621&SUBSYS_40151071 ;idx 145 for Getac S410G4
%bhtsddr.DeviceDesc% = DriverInstallx86_a2521071, PCI\VEN_1217&DEV_8621&SUBSYS_a2521071 ;idx 146 for Getac Raptor
%bhtsddr.DeviceDesc% = DriverInstallx86_b3601071, PCI\VEN_1217&DEV_8621&SUBSYS_b3601071 ;idx 147 for Getac B360
%bhtsddr.DeviceDesc% = DriverInstallx86_e2051071, PCI\VEN_1217&DEV_8621&SUBSYS_e2051071 ;idx 148 for Getac F110G5
%bhtsddr.DeviceDesc% = DriverInstallx86_a1201071, PCI\VEN_1217&DEV_8621&SUBSYS_a1201071 ;idx 149 for Getac K120
%bhtsddr.DeviceDesc% = DriverInstallx86_d3001071, PCI\VEN_1217&DEV_8621&SUBSYS_d3001071 ;idx 150 for Getac UX10G1
%bhtsddr.DeviceDesc% = DriverInstallx86_d3011071, PCI\VEN_1217&DEV_8621&SUBSYS_d3011071 ;idx 151 for Getac UX10G2
%bhtsddr.DeviceDesc% = DriverInstallx86_a1901071, PCI\VEN_1217&DEV_8621&SUBSYS_a1901071 ;idx 152 for Getac V110G5
%bhtsddr.DeviceDesc% = DriverInstallx86_a1911071, PCI\VEN_1217&DEV_8621&SUBSYS_a1911071 ;idx 153 for Getac V110G6
%bhtsddr.DeviceDesc% = DriverInstallx86_96001558, PCI\VEN_1217&DEV_8621&SUBSYS_96001558 ;idx 154 for Clevo N960KR_KP
%bhtsddr.DeviceDesc% = DriverInstallx86_86861558, PCI\VEN_1217&DEV_8621&SUBSYS_86861558 ;idx 155 for Clevo NJ50/70CU
%bhtsddr.DeviceDesc% = DriverInstallx86_385417aa, PCI\VEN_1217&DEV_8621&SUBSYS_385417aa ;idx 156 for Lenovo GLS1A/GLS1B
%bhtsddr.DeviceDesc% = DriverInstallx86_385317aa, PCI\VEN_1217&DEV_8621&SUBSYS_385317aa ;idx 157 for Lenovo S760-16
%bhtsddr.DeviceDesc% = DriverInstallx86_385517aa, PCI\VEN_1217&DEV_8621&SUBSYS_385517aa ;idx 158 for Lenovo S170IJL
%bhtsddr.DeviceDesc% = DriverInstallx86_40501558, PCI\VEN_1217&DEV_8621&SUBSYS_40501558 ;idx 159 for Clevo NL40MU
%bhtsddr.DeviceDesc% = DriverInstallx86_86821558, PCI\VEN_1217&DEV_8621&SUBSYS_86821558 ;idx 160 for Clevo NJ50MU
%bhtsddr.DeviceDesc% = DriverInstallx86_86831558, PCI\VEN_1217&DEV_8621&SUBSYS_86831558 ;idx 161 for Clevo NJ70MU
%bhtsddr.DeviceDesc% = DriverInstallx86_40181558, PCI\VEN_1217&DEV_8621&SUBSYS_40181558 ;idx 162 for Clevo NV40ME/MB/MZ
%bhtsddr.DeviceDesc% = DriverInstallx86_31141DC2, PCI\VEN_1217&DEV_8520&SUBSYS_31141DC2 ;idx 163 for IP3 TN3  update
%bhtsddr.DeviceDesc% = DriverInstallx86_C195144D, PCI\VEN_1217&DEV_8621&SUBSYS_C195144D ;idx 164 for Samsung NB2772
%bhtsddr.DeviceDesc% = DriverInstallx86_001C1E26, PCI\VEN_1217&DEV_8520&SUBSYS_001C1E26 ;idx 165 for Fujitsu/Quanta FB7C update
%bhtsddr.DeviceDesc% = DriverInstallx86_202F1043, PCI\VEN_1217&DEV_8520&SUBSYS_202F1043 ;idx 166 for Asus GA503
%bhtsddr.DeviceDesc% = DriverInstallx86_50ac17aa, PCI\VEN_1217&DEV_8621&SUBSYS_50ac17aa ;idx 167 for Lenovo GLS1A
%bhtsddr.DeviceDesc% = DriverInstallx86_50ad17aa, PCI\VEN_1217&DEV_8621&SUBSYS_50ad17aa ;idx 168 for Lenovo L1415
%bhtsddr.DeviceDesc% = DriverInstallx86_30051a58, PCI\VEN_1217&DEV_8520&SUBSYS_30051a58 ;idx 169 for Leishe Charlotte8
%bhtsddr.DeviceDesc% = DriverInstallx86_201b1a58, PCI\VEN_1217&DEV_8520&SUBSYS_201b1a58 ;idx 170 for Leishe Diane8
%bhtsddr.DeviceDesc% = DriverInstallx86_100b1a58, PCI\VEN_1217&DEV_8520&SUBSYS_100b1a58 ;idx 171 for Leishe M2
%bhtsddr.DeviceDesc% = DriverInstallx86_c1a7144d, PCI\VEN_1217&DEV_8621&SUBSYS_c1a7144d ;idx 172 for Samsung NB3586
%bhtsddr.DeviceDesc% = DriverInstallx86_386117aa, PCI\VEN_1217&DEV_8621&SUBSYS_386117aa ;idx 173 for Lenovo S570Pro-14 IAP(HLI42)
%bhtsddr.DeviceDesc% = DriverInstallx86_387017aa, PCI\VEN_1217&DEV_8621&SUBSYS_387017aa ;idx 174 for Lenovo ThinkBook 14/15 G4
%bhtsddr.DeviceDesc% = DriverInstallx86_386F17aa, PCI\VEN_1217&DEV_8621&SUBSYS_386F17aa ;idx 175 for Lenovo ThinkBook 14/15 G4
%bhtsddr.DeviceDesc% = DriverInstallx86_386617aa, PCI\VEN_1217&DEV_8621&SUBSYS_386617aa ;idx 176 for Lenovo C570
%bhtsddr.DeviceDesc% = DriverInstallx86_387217aa, PCI\VEN_1217&DEV_8621&SUBSYS_387217aa ;idx 177 for Lenovo S570-14 IAP(GLS4I)
%bhtsddr.DeviceDesc% = DriverInstallx86_386217aa, PCI\VEN_1217&DEV_8621&SUBSYS_386217aa ;idx 178 for Lenovo Yoga C770
%bhtsddr.DeviceDesc% = DriverInstallx86_386b17aa, PCI\VEN_1217&DEV_8621&SUBSYS_386b17aa ;idx 179 for Lenovo TB14-14/16
%bhtsddr.DeviceDesc% = DriverInstallx86_866d1558, PCI\VEN_1217&DEV_8621&SUBSYS_866d1558 ;idx 180 for Clevo NP50PNK_PNJ_PNH
%bhtsddr.DeviceDesc% = DriverInstallx86_51631558, PCI\VEN_1217&DEV_8621&SUBSYS_51631558 ;idx 181 for Clevo NH50JNP
%bhtsddr.DeviceDesc% = DriverInstallx86_386417aa, PCI\VEN_1217&DEV_8621&SUBSYS_386417aa ;idx 182 for Lenovo S570-16/intel
%bhtsddr.DeviceDesc% = DriverInstallx86_387117aa, PCI\VEN_1217&DEV_8621&SUBSYS_387117aa ;idx 183 for Lenovo ThinkBook 14/15 G4
%bhtsddr.DeviceDesc% = DriverInstallx86_389b17aa, PCI\VEN_1217&DEV_8621&SUBSYS_389b17aa ;idx 184 for Lenovo Y770S/Draco16
%bhtsddr.DeviceDesc% = DriverInstallx86_866c1558, PCI\VEN_1217&DEV_8621&SUBSYS_866c1558 ;idx 185 for Clevo NP50/60/70PNP
%bhtsddr.DeviceDesc% = DriverInstallx86_50a31558, PCI\VEN_1217&DEV_8621&SUBSYS_50a31558 ;idx 186 for Clevo NJ50GU
%bhtsddr.DeviceDesc% = DriverInstallx86_77161558, PCI\VEN_1217&DEV_8621&SUBSYS_77161558 ;idx 187 for Clevo NS50PU
%bhtsddr.DeviceDesc% = DriverInstallx86_77171558, PCI\VEN_1217&DEV_8621&SUBSYS_77171558 ;idx 188 for Clevo NS70PU
%bhtsddr.DeviceDesc% = DriverInstallx86_65f51558, PCI\VEN_1217&DEV_8621&SUBSYS_65f51558 ;idx 189 for Clevo PDxxPNT
%bhtsddr.DeviceDesc% = DriverInstallx86_387417aa, PCI\VEN_1217&DEV_8621&SUBSYS_387417aa ;idx 190 for Lenovo S370IAP/V17IAP/S1415IAP
%bhtsddr.DeviceDesc% = DriverInstallx86_387517aa, PCI\VEN_1217&DEV_8621&SUBSYS_387517aa ;idx 191 for Lenovo S170IAP
%bhtsddr.DeviceDesc% = DriverInstallx86_387717aa, PCI\VEN_1217&DEV_8621&SUBSYS_387717aa ;idx 192 for Lenovo S170S370ALC/S1415ABA
%bhtsddr.DeviceDesc% = DriverInstallx86_202F1043_8621, PCI\VEN_1217&DEV_8621&SUBSYS_202F1043 ;idx 193 for Asus NB5936
%bhtsddr.DeviceDesc% = DriverInstallx86_77181558, PCI\VEN_1217&DEV_8621&SUBSYS_77181558 ;idx 194 for Clevo L140PU
%bhtsddr.DeviceDesc% = DriverInstallx86_c1ad144d, PCI\VEN_1217&DEV_8621&SUBSYS_c1ad144d ;idx 195 for Samsung NB6033
%bhtsddr.DeviceDesc% = DriverInstallx86_40b11558, PCI\VEN_1217&DEV_8621&SUBSYS_40b11558 ;idx 196 for Clevo NL40GU1
%bhtsddr.DeviceDesc% = DriverInstallx86_40401558, PCI\VEN_1217&DEV_8621&SUBSYS_40401558 ;idx 197 for Clevo NV4xPNx
%bhtsddr.DeviceDesc% = DriverInstallx86_387d17aa, PCI\VEN_1217&DEV_8621&SUBSYS_387d17aa ;idx 198 for Lenovo NB6167A
%bhtsddr.DeviceDesc% = DriverInstallx86_00013100, PCI\VEN_1217&DEV_8621&SUBSYS_00013100 ;idx 199 for Toshiba Dynabook/Compal
%bhtsddr.DeviceDesc% = DriverInstallx86_388317aa, PCI\VEN_1217&DEV_8621&SUBSYS_388317aa ;idx 200 for Lenovo S770


[bhtsddr.NTamd64.10.0...19042]
%bhtsddr.Generic_DeviceDesc% = DriverInstallx64, PCI\VEN_1217&DEV_8520		;Default for Fujin2
%bhtsddr.Generic_DeviceDesc% = DriverInstallx64, PCI\VEN_1217&DEV_8420		;Default for SDS0
%bhtsddr.Generic_DeviceDesc% = DriverInstallx64, PCI\VEN_1217&DEV_8421		;Default for SDS1
%bhtsddr.Generic_DeviceDesc% = DriverInstallx64, PCI\VEN_1217&DEV_8620		;Default for Seabird
%bhtsddr.Generic_DeviceDesc% = DriverInstallx64, PCI\VEN_1217&DEV_8621		;Default for Seabird
%bhtsddr.Generic_DeviceDesc% = DriverInstallx64, PCI\VEN_1217&DEV_8720		;Default for SeaEagle2
%bhtsddr.Generic_DeviceDesc% = DriverInstallx64, PCI\VEN_1217&DEV_8721		;Default for SeaEagle2
%bhtsddr.Generic_DeviceDesc% = DriverInstallx64, PCI\VEN_1217&DEV_8722		;Default for SeaEagle2
%bhtsddr.Generic_DeviceDesc% = DriverInstallx64, PCI\VEN_1217&DEV_8723		;Default for SeaEagle2

%bhtsddr.DeviceDesc% = DriverInstallx64_221117aa, PCI\VEN_1217&DEV_8520&SUBSYS_221117aa ;idx 1
%bhtsddr.DeviceDesc% = DriverInstallx64_504117aa, PCI\VEN_1217&DEV_8620&SUBSYS_504117aa ;idx 2,3
%bhtsddr.DeviceDesc% = DriverInstallx64_504c17aa, PCI\VEN_1217&DEV_8520&SUBSYS_504c17aa ;idx 4
%bhtsddr.DeviceDesc% = DriverInstallx64_222c17aa, PCI\VEN_1217&DEV_8621&SUBSYS_222c17aa ;idx 5
%bhtsddr.DeviceDesc% = DriverInstallx64_380017aa, PCI\VEN_1217&DEV_8620&SUBSYS_380017aa ;idx 6
%bhtsddr.DeviceDesc% = DriverInstallx64_380117aa, PCI\VEN_1217&DEV_8620&SUBSYS_380117aa ;idx 7
%bhtsddr.DeviceDesc% = DriverInstallx64_380017aa_8621, PCI\VEN_1217&DEV_8621&SUBSYS_380017aa ;idx 8
%bhtsddr.DeviceDesc% = DriverInstallx64_390317aa, PCI\VEN_1217&DEV_8621&SUBSYS_390317aa ;idx 9
%bhtsddr.DeviceDesc% = DriverInstallx64_390217aa, PCI\VEN_1217&DEV_8621&SUBSYS_390217aa   ;idx 10
%bhtsddr.DeviceDesc% = DriverInstallx64_06EF1028, PCI\VEN_1217&DEV_8520&SUBSYS_06EF1028 ;idx 13
%bhtsddr.DeviceDesc% = DriverInstallx64_380017aa_8520, PCI\VEN_1217&DEV_8520&SUBSYS_380017aa ;idx 14
%bhtsddr.DeviceDesc% = DriverInstallx64_b28219da, PCI\VEN_1217&DEV_8520&SUBSYS_b28219da ;idx 15
%bhtsddr.DeviceDesc% = DriverInstallx64_10521025, PCI\VEN_1217&DEV_8621&SUBSYS_10521025 ;idx 16
%bhtsddr.DeviceDesc% = DriverInstallx64_10631025, PCI\VEN_1217&DEV_8621&SUBSYS_10631025 ;idx 17
%bhtsddr.DeviceDesc% = DriverInstallx64_000417aa, PCI\VEN_1217&DEV_8620&SUBSYS_000417aa ;idx 18
%bhtsddr.DeviceDesc% = DriverInstallx64_505b17aa, PCI\VEN_1217&DEV_8621&SUBSYS_505b17aa ;idx 19
%bhtsddr.DeviceDesc% = DriverInstallx64_511817aa, PCI\VEN_1217&DEV_8621&SUBSYS_511817aa ;idx 20
%bhtsddr.DeviceDesc% = DriverInstallx64_505c17aa, PCI\VEN_1217&DEV_8621&SUBSYS_505c17aa ;idx 21
%bhtsddr.DeviceDesc% = DriverInstallx64_609517aa, PCI\VEN_1217&DEV_8520&SUBSYS_609517aa ;idx 22
%bhtsddr.DeviceDesc% = DriverInstallx64_607E17aa, PCI\VEN_1217&DEV_8520&SUBSYS_607E17aa ;idx 23
%bhtsddr.DeviceDesc% = DriverInstallx64_369417aa, PCI\VEN_1217&DEV_8520&SUBSYS_369417aa ;idx 24
%bhtsddr.DeviceDesc% = DriverInstallx64_505417aa, PCI\VEN_1217&DEV_8520&SUBSYS_505417aa ;idx 25
%bhtsddr.DeviceDesc% = DriverInstallx64_380317aa, PCI\VEN_1217&DEV_8620&SUBSYS_380317aa ;idx 26
%bhtsddr.DeviceDesc% = DriverInstallx64_20648086, PCI\VEN_1217&DEV_8621&SUBSYS_20648086 ;idx 27
%bhtsddr.DeviceDesc% = DriverInstallx64_380117aa_8621, PCI\VEN_1217&DEV_8621&SUBSYS_380117aa ;idx 30
%bhtsddr.DeviceDesc% = DriverInstallx64_380217aa, PCI\VEN_1217&DEV_8621&SUBSYS_380217aa ;idx 31
%bhtsddr.DeviceDesc% = DriverInstallx64_380417aa, PCI\VEN_1217&DEV_8620&SUBSYS_380417aa ;idx 32
%bhtsddr.DeviceDesc% = DriverInstallx64_60ae17aa, PCI\VEN_1217&DEV_8520&SUBSYS_60ae17aa ;idx 33
%bhtsddr.DeviceDesc% = DriverInstallx64_06251028, PCI\VEN_1217&DEV_8520&SUBSYS_06251028 ;idx 34
%bhtsddr.DeviceDesc% = DriverInstallx64_06261028, PCI\VEN_1217&DEV_8520&SUBSYS_06261028 ;idx 35
%bhtsddr.DeviceDesc% = DriverInstallx64_060f1028, PCI\VEN_1217&DEV_8520&SUBSYS_060f1028 ;idx 36
%bhtsddr.DeviceDesc% = DriverInstallx64_062f1028, PCI\VEN_1217&DEV_8520&SUBSYS_062f1028 ;idx 37
%bhtsddr.DeviceDesc% = DriverInstallx64_06101028, PCI\VEN_1217&DEV_8520&SUBSYS_06101028 ;idx 38
%bhtsddr.DeviceDesc% = DriverInstallx64_224917aa, PCI\VEN_1217&DEV_8621&SUBSYS_224917aa ;idx 39
%bhtsddr.DeviceDesc% = DriverInstallx64_224a17aa, PCI\VEN_1217&DEV_8621&SUBSYS_224a17aa ;idx 40
%bhtsddr.DeviceDesc% = DriverInstallx64_506617aa, PCI\VEN_1217&DEV_8520&SUBSYS_506617aa ;idx 41
%bhtsddr.DeviceDesc% = DriverInstallx64_381f17aa, PCI\VEN_1217&DEV_8621&SUBSYS_381f17aa ;idx 47
%bhtsddr.DeviceDesc% = DriverInstallx64_382017aa, PCI\VEN_1217&DEV_8621&SUBSYS_382017aa ;idx 48
%bhtsddr.DeviceDesc% = DriverInstallx64_388117aa, PCI\VEN_1217&DEV_8520&SUBSYS_388117aa ;idx 49
%bhtsddr.DeviceDesc% = DriverInstallx64_380317aa_8621, PCI\VEN_1217&DEV_8621&SUBSYS_380317aa ;idx 50
%bhtsddr.DeviceDesc% = DriverInstallx64_381217aa, PCI\VEN_1217&DEV_8620&SUBSYS_381217aa ;idx 51
%bhtsddr.DeviceDesc% = DriverInstallx64_740017aa, PCI\VEN_1217&DEV_8621&SUBSYS_740017aa ;idx 52
%bhtsddr.DeviceDesc% = DriverInstallx64_381c17aa, PCI\VEN_1217&DEV_8621&SUBSYS_381c17aa ;idx 53
%bhtsddr.DeviceDesc% = DriverInstallx64_11881025, PCI\VEN_1217&DEV_8621&SUBSYS_11881025 ;idx 54
%bhtsddr.DeviceDesc% = DriverInstallx64_11891025, PCI\VEN_1217&DEV_8621&SUBSYS_11891025 ;idx 55
%bhtsddr.DeviceDesc% = DriverInstallx64_506817aa, PCI\VEN_1217&DEV_8621&SUBSYS_506817aa ;idx 56
%bhtsddr.DeviceDesc% = DriverInstallx64_380517aa, PCI\VEN_1217&DEV_8621&SUBSYS_380517aa ;idx 57
%bhtsddr.DeviceDesc% = DriverInstallx64_506a17aa, PCI\VEN_1217&DEV_8621&SUBSYS_506a17aa ;idx 58
%bhtsddr.DeviceDesc% = DriverInstallx64_506f17aa, PCI\VEN_1217&DEV_8621&SUBSYS_506f17aa ;idx 59
%bhtsddr.DeviceDesc% = DriverInstallx64_60cd17aa, PCI\VEN_1217&DEV_8621&SUBSYS_60cd17aa ;idx 60
%bhtsddr.DeviceDesc% = DriverInstallx64_380717aa, PCI\VEN_1217&DEV_8621&SUBSYS_380717aa ;idx 61
%bhtsddr.DeviceDesc% = DriverInstallx64_226117aa, PCI\VEN_1217&DEV_8621&SUBSYS_226117aa ;idx 62
%bhtsddr.DeviceDesc% = DriverInstallx64_20738086, PCI\VEN_1217&DEV_8621&SUBSYS_20738086 ;idx 63
%bhtsddr.DeviceDesc_SD% = DriverInstallx64_12301025, PCI\VEN_1217&DEV_8621&SUBSYS_12301025 ;idx 64
%bhtsddr.DeviceDesc% = DriverInstallx64_380617aa, PCI\VEN_1217&DEV_8621&SUBSYS_380617aa ;idx 65
%bhtsddr.DeviceDesc% = DriverInstallx64_380417aa_8621, PCI\VEN_1217&DEV_8621&SUBSYS_380417aa ;idx 66
%bhtsddr.DeviceDesc% = DriverInstallx64_380817aa, PCI\VEN_1217&DEV_8621&SUBSYS_380817aa ;idx 67
%bhtsddr.DeviceDesc% = DriverInstallx64_384617aa, PCI\VEN_1217&DEV_8621&SUBSYS_384617aa ;idx 68
%bhtsddr.DeviceDesc% = DriverInstallx64_227317aa, PCI\VEN_1217&DEV_8621&SUBSYS_227317aa ;idx 69
%bhtsddr.DeviceDesc% = DriverInstallx64_380917aa, PCI\VEN_1217&DEV_8621&SUBSYS_380917aa ;idx 70
%bhtsddr.DeviceDesc% = DriverInstallx64_39F617aa, PCI\VEN_1217&DEV_8621&SUBSYS_39F617aa ;idx 71 for Compal EL451 EL4C1
%bhtsddr.DeviceDesc% = DriverInstallx64_381317aa, PCI\VEN_1217&DEV_8621&SUBSYS_381317aa ;idx 72 for Compal EL431 EL531 EL5C3
%bhtsddr.DeviceDesc% = DriverInstallx64_382417aa, PCI\VEN_1217&DEV_8621&SUBSYS_382417aa ;idx 73 for Compal EL452 EL4C2
%bhtsddr.DeviceDesc% = DriverInstallx64_382117aa, PCI\VEN_1217&DEV_8621&SUBSYS_382117aa ;idx 74 for Compal EL432 EL532
%bhtsddr.DeviceDesc% = DriverInstallx64_507517aa, PCI\VEN_1217&DEV_8621&SUBSYS_507517aa ;idx 75
%bhtsddr.DeviceDesc% = DriverInstallx64_383e17aa, PCI\VEN_1217&DEV_8621&SUBSYS_383e17aa ;idx 76 for Compal S740    Support Modernstandby
%bhtsddr.DeviceDesc% = DriverInstallx64_381817aa, PCI\VEN_1217&DEV_8621&SUBSYS_381817aa ;idx 77 for Lenovo
%bhtsddr.DeviceDesc% = DriverInstallx64_381417aa, PCI\VEN_1217&DEV_8621&SUBSYS_381417aa ;idx 78 for Lenovo
%bhtsddr.DeviceDesc% = DriverInstallx64_380f17aa, PCI\VEN_1217&DEV_8621&SUBSYS_380f17aa ;idx 79 for Lenovo         Support Modernstandby
%bhtsddr.DeviceDesc% = DriverInstallx64_507217aa, PCI\VEN_1217&DEV_8621&SUBSYS_507217aa ;idx 80 for Lenovo WU issue
%bhtsddr.DeviceDesc% = DriverInstallx64_383717aa, PCI\VEN_1217&DEV_8621&SUBSYS_383717aa ;idx 81 for Lenovo C340
%bhtsddr.DeviceDesc% = DriverInstallx64_3a3b17aa, PCI\VEN_1217&DEV_8621&SUBSYS_3a3b17aa ;idx 82 for Lenovo C340S340 for ICL
%bhtsddr.DeviceDesc% = DriverInstallx64_383517aa, PCI\VEN_1217&DEV_8621&SUBSYS_383517aa ;idx 83 for Lenovo FLMS0   Support Modernstandby
%bhtsddr.DeviceDesc% = DriverInstallx64_382F17aa, PCI\VEN_1217&DEV_8621&SUBSYS_382F17aa ;idx 84 for Lenovo V340 14
%bhtsddr.DeviceDesc% = DriverInstallx64_383217aa, PCI\VEN_1217&DEV_8621&SUBSYS_383217aa ;idx 85 for Lenovo V340 15
%bhtsddr.DeviceDesc% = DriverInstallx64_385217aa, PCI\VEN_1217&DEV_8621&SUBSYS_385217aa ;idx 86 for Lenovo V340 IIL 14
%bhtsddr.DeviceDesc% = DriverInstallx64_385117aa, PCI\VEN_1217&DEV_8621&SUBSYS_385117aa ;idx 87 for Lenovo V340 IIL 15
%bhtsddr.DeviceDesc% = DriverInstallx64_507c17aa, PCI\VEN_1217&DEV_8621&SUBSYS_507c17aa ;idx 88 for Lenovo L4A0L5A0
%bhtsddr.DeviceDesc% = DriverInstallx64_381617aa, PCI\VEN_1217&DEV_8621&SUBSYS_381617aa ;idx 89 for Lenovo C350-11
%bhtsddr.DeviceDesc% = DriverInstallx64_507e17aa, PCI\VEN_1217&DEV_8621&SUBSYS_507e17aa ;idx 90 for Lenovo Odin Thor
%bhtsddr.DeviceDesc% = DriverInstallx64_383117aa, PCI\VEN_1217&DEV_8621&SUBSYS_383117aa ;idx 91 for Lenovo FLMA0
%bhtsddr.DeviceDesc% = DriverInstallx64_381b17aa, PCI\VEN_1217&DEV_8621&SUBSYS_381b17aa ;idx 92 for Lenovo C550-14AMD
%bhtsddr.DeviceDesc% = DriverInstallx64_382517aa, PCI\VEN_1217&DEV_8621&SUBSYS_382517aa ;idx 93 for Lenovo Ideapad Duet3 D350
%bhtsddr.DeviceDesc% = DriverInstallx64_381717aa, PCI\VEN_1217&DEV_8621&SUBSYS_381717aa ;idx 94 for Lenovo C550-14Intel
%bhtsddr.DeviceDesc% = DriverInstallx64_382217aa, PCI\VEN_1217&DEV_8621&SUBSYS_382217aa ;idx 95 for Lenovo Yoga duet7 D550
%bhtsddr.DeviceDesc% = DriverInstallx64_383d17aa, PCI\VEN_1217&DEV_8621&SUBSYS_383d17aa ;idx 96 for Lenovo GLY5U
%bhtsddr.DeviceDesc% = DriverInstallx64_507b17aa, PCI\VEN_1217&DEV_8621&SUBSYS_507b17aa ;idx 97 for Lenovo LIA
%bhtsddr.DeviceDesc% = DriverInstallx64_381917aa, PCI\VEN_1217&DEV_8621&SUBSYS_381917aa ;idx 98 for Lenovo Y550
%bhtsddr.DeviceDesc% = DriverInstallx64_512417aa, PCI\VEN_1217&DEV_8621&SUBSYS_512417aa ;idx 99 for Lenovo EX95
%bhtsddr.DeviceDesc% = DriverInstallx64_383a17aa, PCI\VEN_1217&DEV_8621&SUBSYS_383a17aa ;idx 100 for Lenovo V350_Titan Intel platform
%bhtsddr.DeviceDesc% = DriverInstallx64_382717aa, PCI\VEN_1217&DEV_8621&SUBSYS_382717aa ;idx 101 for Lenovo V350_Titan AMD platform
%bhtsddr.DeviceDesc% = DriverInstallx64_380a17aa, PCI\VEN_1217&DEV_8621&SUBSYS_380a17aa ;idx 102 for Lenovo Y750S
%bhtsddr.DeviceDesc% = DriverInstallx64_383917aa, PCI\VEN_1217&DEV_8621&SUBSYS_383917aa ;idx 103 for Lenovo Compal GLMS1
%bhtsddr.DeviceDesc% = DriverInstallx64_382617aa, PCI\VEN_1217&DEV_8621&SUBSYS_382617aa ;idx 104 for Lenovo
%bhtsddr.DeviceDesc% = DriverInstallx64_382917aa, PCI\VEN_1217&DEV_8621&SUBSYS_382917aa ;idx 105 for Lenovo 100e 300e 2rd 
%bhtsddr.DeviceDesc% = DriverInstallx64_509317aa, PCI\VEN_1217&DEV_8621&SUBSYS_509317aa ;idx 106 for Lenovo Yoga Gen 6 
%bhtsddr.DeviceDesc% = DriverInstallx64_508f17aa, PCI\VEN_1217&DEV_8621&SUBSYS_508f17aa ;idx 107 for Lenovo Odin2.0 Thor2.0
%bhtsddr.DeviceDesc% = DriverInstallx64_382817aa, PCI\VEN_1217&DEV_8621&SUBSYS_382817aa ;idx 108 for Lenovo LC56-14TGL
%bhtsddr.DeviceDesc% = DriverInstallx64_382b17aa, PCI\VEN_1217&DEV_8621&SUBSYS_382b17aa ;idx 109 for Lenovo Y750A+N
%bhtsddr.DeviceDesc% = DriverInstallx64_382d17aa, PCI\VEN_1217&DEV_8621&SUBSYS_382d17aa ;idx 110 for Lenovo 300W Gen3 JPL
%bhtsddr.DeviceDesc% = DriverInstallx64_383c17aa, PCI\VEN_1217&DEV_8621&SUBSYS_383c17aa ;idx 111 for Lenovo GLI42
%bhtsddr.DeviceDesc% = DriverInstallx64_509117aa, PCI\VEN_1217&DEV_8621&SUBSYS_509117aa ;idx 112 for Lenovo Odin2.0 Thor2.0 AMD update
%bhtsddr.DeviceDesc% = DriverInstallx64_383317aa, PCI\VEN_1217&DEV_8621&SUBSYS_383317aa ;idx 113 for Lenovo D330-10IGL
%bhtsddr.DeviceDesc% = DriverInstallx64_383017aa, PCI\VEN_1217&DEV_8621&SUBSYS_383017aa ;idx 114 for Lenovo LC56 AMD
%bhtsddr.DeviceDesc% = DriverInstallx64_383b17aa, PCI\VEN_1217&DEV_8621&SUBSYS_383b17aa ;idx 115 for Lenovo V350_Titan
%bhtsddr.DeviceDesc% = DriverInstallx64_383417aa, PCI\VEN_1217&DEV_8621&SUBSYS_383417aa ;idx 116 for Lenovo S560-16 ITL 
%bhtsddr.DeviceDesc% = DriverInstallx64_383f17aa, PCI\VEN_1217&DEV_8621&SUBSYS_383f17aa ;idx 117 for Lenovo S560-16ACN
%bhtsddr.DeviceDesc% = DriverInstallx64_384017aa, PCI\VEN_1217&DEV_8621&SUBSYS_384017aa ;idx 118 for Lenovo V350_Titan 
%bhtsddr.DeviceDesc% = DriverInstallx64_384117aa, PCI\VEN_1217&DEV_8621&SUBSYS_384117aa ;idx 119 for Lenovo D760
%bhtsddr.DeviceDesc% = DriverInstallx64_384417aa, PCI\VEN_1217&DEV_8621&SUBSYS_384417aa ;idx 120 for Lenovo Thinkbook 14P
%bhtsddr.DeviceDesc% = DriverInstallx64_384517aa, PCI\VEN_1217&DEV_8621&SUBSYS_384517aa ;idx 121 for Lenovo Thinkbook 16P
%bhtsddr.DeviceDesc% = DriverInstallx64_384717aa, PCI\VEN_1217&DEV_8621&SUBSYS_384717aa ;idx 122 for Lenovo Y560ITH
%bhtsddr.DeviceDesc% = DriverInstallx64_384917aa, PCI\VEN_1217&DEV_8621&SUBSYS_384917aa ;idx 123 for Lenovo 100E/300E
%bhtsddr.DeviceDesc% = DriverInstallx64_384b17aa, PCI\VEN_1217&DEV_8621&SUBSYS_384b17aa ;idx 124 for Lenovo Y760S
%bhtsddr.DeviceDesc% = DriverInstallx64_384c17aa, PCI\VEN_1217&DEV_8621&SUBSYS_384c17aa ;idx 125 for Lenovo Y550IMH
%bhtsddr.DeviceDesc% = DriverInstallx64_50e11558, PCI\VEN_1217&DEV_8621&SUBSYS_50e11558 ;idx 126 for Clevo
%bhtsddr.DeviceDesc% = DriverInstallx64_50e21558, PCI\VEN_1217&DEV_8621&SUBSYS_50e21558 ;idx 127 for Clevo
%bhtsddr.DeviceDesc% = DriverInstallx64_50151558, PCI\VEN_1217&DEV_8621&SUBSYS_50151558 ;idx 128 for Clevo
%bhtsddr.DeviceDesc% = DriverInstallx64_50171558, PCI\VEN_1217&DEV_8621&SUBSYS_50171558 ;idx 129 for Clevo
%bhtsddr.DeviceDesc% = DriverInstallx64_866b1558, PCI\VEN_1217&DEV_8621&SUBSYS_866b1558 ;idx 130 for Clevo
%bhtsddr.DeviceDesc% = DriverInstallx64_867b1558, PCI\VEN_1217&DEV_8621&SUBSYS_867b1558 ;idx 131 for Clevo
%bhtsddr.DeviceDesc% = DriverInstallx64_00021217, PCI\VEN_1217&DEV_8621&SUBSYS_00021217 ;idx 132 for OZ711LV2 default ID update for Clevo AMD
%bhtsddr.DeviceDesc% = DriverInstallx64_85111558, PCI\VEN_1217&DEV_8621&SUBSYS_85111558 ;idx 133 for Clevo
%bhtsddr.DeviceDesc% = DriverInstallx64_87111558, PCI\VEN_1217&DEV_8621&SUBSYS_87111558 ;idx 134 for Clevo
%bhtsddr.DeviceDesc% = DriverInstallx64_50f41558, PCI\VEN_1217&DEV_8621&SUBSYS_50f41558 ;idx 135 for Clevo
%bhtsddr.DeviceDesc% = DriverInstallx64_50c51558, PCI\VEN_1217&DEV_8621&SUBSYS_50c51558 ;idx 136 for Clevo
%bhtsddr.DeviceDesc% = DriverInstallx64_51a11558, PCI\VEN_1217&DEV_8621&SUBSYS_51a11558 ;idx 137 for Clevo TGL-U
%bhtsddr.DeviceDesc% = DriverInstallx64_a5001558, PCI\VEN_1217&DEV_8621&SUBSYS_a5001558 ;idx 138 for Clevo Renoir
%bhtsddr.DeviceDesc% = DriverInstallx64_a6001558, PCI\VEN_1217&DEV_8621&SUBSYS_a6001558 ;idx 139 for Clevo Ryzen
%bhtsddr.DeviceDesc% = DriverInstallx64_40301558, PCI\VEN_1217&DEV_8621&SUBSYS_40301558 ;idx 140 for Clevo NV40Mx
%bhtsddr.DeviceDesc% = DriverInstallx64_14A11558, PCI\VEN_1217&DEV_8621&SUBSYS_14A11558 ;idx 141 for Clevo L140MU
%bhtsddr.DeviceDesc% = DriverInstallx64_384f17aa, PCI\VEN_1217&DEV_8621&SUBSYS_384f17aa ;idx 142 for Lenovo S170-Dali
%bhtsddr.DeviceDesc% = DriverInstallx64_e2071071, PCI\VEN_1217&DEV_8621&SUBSYS_e2071071 ;idx 143 for Getac F110G6
%bhtsddr.DeviceDesc% = DriverInstallx64_a1211071, PCI\VEN_1217&DEV_8621&SUBSYS_a1211071 ;idx 144 for Getac K120G2
%bhtsddr.DeviceDesc% = DriverInstallx64_40151071, PCI\VEN_1217&DEV_8621&SUBSYS_40151071 ;idx 145 for Getac S410G4
%bhtsddr.DeviceDesc% = DriverInstallx64_a2521071, PCI\VEN_1217&DEV_8621&SUBSYS_a2521071 ;idx 146 for Getac Raptor
%bhtsddr.DeviceDesc% = DriverInstallx64_b3601071, PCI\VEN_1217&DEV_8621&SUBSYS_b3601071 ;idx 147 for Getac B360
%bhtsddr.DeviceDesc% = DriverInstallx64_e2051071, PCI\VEN_1217&DEV_8621&SUBSYS_e2051071 ;idx 148 for Getac F110G5
%bhtsddr.DeviceDesc% = DriverInstallx64_a1201071, PCI\VEN_1217&DEV_8621&SUBSYS_a1201071 ;idx 149 for Getac K120
%bhtsddr.DeviceDesc% = DriverInstallx64_d3001071, PCI\VEN_1217&DEV_8621&SUBSYS_d3001071 ;idx 150 for Getac UX10G1
%bhtsddr.DeviceDesc% = DriverInstallx64_d3011071, PCI\VEN_1217&DEV_8621&SUBSYS_d3011071 ;idx 151 for Getac UX10G2
%bhtsddr.DeviceDesc% = DriverInstallx64_a1901071, PCI\VEN_1217&DEV_8621&SUBSYS_a1901071 ;idx 152 for Getac V110G5
%bhtsddr.DeviceDesc% = DriverInstallx64_a1911071, PCI\VEN_1217&DEV_8621&SUBSYS_a1911071 ;idx 153 for Getac V110G6
%bhtsddr.DeviceDesc% = DriverInstallx64_96001558, PCI\VEN_1217&DEV_8621&SUBSYS_96001558 ;idx 154 for Clevo N960KR_KP
%bhtsddr.DeviceDesc% = DriverInstallx64_86861558, PCI\VEN_1217&DEV_8621&SUBSYS_86861558 ;idx 155 for Clevo NJ50/70CU
%bhtsddr.DeviceDesc% = DriverInstallx64_385417aa, PCI\VEN_1217&DEV_8621&SUBSYS_385417aa ;idx 156 for Lenovo GLS1A/GLS1B
%bhtsddr.DeviceDesc% = DriverInstallx64_385317aa, PCI\VEN_1217&DEV_8621&SUBSYS_385317aa ;idx 157 for Lenovo S760-16
%bhtsddr.DeviceDesc% = DriverInstallx64_385517aa, PCI\VEN_1217&DEV_8621&SUBSYS_385517aa ;idx 158 for Lenovo S170IJL
%bhtsddr.DeviceDesc% = DriverInstallx64_40501558, PCI\VEN_1217&DEV_8621&SUBSYS_40501558 ;idx 159 for Clevo NL40MU
%bhtsddr.DeviceDesc% = DriverInstallx64_86821558, PCI\VEN_1217&DEV_8621&SUBSYS_86821558 ;idx 160 for Clevo NJ50MU
%bhtsddr.DeviceDesc% = DriverInstallx64_86831558, PCI\VEN_1217&DEV_8621&SUBSYS_86831558 ;idx 161 for Clevo NJ70MU
%bhtsddr.DeviceDesc% = DriverInstallx64_40181558, PCI\VEN_1217&DEV_8621&SUBSYS_40181558 ;idx 162 for Clevo NV40ME/MB/MZ
%bhtsddr.DeviceDesc% = DriverInstallx64_31141DC2, PCI\VEN_1217&DEV_8520&SUBSYS_31141DC2 ;idx 163 for IP3 TN3  update
%bhtsddr.DeviceDesc% = DriverInstallx64_C195144D, PCI\VEN_1217&DEV_8621&SUBSYS_C195144D ;idx 164 for Samsung NB2772
%bhtsddr.DeviceDesc% = DriverInstallx64_001C1E26, PCI\VEN_1217&DEV_8520&SUBSYS_001C1E26 ;idx 165 for Fujitsu/Quanta FB7C update
%bhtsddr.DeviceDesc% = DriverInstallx64_202F1043, PCI\VEN_1217&DEV_8520&SUBSYS_202F1043 ;idx 166 for Asus GA503
%bhtsddr.DeviceDesc% = DriverInstallx64_50ac17aa, PCI\VEN_1217&DEV_8621&SUBSYS_50ac17aa ;idx 167 for Lenovo GLS1A
%bhtsddr.DeviceDesc% = DriverInstallx64_50ad17aa, PCI\VEN_1217&DEV_8621&SUBSYS_50ad17aa ;idx 168 for Lenovo L1415
%bhtsddr.DeviceDesc% = DriverInstallx64_30051a58, PCI\VEN_1217&DEV_8520&SUBSYS_30051a58 ;idx 169 for Leishe Charlotte8
%bhtsddr.DeviceDesc% = DriverInstallx64_201b1a58, PCI\VEN_1217&DEV_8520&SUBSYS_201b1a58 ;idx 170 for Leishe Diane8
%bhtsddr.DeviceDesc% = DriverInstallx64_100b1a58, PCI\VEN_1217&DEV_8520&SUBSYS_100b1a58 ;idx 171 for Leishe M2
%bhtsddr.DeviceDesc% = DriverInstallx64_c1a7144d, PCI\VEN_1217&DEV_8621&SUBSYS_c1a7144d ;idx 172 for Samsung NB3586
%bhtsddr.DeviceDesc% = DriverInstallx64_386117aa, PCI\VEN_1217&DEV_8621&SUBSYS_386117aa ;idx 173 for Lenovo S570Pro-14 IAP(HLI42)
%bhtsddr.DeviceDesc% = DriverInstallx64_387017aa, PCI\VEN_1217&DEV_8621&SUBSYS_387017aa ;idx 174 for Lenovo ThinkBook 14/15 G4
%bhtsddr.DeviceDesc% = DriverInstallx64_386F17aa, PCI\VEN_1217&DEV_8621&SUBSYS_386F17aa ;idx 175 for Lenovo ThinkBook 14/15 G4
%bhtsddr.DeviceDesc% = DriverInstallx64_386617aa, PCI\VEN_1217&DEV_8621&SUBSYS_386617aa ;idx 176 for Lenovo C570
%bhtsddr.DeviceDesc% = DriverInstallx64_387217aa, PCI\VEN_1217&DEV_8621&SUBSYS_387217aa ;idx 177 for Lenovo S570-14 IAP(GLS4I)
%bhtsddr.DeviceDesc% = DriverInstallx64_386217aa, PCI\VEN_1217&DEV_8621&SUBSYS_386217aa ;idx 178 for Lenovo Yoga C770
%bhtsddr.DeviceDesc% = DriverInstallx64_386b17aa, PCI\VEN_1217&DEV_8621&SUBSYS_386b17aa ;idx 179 for Lenovo TB14-14/16
%bhtsddr.DeviceDesc% = DriverInstallx64_866d1558, PCI\VEN_1217&DEV_8621&SUBSYS_866d1558 ;idx 180 for Clevo NP50PNK_PNJ_PNH
%bhtsddr.DeviceDesc% = DriverInstallx64_51631558, PCI\VEN_1217&DEV_8621&SUBSYS_51631558 ;idx 181 for Clevo NH50JNP
%bhtsddr.DeviceDesc% = DriverInstallx64_386417aa, PCI\VEN_1217&DEV_8621&SUBSYS_386417aa ;idx 182 for Lenovo S570-16/intel
%bhtsddr.DeviceDesc% = DriverInstallx64_387117aa, PCI\VEN_1217&DEV_8621&SUBSYS_387117aa ;idx 183 for Lenovo ThinkBook 14/15 G4
%bhtsddr.DeviceDesc% = DriverInstallx64_389b17aa, PCI\VEN_1217&DEV_8621&SUBSYS_389b17aa ;idx 184 for Lenovo Y770S/Draco16
%bhtsddr.DeviceDesc% = DriverInstallx64_866c1558, PCI\VEN_1217&DEV_8621&SUBSYS_866c1558 ;idx 185 for Clevo NP50/60/70PNP
%bhtsddr.DeviceDesc% = DriverInstallx64_50a31558, PCI\VEN_1217&DEV_8621&SUBSYS_50a31558 ;idx 186 for Clevo NJ50GU
%bhtsddr.DeviceDesc% = DriverInstallx64_77161558, PCI\VEN_1217&DEV_8621&SUBSYS_77161558 ;idx 187 for Clevo NS50PU
%bhtsddr.DeviceDesc% = DriverInstallx64_77171558, PCI\VEN_1217&DEV_8621&SUBSYS_77171558 ;idx 188 for Clevo NS70PU
%bhtsddr.DeviceDesc% = DriverInstallx64_65f51558, PCI\VEN_1217&DEV_8621&SUBSYS_65f51558 ;idx 189 for Clevo PDxxPNT
%bhtsddr.DeviceDesc% = DriverInstallx64_387417aa, PCI\VEN_1217&DEV_8621&SUBSYS_387417aa ;idx 190 for Lenovo S370IAP/V17IAP/S1415IAP
%bhtsddr.DeviceDesc% = DriverInstallx64_387517aa, PCI\VEN_1217&DEV_8621&SUBSYS_387517aa ;idx 191 for Lenovo S170IAP
%bhtsddr.DeviceDesc% = DriverInstallx64_387717aa, PCI\VEN_1217&DEV_8621&SUBSYS_387717aa ;idx 192 for Lenovo S170S370ALC/S1415ABA
%bhtsddr.DeviceDesc% = DriverInstallx64_202F1043_8621, PCI\VEN_1217&DEV_8621&SUBSYS_202F1043 ;idx 193 for Asus NB5936
%bhtsddr.DeviceDesc% = DriverInstallx64_77181558, PCI\VEN_1217&DEV_8621&SUBSYS_77181558 ;idx 194 for Clevo L140PU
%bhtsddr.DeviceDesc% = DriverInstallx64_c1ad144d, PCI\VEN_1217&DEV_8621&SUBSYS_c1ad144d ;idx 195 for Samsung NB6033
%bhtsddr.DeviceDesc% = DriverInstallx64_40b11558, PCI\VEN_1217&DEV_8621&SUBSYS_40b11558 ;idx 196 for Clevo NL40GU1
%bhtsddr.DeviceDesc% = DriverInstallx64_40401558, PCI\VEN_1217&DEV_8621&SUBSYS_40401558 ;idx 197 for Clevo NV4xPNx
%bhtsddr.DeviceDesc% = DriverInstallx64_387d17aa, PCI\VEN_1217&DEV_8621&SUBSYS_387d17aa ;idx 198 for Lenovo NB6167A
%bhtsddr.DeviceDesc% = DriverInstallx64_00013100, PCI\VEN_1217&DEV_8621&SUBSYS_00013100 ;idx 199 for Toshiba Dynabook/Compal
%bhtsddr.DeviceDesc% = DriverInstallx64_388317aa, PCI\VEN_1217&DEV_8621&SUBSYS_388317aa ;idx 200 for Lenovo S770


[DriverInstallx86.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg 
;AddReg         = default_cfg_se_pcr
;AddReg         = default_cfg_sb_pcr

[DriverInstallx86.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86;, EventLogService

[DriverInstallx64.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg 
;AddReg         = default_cfg_se_pcr
;AddReg         = default_cfg_sb_pcr

[DriverInstallx64.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64;, EventLogService

[DriverServicex64]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg 
AddReg         = default_cfg_se
AddReg         = default_cfg_sb
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverServicex86]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg 
AddReg         = default_cfg_se
AddReg         = default_cfg_sb
AddReg         = bus_type
AddReg         = autorun_addreg

;cfg idx 1 
[DriverInstallx86_221117aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_221117aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 221117aa_cfg_pcr

[DriverInstallx86_221117aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_221117aa;, EventLogService

[DriverServicex86_221117aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = autorun_addreg
AddReg         = 221117aa_cfg

[DriverInstallx64_221117aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_221117aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg 
AddReg         = 221117aa_cfg_pcr

[DriverInstallx64_221117aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_221117aa;, EventLogService

[DriverServicex64_221117aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg 
AddReg         = 221117aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[221117aa_cfg]
HKR,"seaeagle", "driver_item", 0x00010001, 0x8000001a
HKR,"seaeagle", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seaeagle", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seaeagle", "output_tuning", 0x00010001, 0x8001000a

[221117aa_cfg_pcr]
HKR,"seaeagle\pcr", "pcr_value", 1, 00,00,03,00,00,ff,00,44,00,00,03,e0,00,40,00,00


;cfg idx 2,3
[DriverInstallx86_504117aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_504117aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 504117aa_cfg_pcr

[DriverInstallx86_504117aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_504117aa;, EventLogService

[DriverServicex86_504117aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg 
AddReg         = 504117aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_504117aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_504117aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg 
AddReg         = 504117aa_cfg_pcr

[DriverInstallx64_504117aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_504117aa;, EventLogService

[DriverServicex64_504117aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg 
AddReg         = 504117aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[504117aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[504117aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,00,55,00,00,00,e2,f0,00,10,00,00,00,00,fe,00,0f,00,0c,00,00,03,e6,00,08,00,08


;cfg idx 4 
[DriverInstallx86_504c17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_504c17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 504c17aa_cfg_pcr

[DriverInstallx86_504c17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_504c17aa;, EventLogService

[DriverServicex86_504c17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg 
AddReg         = 504c17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_504c17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_504c17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg 
AddReg         = 504c17aa_cfg_pcr

[DriverInstallx64_504c17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_504c17aa;, EventLogService

[DriverServicex64_504c17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg 
AddReg         = 504c17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[504c17aa_cfg]
HKR,"seaeagle", "driver_item", 0x00010001, 0x8000001a
HKR,"seaeagle", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seaeagle", "MS_SDIO_CTRL", 0x00010001, 0x0

[504c17aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,00,55,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e4,00,7e,00,48


;cfg idx 5 
[DriverInstallx86_222c17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_222c17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 222c17aa_cfg_pcr

[DriverInstallx86_222c17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_222c17aa;, EventLogService

[DriverServicex86_222c17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg 
AddReg         = 222c17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_222c17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_222c17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg 
AddReg         = 222c17aa_cfg_pcr

[DriverInstallx64_222c17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_222c17aa;, EventLogService

[DriverServicex64_222c17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg 
AddReg         = 222c17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[222c17aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird", "output_tuning", 0x00010001, 0x8001000a

[222c17aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,00,55,00,00,00,e2,f0,00,10,00,00,00,00,fe,00,0f,00,0c,00,00,03,e6,00,08,00,08


;cfg idx 6 
[DriverInstallx86_380017aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_380017aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 380017aa_cfg_pcr

[DriverInstallx86_380017aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_380017aa;, EventLogService

[DriverServicex86_380017aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 380017aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_380017aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_380017aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 380017aa_cfg_pcr

[DriverInstallx64_380017aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_380017aa;, EventLogService

[DriverServicex64_380017aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 380017aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[380017aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[380017aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,00,55,00,00,00,e2,f0,00,10,00,00,00,00,fe,00,0f,00,0c,00,00,03,e6,00,08,00,08


;cfg idx 7 
[DriverInstallx86_380117aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_380117aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 380117aa_cfg_pcr

[DriverInstallx86_380117aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_380117aa;, EventLogService

[DriverServicex86_380117aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 380117aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_380117aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_380117aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 380117aa_cfg_pcr

[DriverInstallx64_380117aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_380117aa;, EventLogService

[DriverServicex64_380117aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 380117aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[380117aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[380117aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,00,55,00,00,00,e2,f0,00,10,00,00,00,00,fe,00,0f,00,0c,00,00,03,e6,00,08,00,08


;cfg idx 8
[DriverInstallx86_380017aa_8621.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_380017aa_8621.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 380017aa_8621_cfg_pcr

[DriverInstallx86_380017aa_8621.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_380017aa_8621;, EventLogService

[DriverServicex86_380017aa_8621]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 380017aa_8621_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_380017aa_8621.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_380017aa_8621.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 380017aa_8621_cfg_pcr

[DriverInstallx64_380017aa_8621.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_380017aa_8621;, EventLogService

[DriverServicex64_380017aa_8621]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 380017aa_8621_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[380017aa_8621_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird", "output_tuning", 0x00010001, 0x8001000a

[380017aa_8621_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,00,55,00,00,00,e2,f0,00,10,00,00,00,00,fe,00,0f,00,0c,00,00,03,e6,00,08,00,08


;cfg idx 9
[DriverInstallx86_390317aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_390317aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 390317aa_cfg_pcr

[DriverInstallx86_390317aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_390317aa;, EventLogService

[DriverServicex86_390317aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 390317aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_390317aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_390317aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 390317aa_cfg_pcr

[DriverInstallx64_390317aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_390317aa;, EventLogService

[DriverServicex64_390317aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 390317aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[390317aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird", "output_tuning", 0x00010001, 0x8001000a

[390317aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,00,55,00,00,00,e2,f0,00,10,00,00,00,00,fe,00,0f,00,0c,00,00,03,e6,00,08,00,08


;cfg idx 10
[DriverInstallx86_390217aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_390217aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 390217aa_cfg_pcr

[DriverInstallx86_390217aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_390217aa;, EventLogService

[DriverServicex86_390217aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 390217aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_390217aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_390217aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 390217aa_cfg_pcr

[DriverInstallx64_390217aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_390217aa;, EventLogService

[DriverServicex64_390217aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 390217aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[390217aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[390217aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,00,55,00,00,00,e2,f0,00,10,00,00,00,00,fe,00,0f,00,0c,00,00,03,e6,00,08,00,08


;cfg idx 13
[DriverInstallx86_06EF1028.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_06EF1028.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_06EF1028.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_06EF1028;, EventLogService

[DriverServicex86_06EF1028]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 06EF1028_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_06EF1028.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_06EF1028.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_06EF1028.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_06EF1028;, EventLogService

[DriverServicex64_06EF1028]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 06EF1028_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[06EF1028_cfg]
HKR,"seaeagle", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seaeagle", "output_tuning", 0x00010001, 0x80010000


;cfg idx 14
[DriverInstallx86_380017aa_8520.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_380017aa_8520.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_380017aa_8520.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_380017aa_8520;, EventLogService

[DriverServicex86_380017aa_8520]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 380017aa_8520_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_380017aa_8520.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_380017aa_8520.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_380017aa_8520.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_380017aa_8520;, EventLogService

[DriverServicex64_380017aa_8520]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 380017aa_8520_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[380017aa_8520_cfg]
HKR,"seaeagle", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seaeagle", "MS_SDIO_CTRL", 0x00010001, 0x0

;cfg idx 15
[DriverInstallx86_b28219da.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_b28219da.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = b28219da_cfg_pcr

[DriverInstallx86_b28219da.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_b28219da;, EventLogService

[DriverServicex86_b28219da]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = b28219da_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_b28219da.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_b28219da.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = b28219da_cfg_pcr

[DriverInstallx64_b28219da.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_b28219da;, EventLogService

[DriverServicex64_b28219da]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = b28219da_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[b28219da_cfg]
HKR,"seaeagle", "driver_item", 0x00010001, 0x8000001a
HKR,"seaeagle", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seaeagle", "MS_SDIO_CTRL", 0x00010001, 0x0

[b28219da_cfg_pcr]
HKR,"seaeagle\pcr", "pcr_value", 1, 00,00,03,00,00,ff,00,44,00,00,03,e0,00,40,00,00


;cfg idx 16
[DriverInstallx86_10521025.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_10521025.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_10521025.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_10521025;, EventLogService

[DriverServicex86_10521025]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 10521025_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_10521025.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_10521025.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues


[DriverInstallx64_10521025.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_10521025;, EventLogService

[DriverServicex64_10521025]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 10521025_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[10521025_cfg]
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0


;cfg idx 17
[DriverInstallx86_10631025.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_10631025.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_10631025.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_10631025;, EventLogService

[DriverServicex86_10631025]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 10631025_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_10631025.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_10631025.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues


[DriverInstallx64_10631025.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_10631025;, EventLogService

[DriverServicex64_10631025]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 10631025_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[10631025_cfg]
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0


;cfg idx 18
[DriverInstallx86_000417aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_000417aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_000417aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_000417aa;, EventLogService

[DriverServicex86_000417aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 000417aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_000417aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_000417aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_000417aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_000417aa;, EventLogService

[DriverServicex64_000417aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 000417aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[000417aa_cfg]
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0


;cfg idx 19
[DriverInstallx86_505b17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_505b17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_505b17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_505b17aa;, EventLogService

[DriverServicex86_505b17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 505b17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_505b17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_505b17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_505b17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_505b17aa;, EventLogService

[DriverServicex64_505b17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 505b17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[505b17aa_cfg]
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

;cfg idx 20
[DriverInstallx86_511817aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_511817aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_511817aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_511817aa;, EventLogService

[DriverServicex86_511817aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 511817aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_511817aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_511817aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_511817aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_511817aa;, EventLogService

[DriverServicex64_511817aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 511817aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[511817aa_cfg]
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird", "output_tuning", 0x00010001, 0x80010009

;cfg idx 21
[DriverInstallx86_505c17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_505c17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_505c17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_505c17aa;, EventLogService

[DriverServicex86_505c17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 505c17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_505c17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_505c17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_505c17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_505c17aa;, EventLogService

[DriverServicex64_505c17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 505c17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[505c17aa_cfg]
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird", "output_tuning", 0x00010001, 0x8001000a


;cfg idx 22 
[DriverInstallx86_609517aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_609517aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 609517aa_cfg_pcr

[DriverInstallx86_609517aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_609517aa;, EventLogService

[DriverServicex86_609517aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 609517aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_609517aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_609517aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 609517aa_cfg_pcr

[DriverInstallx64_609517aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_609517aa;, EventLogService

[DriverServicex64_609517aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 609517aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[609517aa_cfg]
HKR,"seaeagle", "driver_item", 0x00010001, 0x8000001a
HKR,"seaeagle", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seaeagle", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seaeagle", "MMC_MODE_DIS", 0x00010001, 0x80000000
HKR,"seaeagle", "output_tuning", 0x00010001, 0x80110000

[609517aa_cfg_pcr]
HKR,"seaeagle\pcr", "pcr_value", 1, 00,00,03,00,00,ff,00,44,00,00,03,e0,00,40,00,00


;cfg idx 23
[DriverInstallx86_607E17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_607E17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 607E17aa_cfg_pcr

[DriverInstallx86_607E17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_607E17aa;, EventLogService

[DriverServicex86_607E17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 607E17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_607E17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_607E17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 607E17aa_cfg_pcr

[DriverInstallx64_607E17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_607E17aa;, EventLogService

[DriverServicex64_607E17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 607E17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[607E17aa_cfg]
HKR,"seaeagle", "driver_item", 0x00010001, 0x8000001a
HKR,"seaeagle", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seaeagle", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seaeagle", "MMC_MODE_DIS", 0x00010001, 0x80000000
HKR,"seaeagle", "output_tuning", 0x00010001, 0x80110000

[607E17aa_cfg_pcr]
HKR,"seaeagle\pcr", "pcr_value", 1, 00,00,03,00,00,ff,00,44,00,00,03,e0,00,40,00,00


;cfg idx 24
[DriverInstallx86_369417aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_369417aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 369417aa_cfg_pcr

[DriverInstallx86_369417aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_369417aa;, EventLogService

[DriverServicex86_369417aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 369417aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_369417aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_369417aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 369417aa_cfg_pcr

[DriverInstallx64_369417aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_369417aa;, EventLogService

[DriverServicex64_369417aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 369417aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[369417aa_cfg]
HKR,"seaeagle", "driver_item", 0x00010001, 0x8000001a
HKR,"seaeagle", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seaeagle", "MS_SDIO_CTRL", 0x00010001, 0x0

[369417aa_cfg_pcr]
HKR,"seaeagle\pcr", "pcr_value", 1, 00,00,03,00,00,ff,00,44,00,00,03,e0,00,40,00,00


;cfg idx 25
[DriverInstallx86_505417aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_505417aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 505417aa_cfg_pcr

[DriverInstallx86_505417aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_505417aa;, EventLogService

[DriverServicex86_505417aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 505417aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_505417aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_505417aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 505417aa_cfg_pcr

[DriverInstallx64_505417aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_505417aa;, EventLogService

[DriverServicex64_505417aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 505417aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[505417aa_cfg]
HKR,"seaeagle", "driver_item", 0x00010001, 0x8000001a
HKR,"seaeagle", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seaeagle", "MS_SDIO_CTRL", 0x00010001, 0x0

[505417aa_cfg_pcr]
HKR,"seaeagle\pcr", "pcr_value", 1, 00,00,03,00,00,ff,00,44,00,00,03,e0,00,40,00,00


;cfg idx 26 
[DriverInstallx86_380317aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_380317aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_380317aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_380317aa;, EventLogService

[DriverServicex86_380317aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 380317aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_380317aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_380317aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_380317aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_380317aa;, EventLogService

[DriverServicex64_380317aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 380317aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[380317aa_cfg]
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001


;cfg idx 27
[DriverInstallx86_20648086.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_20648086.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_20648086.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_20648086;, EventLogService

[DriverServicex86_20648086]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 20648086_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_20648086.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_20648086.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_20648086.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_20648086;, EventLogService

[DriverServicex64_20648086]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 20648086_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[20648086_cfg]
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x80000000


;cfg idx 30 
[DriverInstallx86_380117aa_8621.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_380117aa_8621.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 380117aa_8621_cfg_pcr

[DriverInstallx86_380117aa_8621.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_380117aa_8621;, EventLogService

[DriverServicex86_380117aa_8621]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 380117aa_8621_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_380117aa_8621.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_380117aa_8621.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 380117aa_8621_cfg_pcr

[DriverInstallx64_380117aa_8621.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_380117aa_8621;, EventLogService

[DriverServicex64_380117aa_8621]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 380117aa_8621_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[380117aa_8621_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[380117aa_8621_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,00,ff,00,55,00,00,00,e2,f0,00,10,00,00,00,00,fe,00,0f,00,0c,00,00,03,e6,00,08,00,08


;cfg idx 31 
[DriverInstallx86_380217aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_380217aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 380217aa_cfg_pcr

[DriverInstallx86_380217aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_380217aa;, EventLogService

[DriverServicex86_380217aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 380217aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_380217aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_380217aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 380217aa_cfg_pcr

[DriverInstallx64_380217aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_380217aa;, EventLogService

[DriverServicex64_380217aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 380217aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[380217aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[380217aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,00,ff,00,55,00,00,00,e2,f0,00,10,00,00,00,00,fe,00,0f,00,0c,00,00,03,e6,00,08,00,08


;cfg idx 32 
[DriverInstallx86_380417aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_380417aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 380417aa_cfg_pcr

[DriverInstallx86_380417aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_380417aa;, EventLogService

[DriverServicex86_380417aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 380417aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_380417aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_380417aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 380417aa_cfg_pcr

[DriverInstallx64_380417aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_380417aa;, EventLogService

[DriverServicex64_380417aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 380417aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[380417aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[380417aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,00,ff,00,55,00,00,00,e2,f0,00,10,00,00,00,00,fe,00,0f,00,0c,00,00,03,e6,00,08,00,08


;cfg idx 33 
[DriverInstallx86_60ae17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_60ae17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 60ae17aa_cfg_pcr

[DriverInstallx86_60ae17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_60ae17aa;, EventLogService

[DriverServicex86_60ae17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 60ae17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_60ae17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_60ae17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 60ae17aa_cfg_pcr

[DriverInstallx64_60ae17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_60ae17aa;, EventLogService

[DriverServicex64_60ae17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 60ae17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[60ae17aa_cfg]
HKR,"seaeagle", "driver_item", 0x00010001, 0x8000001a
HKR,"seaeagle", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seaeagle", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seaeagle", "MMC_MODE_DIS", 0x00010001, 0x80000000
HKR,"seaeagle", "output_tuning", 0x00010001, 0x80110000

[60ae17aa_cfg_pcr]
HKR,"seaeagle\pcr", "pcr_value", 1, 00,00,03,00,00,ff,00,44,00,00,03,e0,00,40,00,00


;cfg idx 34 
[DriverInstallx86_06251028.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_06251028.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 06251028_cfg_pcr

[DriverInstallx86_06251028.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_06251028;, EventLogService

[DriverServicex86_06251028]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 06251028_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_06251028.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_06251028.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 06251028_cfg_pcr

[DriverInstallx64_06251028.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_06251028;, EventLogService

[DriverServicex64_06251028]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 06251028_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[06251028_cfg]
HKR,"seaeagle", "driver_item", 0x00010001, 0x8000001a
HKR,"seaeagle", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seaeagle", "output_tuning", 0x00010001, 0x8001000b
HKR,"seaeagle", "power_wait_time", 0x00010001, 0x015e000a

[06251028_cfg_pcr]
HKR,"seaeagle\pcr", "pcr_value", 1, 00,00,03,00,00,ff,00,44,00,00,03,e0,00,40,00,00,00,00,03,04,70,70,20,20


;cfg idx 35 
[DriverInstallx86_06261028.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_06261028.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 06261028_cfg_pcr

[DriverInstallx86_06261028.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_06261028;, EventLogService

[DriverServicex86_06261028]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 06261028_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_06261028.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_06261028.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 06261028_cfg_pcr

[DriverInstallx64_06261028.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_06261028;, EventLogService

[DriverServicex64_06261028]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 06261028_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[06261028_cfg]
HKR,"seaeagle", "driver_item", 0x00010001, 0x8000001a
HKR,"seaeagle", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seaeagle", "output_tuning", 0x00010001, 0x8001000b
HKR,"seaeagle", "power_wait_time", 0x00010001, 0x015e000a

[06261028_cfg_pcr]
HKR,"seaeagle\pcr", "pcr_value", 1, 00,00,03,00,00,ff,00,44,00,00,03,e0,00,40,00,00,00,00,03,04,70,70,20,20


;cfg idx 36 
[DriverInstallx86_060f1028.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_060f1028.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 060f1028_cfg_pcr

[DriverInstallx86_060f1028.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_060f1028;, EventLogService

[DriverServicex86_060f1028]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 060f1028_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_060f1028.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_060f1028.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 060f1028_cfg_pcr

[DriverInstallx64_060f1028.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_060f1028;, EventLogService

[DriverServicex64_060f1028]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 060f1028_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[060f1028_cfg]
HKR,"seaeagle", "driver_item", 0x00010001, 0x8000001a
HKR,"seaeagle", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seaeagle", "output_tuning", 0x00010001, 0x8001000b
HKR,"seaeagle", "power_wait_time", 0x00010001, 0x015e000a


[060f1028_cfg_pcr]
HKR,"seaeagle\pcr", "pcr_value", 1, 00,00,03,00,00,ff,00,44,00,00,03,e0,00,40,00,00,00,00,03,04,70,70,20,20


;cfg idx 37 
[DriverInstallx86_062f1028.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_062f1028.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 062f1028_cfg_pcr

[DriverInstallx86_062f1028.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_062f1028;, EventLogService

[DriverServicex86_062f1028]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 062f1028_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_062f1028.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_062f1028.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 062f1028_cfg_pcr

[DriverInstallx64_062f1028.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_062f1028;, EventLogService

[DriverServicex64_062f1028]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 062f1028_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[062f1028_cfg]
HKR,"seaeagle", "driver_item", 0x00010001, 0x8000001a
HKR,"seaeagle", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seaeagle", "output_tuning", 0x00010001, 0x8001000b
HKR,"seaeagle", "power_wait_time", 0x00010001, 0x015e000a

[062f1028_cfg_pcr]
HKR,"seaeagle\pcr", "pcr_value", 1, 00,00,03,00,00,ff,00,44,00,00,03,e0,00,40,00,00,00,00,03,04,70,70,20,20


;cfg idx 38 
[DriverInstallx86_06101028.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_06101028.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 06101028_cfg_pcr

[DriverInstallx86_06101028.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_06101028;, EventLogService

[DriverServicex86_06101028]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 06101028_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_06101028.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_06101028.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 06101028_cfg_pcr

[DriverInstallx64_06101028.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_06101028;, EventLogService

[DriverServicex64_06101028]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 06101028_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[06101028_cfg]
HKR,"seaeagle", "driver_item", 0x00010001, 0x8000001a
HKR,"seaeagle", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seaeagle", "output_tuning", 0x00010001, 0x8001000b
HKR,"seaeagle", "power_wait_time", 0x00010001, 0x015e000a

[06101028_cfg_pcr]
HKR,"seaeagle\pcr", "pcr_value", 1, 00,00,03,00,00,ff,00,44,00,00,03,e0,00,40,00,00,00,00,03,04,70,70,20,20


;cfg idx 39 
[DriverInstallx86_224917aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_224917aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 224917aa_cfg_pcr

[DriverInstallx86_224917aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_224917aa;, EventLogService

[DriverServicex86_224917aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 224917aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_224917aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_224917aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 224917aa_cfg_pcr

[DriverInstallx64_224917aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_224917aa;, EventLogService

[DriverServicex64_224917aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 224917aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[224917aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird", "output_tuning", 0x00010001, 0x8001000a

[224917aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,00,55,00,00,00,e2,f0,00,10,00,00,00,00,fe,00,0f,00,0c,00,00,03,e6,00,08,00,08


;cfg idx 40 
[DriverInstallx86_224a17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_224a17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 224a17aa_cfg_pcr

[DriverInstallx86_224a17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_224a17aa;, EventLogService

[DriverServicex86_224a17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 224a17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_224a17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_224a17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 224a17aa_cfg_pcr

[DriverInstallx64_224a17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_224a17aa;, EventLogService

[DriverServicex64_224a17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 224a17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[224a17aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird", "output_tuning", 0x00010001, 0x8001000a

[224a17aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,00,55,00,00,00,e2,f0,00,10,00,00,00,00,fe,00,0f,00,0c,00,00,03,e6,00,08,00,08


;cfg idx 41 
[DriverInstallx86_506617aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_506617aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 506617aa_cfg_pcr

[DriverInstallx86_506617aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_506617aa;, EventLogService

[DriverServicex86_506617aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 506617aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_506617aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_506617aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 506617aa_cfg_pcr

[DriverInstallx64_506617aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_506617aa;, EventLogService

[DriverServicex64_506617aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 506617aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[506617aa_cfg]
HKR,"seaeagle", "driver_item", 0x00010001, 0x8000001a
HKR,"seaeagle", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seaeagle", "MS_SDIO_CTRL", 0x00010001, 0x0

[506617aa_cfg_pcr]
HKR,"seaeagle\pcr", "pcr_value", 1, 00,00,03,00,00,ff,00,44,00,00,03,e0,00,40,00,00


;cfg idx 47 
[DriverInstallx86_381f17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_381f17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 381f17aa_cfg_pcr

[DriverInstallx86_381f17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_381f17aa;, EventLogService

[DriverServicex86_381f17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 381f17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_381f17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_381f17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 381f17aa_cfg_pcr

[DriverInstallx64_381f17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_381f17aa;, EventLogService

[DriverServicex64_381f17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 381f17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[381f17aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird", "output_tuning", 0x00010001, 0x8001000a

[381f17aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,00,ff,60,55,00,00,00,e2,f0,00,10,00,00,00,00,fe,00,0f,00,0c,00,00,03,e6,00,08,00,08


;cfg idx 48 
[DriverInstallx86_382017aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_382017aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 382017aa_cfg_pcr

[DriverInstallx86_382017aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_382017aa;, EventLogService

[DriverServicex86_382017aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 382017aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_382017aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_382017aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 382017aa_cfg_pcr

[DriverInstallx64_382017aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_382017aa;, EventLogService

[DriverServicex64_382017aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 382017aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[382017aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[382017aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,00,ff,60,55,00,00,00,e2,f0,00,10,00,00,00,00,fe,00,0f,00,0c,00,00,03,e6,00,08,00,08


;cfg idx 49 
[DriverInstallx86_388117aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_388117aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 388117aa_cfg_pcr

[DriverInstallx86_388117aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_388117aa;, EventLogService

[DriverServicex86_388117aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 388117aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_388117aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_388117aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 388117aa_cfg_pcr

[DriverInstallx64_388117aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_388117aa;, EventLogService

[DriverServicex64_388117aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 388117aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[388117aa_cfg]
HKR,"seaeagle", "driver_item", 0x00010001, 0x8000001a
HKR,"seaeagle", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seaeagle", "MS_SDIO_CTRL", 0x00010001, 0x0

[388117aa_cfg_pcr]
HKR,"seaeagle\pcr", "pcr_value", 1, 00,00,03,00,00,ff,00,44,00,00,03,e0,00,40,00,00


;cfg idx 50 
[DriverInstallx86_380317aa_8621.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_380317aa_8621.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 380317aa_8621_cfg_pcr

[DriverInstallx86_380317aa_8621.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_380317aa_8621;, EventLogService

[DriverServicex86_380317aa_8621]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 380317aa_8621_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_380317aa_8621.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_380317aa_8621.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 380317aa_8621_cfg_pcr

[DriverInstallx64_380317aa_8621.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_380317aa_8621;, EventLogService

[DriverServicex64_380317aa_8621]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 380317aa_8621_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[380317aa_8621_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[380317aa_8621_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 51 
[DriverInstallx86_381217aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_381217aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 381217aa_cfg_pcr

[DriverInstallx86_381217aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_381217aa;, EventLogService

[DriverServicex86_381217aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 381217aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_381217aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_381217aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 381217aa_cfg_pcr

[DriverInstallx64_381217aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_381217aa;, EventLogService

[DriverServicex64_381217aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 381217aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[381217aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[381217aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 52 
[DriverInstallx86_740017aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_740017aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 740017aa_cfg_pcr

[DriverInstallx86_740017aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_740017aa;, EventLogService

[DriverServicex86_740017aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 740017aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_740017aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_740017aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 740017aa_cfg_pcr

[DriverInstallx64_740017aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_740017aa;, EventLogService

[DriverServicex64_740017aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 740017aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[740017aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[740017aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,00,48,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 53 
[DriverInstallx86_381c17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_381c17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 381c17aa_cfg_pcr

[DriverInstallx86_381c17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_381c17aa;, EventLogService

[DriverServicex86_381c17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 381c17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_381c17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_381c17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 381c17aa_cfg_pcr

[DriverInstallx64_381c17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_381c17aa;, EventLogService

[DriverServicex64_381c17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 381c17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[381c17aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0


[381c17aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,00,48,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 54 
[DriverInstallx86_11881025.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_11881025.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 11881025_cfg_pcr

[DriverInstallx86_11881025.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_11881025;, EventLogService

[DriverServicex86_11881025]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 11881025_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_11881025.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_11881025.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 11881025_cfg_pcr

[DriverInstallx64_11881025.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_11881025;, EventLogService

[DriverServicex64_11881025]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 11881025_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[11881025_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0         
HKR,"seabird", "MMC_MODE_DIS", 0x00010001, 0x80000000

[11881025_cfg_pcr]                                                                                                             
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,00,48,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 55 
[DriverInstallx86_11891025.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_11891025.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 11891025_cfg_pcr

[DriverInstallx86_11891025.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_11891025;, EventLogService

[DriverServicex86_11891025]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 11891025_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_11891025.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_11891025.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 11891025_cfg_pcr

[DriverInstallx64_11891025.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_11891025;, EventLogService

[DriverServicex64_11891025]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 11891025_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[11891025_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0                                   
HKR,"seabird", "MMC_MODE_DIS", 0x00010001, 0x80000000

[11891025_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,00,48,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 56 
[DriverInstallx86_506817aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_506817aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 506817aa_cfg_pcr

[DriverInstallx86_506817aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_506817aa;, EventLogService

[DriverServicex86_506817aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 506817aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_506817aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_506817aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 506817aa_cfg_pcr

[DriverInstallx64_506817aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_506817aa;, EventLogService

[DriverServicex64_506817aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 506817aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[506817aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[506817aa_cfg_pcr]                            
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,ff,ff,21,33,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 57 
[DriverInstallx86_380517aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_380517aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 380517aa_cfg_pcr

[DriverInstallx86_380517aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_380517aa;, EventLogService

[DriverServicex86_380517aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 380517aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_380517aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_380517aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 380517aa_cfg_pcr

[DriverInstallx64_380517aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_380517aa;, EventLogService

[DriverServicex64_380517aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 380517aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[380517aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird", "output_tuning",0x00010001, 0x80010009

[380517aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 58 
[DriverInstallx86_506a17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_506a17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 506a17aa_cfg_pcr

[DriverInstallx86_506a17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_506a17aa;, EventLogService

[DriverServicex86_506a17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 506a17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_506a17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_506a17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 506a17aa_cfg_pcr

[DriverInstallx64_506a17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_506a17aa;, EventLogService

[DriverServicex64_506a17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 506a17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[506a17aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0


[506a17aa_cfg_pcr]                      
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,ff,ff,21,33,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 59 
[DriverInstallx86_506f17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_506f17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 506f17aa_cfg_pcr

[DriverInstallx86_506f17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_506f17aa;, EventLogService

[DriverServicex86_506f17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 506f17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_506f17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_506f17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 506f17aa_cfg_pcr

[DriverInstallx64_506f17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_506f17aa;, EventLogService

[DriverServicex64_506f17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 506f17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[506f17aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0     

[506f17aa_cfg_pcr]                              
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,ff,ff,21,33,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 60 
[DriverInstallx86_60cd17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_60cd17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 60cd17aa_cfg_pcr

[DriverInstallx86_60cd17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_60cd17aa;, EventLogService

[DriverServicex86_60cd17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 60cd17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_60cd17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_60cd17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 60cd17aa_cfg_pcr

[DriverInstallx64_60cd17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_60cd17aa;, EventLogService

[DriverServicex64_60cd17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 60cd17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[60cd17aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird", "MMC_MODE_DIS", 0x00010001, 0x80000000
HKR,"seabird", "output_tuning", 0x00010001, 0x80110000
HKR,"seabird", "LTR_C10_Patch", 0x00010001, 0x80000000

[60cd17aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 61 
[DriverInstallx86_380717aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_380717aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 380717aa_cfg_pcr

[DriverInstallx86_380717aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_380717aa;, EventLogService

[DriverServicex86_380717aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_380717aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_380717aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 380717aa_cfg_pcr

[DriverInstallx64_380717aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_380717aa;, EventLogService

[DriverServicex64_380717aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = bus_type
AddReg         = autorun_addreg

[380717aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 62
[DriverInstallx86_226117aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_226117aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 226117aa_cfg_pcr

[DriverInstallx86_226117aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_226117aa;, EventLogService

[DriverServicex86_226117aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 226117aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_226117aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_226117aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 226117aa_cfg_pcr

[DriverInstallx64_226117aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_226117aa;, EventLogService

[DriverServicex64_226117aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 226117aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[226117aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[226117aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 63
[DriverInstallx86_20738086.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_20738086.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 20738086_cfg_pcr

[DriverInstallx86_20738086.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_20738086;, EventLogService

[DriverServicex86_20738086]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelDiskReg         = cfg_DelDiskReg
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 20738086_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_20738086.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_20738086.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 20738086_cfg_pcr

[DriverInstallx64_20738086.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_20738086;, EventLogService

[DriverServicex64_20738086]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelDiskReg         = cfg_DelDiskReg
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 20738086_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[20738086_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0     
HKR,"seabird", "sw_write_protect", 0x00010001, 0x80000000

[20738086_cfg_pcr]                                                                                                                     
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,00,48,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 64
[DriverInstallx86_12301025.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_12301025.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 12301025_cfg_pcr

[DriverInstallx86_12301025.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_12301025;, EventLogService

[DriverServicex86_12301025]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 12301025_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_12301025.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_12301025.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 12301025_cfg_pcr

[DriverInstallx64_12301025.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_12301025;, EventLogService

[DriverServicex64_12301025]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 12301025_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[12301025_cfg]
HKR,"seabird", "MMC_MODE_DIS", 0x00010001, 0x80000000 
HKR,"seabird", "output_tuning", 0x00010001, 0x80010009   

[12301025_cfg_pcr]                                                                                                                      
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 65
[DriverInstallx86_380617aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_380617aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 380617aa_cfg_pcr

[DriverInstallx86_380617aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_380617aa;, EventLogService

[DriverServicex86_380617aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 380617aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_380617aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_380617aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 380617aa_cfg_pcr

[DriverInstallx64_380617aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_380617aa;, EventLogService

[DriverServicex64_380617aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 380617aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[380617aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[380617aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 66
[DriverInstallx86_380417aa_8621.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_380417aa_8621.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 380417aa_8621_cfg_pcr

[DriverInstallx86_380417aa_8621.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_380417aa_8621;, EventLogService

[DriverServicex86_380417aa_8621]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 380417aa_8621_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_380417aa_8621.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_380417aa_8621.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 380417aa_8621_cfg_pcr

[DriverInstallx64_380417aa_8621.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_380417aa_8621;, EventLogService

[DriverServicex64_380417aa_8621]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 380417aa_8621_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[380417aa_8621_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[380417aa_8621_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 67
[DriverInstallx86_380817aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_380817aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 380817aa_cfg_pcr

[DriverInstallx86_380817aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_380817aa;, EventLogService

[DriverServicex86_380817aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 380817aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_380817aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_380817aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 380817aa_cfg_pcr

[DriverInstallx64_380817aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_380817aa;, EventLogService

[DriverServicex64_380817aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 380817aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[380817aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[380817aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 68
[DriverInstallx86_384617aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_384617aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 384617aa_cfg_pcr

[DriverInstallx86_384617aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_384617aa;, EventLogService

[DriverServicex86_384617aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 384617aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_384617aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_384617aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 384617aa_cfg_pcr

[DriverInstallx64_384617aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_384617aa;, EventLogService

[DriverServicex64_384617aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 384617aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[384617aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[384617aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08
HKR,"seabird\dmdn", "dmdn_value", 1, 2f,2e,00,02


;cfg idx 69
[DriverInstallx86_227317aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_227317aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 227317aa_cfg_pcr

[DriverInstallx86_227317aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_227317aa;, EventLogService

[DriverServicex86_227317aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 227317aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_227317aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_227317aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 227317aa_cfg_pcr

[DriverInstallx64_227317aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_227317aa;, EventLogService

[DriverServicex64_227317aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 227317aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[227317aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[227317aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 70
[DriverInstallx86_380917aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_380917aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx86_380917aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_380917aa;, EventLogService

[DriverServicex86_380917aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 380917aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_380917aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_380917aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues

[DriverInstallx64_380917aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_380917aa;, EventLogService

[DriverServicex64_380917aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 380917aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[380917aa_cfg]
HKR,"seabird", "psd_mode", 0x00010001, 0x80000000


;cfg idx 71
[DriverInstallx86_39f617aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_39f617aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 39f617aa_cfg_pcr

[DriverInstallx86_39f617aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_39f617aa;, EventLogService

[DriverServicex86_39f617aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 39f617aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_39f617aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_39f617aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 39f617aa_cfg_pcr

[DriverInstallx64_39f617aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_39f617aa;, EventLogService

[DriverServicex64_39f617aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 39f617aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[39f617aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird", "output_tuning", 0x00010001, 0x8001000a

[39f617aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 72
[DriverInstallx86_381317aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_381317aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 381317aa_cfg_pcr

[DriverInstallx86_381317aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_381317aa;, EventLogService

[DriverServicex86_381317aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 381317aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_381317aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_381317aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 381317aa_cfg_pcr

[DriverInstallx64_381317aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_381317aa;, EventLogService

[DriverServicex64_381317aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 381317aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[381317aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird", "output_tuning", 0x00010001, 0x8001000a

[381317aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 73
[DriverInstallx86_382417aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_382417aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 382417aa_cfg_pcr

[DriverInstallx86_382417aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_382417aa;, EventLogService

[DriverServicex86_382417aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 382417aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_382417aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_382417aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 382417aa_cfg_pcr

[DriverInstallx64_382417aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_382417aa;, EventLogService

[DriverServicex64_382417aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 382417aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[382417aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird", "output_tuning", 0x00010001, 0x8001000a

[382417aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 74
[DriverInstallx86_382117aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_382117aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 382117aa_cfg_pcr

[DriverInstallx86_382117aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_382117aa;, EventLogService

[DriverServicex86_382117aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 382117aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_382117aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_382117aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 382117aa_cfg_pcr

[DriverInstallx64_382117aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_382117aa;, EventLogService

[DriverServicex64_382117aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 382117aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[382117aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird", "output_tuning", 0x00010001, 0x8001000a

[382117aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 75
[DriverInstallx86_507517aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_507517aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 507517aa_cfg_pcr

[DriverInstallx86_507517aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_507517aa;, EventLogService

[DriverServicex86_507517aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 507517aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_507517aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_507517aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 507517aa_cfg_pcr

[DriverInstallx64_507517aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_507517aa;, EventLogService

[DriverServicex64_507517aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 507517aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[507517aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[507517aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 76 update on 20190724
[DriverInstallx86_383e17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_383e17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 383e17aa_cfg_pcr

[DriverInstallx86_383e17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_383e17aa;, EventLogService

[DriverServicex86_383e17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 383e17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_383e17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_383e17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 383e17aa_cfg_pcr

[DriverInstallx64_383e17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_383e17aa;, EventLogService

[DriverServicex64_383e17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 383e17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[383e17aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird", "output_tuning", 0x00010001, 0x8001000a

[383e17aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 77
[DriverInstallx86_381817aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_381817aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 381817aa_cfg_pcr

[DriverInstallx86_381817aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_381817aa;, EventLogService

[DriverServicex86_381817aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 381817aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_381817aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_381817aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 381817aa_cfg_pcr

[DriverInstallx64_381817aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_381817aa;, EventLogService

[DriverServicex64_381817aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 381817aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[381817aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird", "output_tuning", 0x00010001, 0x8001000a

[381817aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 78
[DriverInstallx86_381417aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_381417aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 381417aa_cfg_pcr

[DriverInstallx86_381417aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_381417aa;, EventLogService

[DriverServicex86_381417aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 381417aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_381417aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_381417aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 381417aa_cfg_pcr

[DriverInstallx64_381417aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_381417aa;, EventLogService

[DriverServicex64_381417aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 381417aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[381417aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird", "output_tuning", 0x00010001, 0x8001000a

[381417aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 79  update on 20190724
[DriverInstallx86_380f17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_380f17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 380f17aa_cfg_pcr

[DriverInstallx86_380f17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_380f17aa;, EventLogService

[DriverServicex86_380f17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 380f17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_380f17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_380f17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 380f17aa_cfg_pcr

[DriverInstallx64_380f17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_380f17aa;, EventLogService

[DriverServicex64_380f17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 380f17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[380f17aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird", "output_tuning", 0x00010001, 0x8001000a

[380f17aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 80
[DriverInstallx86_507217aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_507217aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 507217aa_cfg_pcr

[DriverInstallx86_507217aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_507217aa;, EventLogService

[DriverServicex86_507217aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 507217aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_507217aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_507217aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 507217aa_cfg_pcr

[DriverInstallx64_507217aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_507217aa;, EventLogService

[DriverServicex64_507217aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 507217aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[507217aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[507217aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,00,36,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 81
[DriverInstallx86_383717aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_383717aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 383717aa_cfg_pcr

[DriverInstallx86_383717aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_383717aa;, EventLogService

[DriverServicex86_383717aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 383717aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_383717aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_383717aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 383717aa_cfg_pcr

[DriverInstallx64_383717aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_383717aa;, EventLogService

[DriverServicex64_383717aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 383717aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[383717aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird", "output_tuning", 0x00010001, 0x8001000a

[383717aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 82
[DriverInstallx86_3a3b17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_3a3b17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 3a3b17aa_cfg_pcr

[DriverInstallx86_3a3b17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_3a3b17aa;, EventLogService

[DriverServicex86_3a3b17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 3a3b17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_3a3b17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_3a3b17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 3a3b17aa_cfg_pcr

[DriverInstallx64_3a3b17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_3a3b17aa;, EventLogService

[DriverServicex64_3a3b17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 3a3b17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[3a3b17aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird", "output_tuning", 0x00010001, 0x8001000a

[3a3b17aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 83
[DriverInstallx86_383517aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_383517aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 383517aa_cfg_pcr

[DriverInstallx86_383517aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_383517aa;, EventLogService

[DriverServicex86_383517aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 383517aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_383517aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_383517aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 383517aa_cfg_pcr

[DriverInstallx64_383517aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_383517aa;, EventLogService

[DriverServicex64_383517aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 383517aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[383517aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird", "output_tuning", 0x00010001, 0x8001000a

[383517aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 84
[DriverInstallx86_382f17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_382f17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 382f17aa_cfg_pcr

[DriverInstallx86_382f17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_382f17aa;, EventLogService

[DriverServicex86_382f17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 382f17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_382f17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_382f17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 382f17aa_cfg_pcr

[DriverInstallx64_382f17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_382f17aa;, EventLogService

[DriverServicex64_382f17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 382f17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[382f17aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[382f17aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,00,36,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 85
[DriverInstallx86_383217aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_383217aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 383217aa_cfg_pcr

[DriverInstallx86_383217aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_383217aa;, EventLogService

[DriverServicex86_383217aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 383217aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_383217aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_383217aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 383217aa_cfg_pcr

[DriverInstallx64_383217aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_383217aa;, EventLogService

[DriverServicex64_383217aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 383217aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[383217aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[383217aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,00,36,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 86
[DriverInstallx86_385217aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_385217aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 385217aa_cfg_pcr

[DriverInstallx86_385217aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_385217aa;, EventLogService

[DriverServicex86_385217aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 385217aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_385217aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_385217aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 385217aa_cfg_pcr

[DriverInstallx64_385217aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_385217aa;, EventLogService

[DriverServicex64_385217aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 385217aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[385217aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[385217aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,00,36,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 87
[DriverInstallx86_385117aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_385117aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 385117aa_cfg_pcr

[DriverInstallx86_385117aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_385117aa;, EventLogService

[DriverServicex86_385117aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 385117aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_385117aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_385117aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 385117aa_cfg_pcr

[DriverInstallx64_385117aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_385117aa;, EventLogService

[DriverServicex64_385117aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 385117aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[385117aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[385117aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,00,36,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 88
[DriverInstallx86_507c17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_507c17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 507c17aa_cfg_pcr

[DriverInstallx86_507c17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_507c17aa;, EventLogService

[DriverServicex86_507c17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 507c17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_507c17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_507c17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 507c17aa_cfg_pcr

[DriverInstallx64_507c17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_507c17aa;, EventLogService

[DriverServicex64_507c17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 507c17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[507c17aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000

[507c17aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,00,36,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 89
[DriverInstallx86_381617aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_381617aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 381617aa_cfg_pcr

[DriverInstallx86_381617aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_381617aa;, EventLogService

[DriverServicex86_381617aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 381617aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_381617aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_381617aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 381617aa_cfg_pcr

[DriverInstallx64_381617aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_381617aa;, EventLogService

[DriverServicex64_381617aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 381617aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[381617aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80000000

[381617aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,00,36,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 90
[DriverInstallx86_507e17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_507e17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 507e17aa_cfg_pcr

[DriverInstallx86_507e17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_507e17aa;, EventLogService

[DriverServicex86_507e17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 507e17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_507e17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_507e17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 507e17aa_cfg_pcr

[DriverInstallx64_507e17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_507e17aa;, EventLogService

[DriverServicex64_507e17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 507e17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[507e17aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000

[507e17aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,00,36


;cfg idx 91
[DriverInstallx86_383117aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_383117aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 383117aa_cfg_pcr

[DriverInstallx86_383117aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_383117aa;, EventLogService

[DriverServicex86_383117aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 383117aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_383117aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_383117aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 383117aa_cfg_pcr

[DriverInstallx64_383117aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_383117aa;, EventLogService

[DriverServicex64_383117aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 383117aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[383117aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "output_tuning", 0x00010001, 0x8001000a

[383117aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,00,36


;cfg idx 92
[DriverInstallx86_381b17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_381b17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 381b17aa_cfg_pcr

[DriverInstallx86_381b17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_381b17aa;, EventLogService

[DriverServicex86_381b17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 381b17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_381b17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_381b17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 381b17aa_cfg_pcr

[DriverInstallx64_381b17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_381b17aa;, EventLogService

[DriverServicex64_381b17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 381b17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[381b17aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "output_tuning", 0x00010001, 0x8001000a

[381b17aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,00,36


;cfg idx 93
[DriverInstallx86_382517aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_382517aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 382517aa_cfg_pcr

[DriverInstallx86_382517aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_382517aa;, EventLogService

[DriverServicex86_382517aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 382517aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_382517aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_382517aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 382517aa_cfg_pcr

[DriverInstallx64_382517aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_382517aa;, EventLogService

[DriverServicex64_382517aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 382517aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[382517aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[382517aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,00,36,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 94
[DriverInstallx86_381717aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_381717aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 381717aa_cfg_pcr

[DriverInstallx86_381717aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_381717aa;, EventLogService

[DriverServicex86_381717aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 381717aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_381717aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_381717aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 381717aa_cfg_pcr

[DriverInstallx64_381717aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_381717aa;, EventLogService

[DriverServicex64_381717aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 381717aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[381717aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird", "output_tuning", 0x00010001, 0x8001000a

[381717aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,00,36,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 95
[DriverInstallx86_382217aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_382217aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 382217aa_cfg_pcr

[DriverInstallx86_382217aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_382217aa;, EventLogService

[DriverServicex86_382217aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 382217aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_382217aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_382217aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 382217aa_cfg_pcr

[DriverInstallx64_382217aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_382217aa;, EventLogService

[DriverServicex64_382217aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 382217aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[382217aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird", "output_tuning", 0x00010001, 0x8001000a

[382217aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,00,36,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 96
[DriverInstallx86_383d17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_383d17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 383d17aa_cfg_pcr

[DriverInstallx86_383d17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_383d17aa;, EventLogService

[DriverServicex86_383d17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 383d17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_383d17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_383d17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 383d17aa_cfg_pcr

[DriverInstallx64_383d17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_383d17aa;, EventLogService

[DriverServicex64_383d17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 383d17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[383d17aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird", "output_tuning", 0x00010001, 0x8001000a

[383d17aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,00,36,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 97
[DriverInstallx86_507b17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_507b17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 507b17aa_cfg_pcr

[DriverInstallx86_507b17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_507b17aa;, EventLogService

[DriverServicex86_507b17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 507b17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_507b17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_507b17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 507b17aa_cfg_pcr

[DriverInstallx64_507b17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_507b17aa;, EventLogService

[DriverServicex64_507b17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 507b17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[507b17aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[507b17aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,00,36,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 98
[DriverInstallx86_381917aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_381917aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 381917aa_cfg_pcr

[DriverInstallx86_381917aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_381917aa;, EventLogService

[DriverServicex86_381917aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 381917aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_381917aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_381917aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 381917aa_cfg_pcr

[DriverInstallx64_381917aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_381917aa;, EventLogService

[DriverServicex64_381917aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 381917aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[381917aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[381917aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,44,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 99
[DriverInstallx86_512417aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_512417aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 512417aa_cfg_pcr

[DriverInstallx86_512417aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_512417aa;, EventLogService

[DriverServicex86_512417aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 512417aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_512417aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_512417aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 512417aa_cfg_pcr

[DriverInstallx64_512417aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_512417aa;, EventLogService

[DriverServicex64_512417aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 512417aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[512417aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "write_data_timeout", 0x00010001, 0x80003ee0
HKR,"seabird", "read_data_timeout", 0x00010001, 0x80003ee0
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[512417aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55


;cfg idx 100
[DriverInstallx86_383a17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_383a17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 383a17aa_cfg_pcr

[DriverInstallx86_383a17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_383a17aa;, EventLogService

[DriverServicex86_383a17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 383a17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_383a17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_383a17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 383a17aa_cfg_pcr

[DriverInstallx64_383a17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_383a17aa;, EventLogService

[DriverServicex64_383a17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 383a17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[383a17aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000

[383a17aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0


;cfg idx 101
[DriverInstallx86_382717aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_382717aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 382717aa_cfg_pcr

[DriverInstallx86_382717aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_382717aa;, EventLogService

[DriverServicex86_382717aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 382717aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_382717aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_382717aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 382717aa_cfg_pcr

[DriverInstallx64_382717aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_382717aa;, EventLogService

[DriverServicex64_382717aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 382717aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[382717aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000

[382717aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0


;cfg idx 102
[DriverInstallx86_380a17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_380a17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 380a17aa_cfg_pcr

[DriverInstallx86_380a17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_380a17aa;, EventLogService

[DriverServicex86_380a17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 380a17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_380a17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_380a17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 380a17aa_cfg_pcr

[DriverInstallx64_380a17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_380a17aa;, EventLogService

[DriverServicex64_380a17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 380a17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[380a17aa_cfg]
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80000000

[380a17aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,44,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 103
[DriverInstallx86_383917aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_383917aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 383917aa_cfg_pcr

[DriverInstallx86_383917aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_383917aa;, EventLogService

[DriverServicex86_383917aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 383917aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_383917aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_383917aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 383917aa_cfg_pcr

[DriverInstallx64_383917aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_383917aa;, EventLogService

[DriverServicex64_383917aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 383917aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[383917aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird", "output_tuning", 0x00010001, 0x8001000a

[383917aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 104
[DriverInstallx86_382617aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_382617aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 382617aa_cfg_pcr

[DriverInstallx86_382617aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_382617aa;, EventLogService

[DriverServicex86_382617aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 382617aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_382617aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_382617aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 382617aa_cfg_pcr

[DriverInstallx64_382617aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_382617aa;, EventLogService

[DriverServicex64_382617aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 382617aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[382617aa_cfg]
HKR,"seabird", "psd_mode", 0x00010001, 0x80000000
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a

[382617aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,00,36


;cfg idx 105
[DriverInstallx86_382917aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_382917aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 382917aa_cfg_pcr

[DriverInstallx86_382917aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_382917aa;, EventLogService

[DriverServicex86_382917aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 382917aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_382917aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_382917aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 382917aa_cfg_pcr

[DriverInstallx64_382917aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_382917aa;, EventLogService

[DriverServicex64_382917aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 382917aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[382917aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[382917aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,00,36,00,00,00,fe,02,0f,02,0e,00,00,03,e2,20,00,20,00,\
                                                      00,00,00,a8,04,00,04,00,00,00,02,34,ff,ff,10,01,00,00,02,36,ff,ff,10,01,00,00,03,f4,00,0f,00,0a,\
                                                      00,00,02,48,00,0f,00,0a,00,00,00,90,01,03,01,03


;cfg idx 106
[DriverInstallx86_509317aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_509317aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 509317aa_cfg_pcr

[DriverInstallx86_509317aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_509317aa;, EventLogService

[DriverServicex86_509317aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 509317aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_509317aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_509317aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 509317aa_cfg_pcr

[DriverInstallx64_509317aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_509317aa;, EventLogService

[DriverServicex64_509317aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 509317aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[509317aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[509317aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,00,36,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 107
[DriverInstallx86_508f17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_508f17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 508f17aa_cfg_pcr

[DriverInstallx86_508f17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_508f17aa;, EventLogService

[DriverServicex86_508f17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 508f17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_508f17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_508f17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 508f17aa_cfg_pcr

[DriverInstallx64_508f17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_508f17aa;, EventLogService

[DriverServicex64_508f17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 508f17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[508f17aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[508f17aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 108
[DriverInstallx86_382817aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_382817aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 382817aa_cfg_pcr

[DriverInstallx86_382817aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_382817aa;, EventLogService

[DriverServicex86_382817aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 382817aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_382817aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_382817aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 382817aa_cfg_pcr

[DriverInstallx64_382817aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_382817aa;, EventLogService

[DriverServicex64_382817aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 382817aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[382817aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[382817aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 109
[DriverInstallx86_382b17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_382b17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 382b17aa_cfg_pcr

[DriverInstallx86_382b17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_382b17aa;, EventLogService

[DriverServicex86_382b17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 382b17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_382b17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_382b17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 382b17aa_cfg_pcr

[DriverInstallx64_382b17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_382b17aa;, EventLogService

[DriverServicex64_382b17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 382b17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[382b17aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[382b17aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,00,36,00,00,00,fe,02,0f,02,0e,\
                                                      00,00,00,a8,04,00,04,00,00,00,02,34,ff,ff,10,01,00,00,02,36,ff,ff,10,01,00,00,03,f4,00,0f,00,0a,\
                                                      00,00,02,48,00,0f,00,0a,00,00,00,90,01,03,01,03


;cfg idx 110
[DriverInstallx86_382d17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_382d17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 382d17aa_cfg_pcr

[DriverInstallx86_382d17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_382d17aa;, EventLogService

[DriverServicex86_382d17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 382d17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_382d17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_382d17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 382d17aa_cfg_pcr

[DriverInstallx64_382d17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_382d17aa;, EventLogService

[DriverServicex64_382d17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 382d17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[382d17aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[382d17aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 111
[DriverInstallx86_383c17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_383c17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 383c17aa_cfg_pcr

[DriverInstallx86_383c17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_383c17aa;, EventLogService

[DriverServicex86_383c17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 383c17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_383c17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_383c17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 383c17aa_cfg_pcr

[DriverInstallx64_383c17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_383c17aa;, EventLogService

[DriverServicex64_383c17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 383c17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[383c17aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0 

[383c17aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 112
[DriverInstallx86_509117aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_509117aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 509117aa_cfg_pcr

[DriverInstallx86_509117aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_509117aa;, EventLogService

[DriverServicex86_509117aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 509117aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_509117aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_509117aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 509117aa_cfg_pcr

[DriverInstallx64_509117aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_509117aa;, EventLogService

[DriverServicex64_509117aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 509117aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[509117aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[509117aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,00,fe,02,0f,02,0e,\
                                                      00,00,00,a8,04,00,04,00,00,00,02,34,ff,ff,10,01,00,00,02,36,ff,ff,10,01,00,00,03,f4,00,0f,00,0a,\
                                                      00,00,02,48,00,0f,00,0a,00,00,00,90,01,03,01,03


;cfg idx 113
[DriverInstallx86_383317aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_383317aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 383317aa_cfg_pcr

[DriverInstallx86_383317aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_383317aa;, EventLogService

[DriverServicex86_383317aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 383317aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_383317aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_383317aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 383317aa_cfg_pcr

[DriverInstallx64_383317aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_383317aa;, EventLogService

[DriverServicex64_383317aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 383317aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[383317aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[383317aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 114
[DriverInstallx86_383017aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_383017aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 383017aa_cfg_pcr

[DriverInstallx86_383017aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_383017aa;, EventLogService

[DriverServicex86_383017aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 383017aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_383017aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_383017aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 383017aa_cfg_pcr

[DriverInstallx64_383017aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_383017aa;, EventLogService

[DriverServicex64_383017aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 383017aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[383017aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[383017aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,44,00,00,00,fe,02,0f,02,0e,\
                                                      00,00,00,a8,04,00,04,00,00,00,02,34,ff,ff,10,01,00,00,02,36,ff,ff,10,01,00,00,03,f4,00,0f,00,0a,\
                                                      00,00,02,48,00,0f,00,0a,00,00,00,90,01,03,01,03


;cfg idx 115
[DriverInstallx86_383b17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_383b17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 383b17aa_cfg_pcr

[DriverInstallx86_383b17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_383b17aa;, EventLogService

[DriverServicex86_383b17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 383b17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_383b17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_383b17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 383b17aa_cfg_pcr

[DriverInstallx64_383b17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_383b17aa;, EventLogService

[DriverServicex64_383b17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 383b17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[383b17aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000

[383b17aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0


;cfg idx 116
[DriverInstallx86_383417aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_383417aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 383417aa_cfg_pcr

[DriverInstallx86_383417aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_383417aa;, EventLogService

[DriverServicex86_383417aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 383417aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_383417aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_383417aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 383417aa_cfg_pcr

[DriverInstallx64_383417aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_383417aa;, EventLogService

[DriverServicex64_383417aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 383417aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[383417aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[383417aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 117
[DriverInstallx86_383f17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_383f17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 383f17aa_cfg_pcr

[DriverInstallx86_383f17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_383f17aa;, EventLogService

[DriverServicex86_383f17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 383f17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_383f17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_383f17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 383f17aa_cfg_pcr

[DriverInstallx64_383f17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_383f17aa;, EventLogService

[DriverServicex64_383f17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 383f17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[383f17aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[383f17aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,00,36,00,00,00,fe,02,0f,02,0e,\
                                                      00,00,00,a8,04,00,04,00,00,00,02,34,ff,ff,10,01,00,00,02,36,ff,ff,10,01,00,00,03,f4,00,0f,00,0a,\
                                                      00,00,02,48,00,0f,00,0a,00,00,00,90,01,03,01,03


;cfg idx 118
[DriverInstallx86_384017aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_384017aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 384017aa_cfg_pcr

[DriverInstallx86_384017aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_384017aa;, EventLogService

[DriverServicex86_384017aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 384017aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_384017aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_384017aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 384017aa_cfg_pcr

[DriverInstallx64_384017aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_384017aa;, EventLogService

[DriverServicex64_384017aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 384017aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[384017aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000

[384017aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0


;cfg idx 119
[DriverInstallx86_384117aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_384117aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 384117aa_cfg_pcr

[DriverInstallx86_384117aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_384117aa;, EventLogService

[DriverServicex86_384117aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 384117aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_384117aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_384117aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 384117aa_cfg_pcr

[DriverInstallx64_384117aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_384117aa;, EventLogService

[DriverServicex64_384117aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 384117aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[384117aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[384117aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 120
[DriverInstallx86_384417aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_384417aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 384417aa_cfg_pcr

[DriverInstallx86_384417aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_384417aa;, EventLogService

[DriverServicex86_384417aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 384417aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_384417aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_384417aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 384417aa_cfg_pcr

[DriverInstallx64_384417aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_384417aa;, EventLogService

[DriverServicex64_384417aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 384417aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[384417aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[384417aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,00,36,00,00,00,fe,02,0f,02,0e,\
                                                      00,00,00,a8,04,00,04,00,00,00,02,34,ff,ff,10,01,00,00,02,36,ff,ff,10,01,00,00,03,f4,00,0f,00,0a,\
                                                      00,00,02,48,00,0f,00,0a,00,00,00,90,01,03,01,03


;cfg idx 121
[DriverInstallx86_384517aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_384517aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 384517aa_cfg_pcr

[DriverInstallx86_384517aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_384517aa;, EventLogService

[DriverServicex86_384517aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 384517aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_384517aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_384517aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 384517aa_cfg_pcr

[DriverInstallx64_384517aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_384517aa;, EventLogService

[DriverServicex64_384517aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 384517aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[384517aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[384517aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,00,36,00,00,00,fe,02,0f,02,0e,\
                                                      00,00,00,a8,04,00,04,00,00,00,02,34,ff,ff,10,01,00,00,02,36,ff,ff,10,01,00,00,03,f4,00,0f,00,0a,\
                                                      00,00,02,48,00,0f,00,0a,00,00,00,90,01,03,01,03


;cfg idx 122
[DriverInstallx86_384717aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_384717aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 384717aa_cfg_pcr

[DriverInstallx86_384717aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_384717aa;, EventLogService

[DriverServicex86_384717aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 384717aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_384717aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_384717aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 384717aa_cfg_pcr

[DriverInstallx64_384717aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_384717aa;, EventLogService

[DriverServicex64_384717aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 384717aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[384717aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[384717aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 123
[DriverInstallx86_384917aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_384917aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 384917aa_cfg_pcr

[DriverInstallx86_384917aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_384917aa;, EventLogService

[DriverServicex86_384917aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 384917aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_384917aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_384917aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 384917aa_cfg_pcr

[DriverInstallx64_384917aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_384917aa;, EventLogService

[DriverServicex64_384917aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 384917aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[384917aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[384917aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,00,36,00,00,00,fe,02,0f,02,0e,\
                                                      00,00,00,a8,04,00,04,00,00,00,02,34,ff,ff,10,01,00,00,02,36,ff,ff,10,01,00,00,03,f4,00,0f,00,0a,\
                                                      00,00,02,48,00,0f,00,0a,00,00,00,90,01,03,01,03


;cfg idx 124
[DriverInstallx86_384b17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_384b17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 384b17aa_cfg_pcr

[DriverInstallx86_384b17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_384b17aa;, EventLogService

[DriverServicex86_384b17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 384b17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_384b17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_384b17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 384b17aa_cfg_pcr

[DriverInstallx64_384b17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_384b17aa;, EventLogService

[DriverServicex64_384b17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 384b17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[384b17aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[384b17aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,00,36,00,00,00,fe,02,0f,02,0e,\
                                                      00,00,00,a8,04,00,04,00,00,00,02,34,ff,ff,10,01,00,00,02,36,ff,ff,10,01,00,00,03,f4,00,0f,00,0a,\
                                                      00,00,02,48,00,0f,00,0a,00,00,00,90,01,03,01,03


;cfg idx 125
[DriverInstallx86_384c17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_384c17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 384c17aa_cfg_pcr

[DriverInstallx86_384c17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_384c17aa;, EventLogService

[DriverServicex86_384c17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 384c17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_384c17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_384c17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 384c17aa_cfg_pcr

[DriverInstallx64_384c17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_384c17aa;, EventLogService

[DriverServicex64_384c17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 384c17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[384c17aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[384c17aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 126
[DriverInstallx86_50e11558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_50e11558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 50e11558_cfg_pcr

[DriverInstallx86_50e11558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_50e11558;, EventLogService

[DriverServicex86_50e11558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 50e11558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_50e11558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_50e11558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 50e11558_cfg_pcr

[DriverInstallx64_50e11558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_50e11558;, EventLogService

[DriverServicex64_50e11558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 50e11558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[50e11558_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[50e11558_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 127
[DriverInstallx86_50e21558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_50e21558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 50e21558_cfg_pcr

[DriverInstallx86_50e21558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_50e21558;, EventLogService

[DriverServicex86_50e21558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 50e21558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_50e21558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_50e21558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 50e21558_cfg_pcr

[DriverInstallx64_50e21558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_50e21558;, EventLogService

[DriverServicex64_50e21558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 50e21558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[50e21558_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[50e21558_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 128
[DriverInstallx86_50151558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_50151558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 50151558_cfg_pcr

[DriverInstallx86_50151558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_50151558;, EventLogService

[DriverServicex86_50151558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 50151558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_50151558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_50151558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 50151558_cfg_pcr

[DriverInstallx64_50151558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_50151558;, EventLogService

[DriverServicex64_50151558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 50151558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[50151558_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[50151558_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 129
[DriverInstallx86_50171558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_50171558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 50171558_cfg_pcr

[DriverInstallx86_50171558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_50171558;, EventLogService

[DriverServicex86_50171558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 50171558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_50171558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_50171558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 50171558_cfg_pcr

[DriverInstallx64_50171558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_50171558;, EventLogService

[DriverServicex64_50171558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 50171558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[50171558_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[50171558_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 130
[DriverInstallx86_866b1558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_866b1558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 866b1558_cfg_pcr

[DriverInstallx86_866b1558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_866b1558;, EventLogService

[DriverServicex86_866b1558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 866b1558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_866b1558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_866b1558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 866b1558_cfg_pcr

[DriverInstallx64_866b1558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_866b1558;, EventLogService

[DriverServicex64_866b1558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 866b1558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[866b1558_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[866b1558_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 131
[DriverInstallx86_867b1558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_867b1558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 867b1558_cfg_pcr

[DriverInstallx86_867b1558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_867b1558;, EventLogService

[DriverServicex86_867b1558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 867b1558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_867b1558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_867b1558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 867b1558_cfg_pcr

[DriverInstallx64_867b1558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_867b1558;, EventLogService

[DriverServicex64_867b1558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 867b1558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[867b1558_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[867b1558_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 132
[DriverInstallx86_00021217.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_00021217.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 00021217_cfg_pcr

[DriverInstallx86_00021217.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_00021217;, EventLogService

[DriverServicex86_00021217]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 00021217_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_00021217.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_00021217.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 00021217_cfg_pcr

[DriverInstallx64_00021217.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_00021217;, EventLogService

[DriverServicex64_00021217]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 00021217_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[00021217_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[00021217_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0


;cfg idx 133
[DriverInstallx86_85111558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_85111558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 85111558_cfg_pcr

[DriverInstallx86_85111558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_85111558;, EventLogService

[DriverServicex86_85111558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 85111558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_85111558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_85111558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 85111558_cfg_pcr

[DriverInstallx64_85111558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_85111558;, EventLogService

[DriverServicex64_85111558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 85111558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[85111558_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[85111558_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 134
[DriverInstallx86_87111558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_87111558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 87111558_cfg_pcr

[DriverInstallx86_87111558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_87111558;, EventLogService

[DriverServicex86_87111558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 87111558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_87111558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_87111558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 87111558_cfg_pcr

[DriverInstallx64_87111558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_87111558;, EventLogService

[DriverServicex64_87111558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 87111558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[87111558_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[87111558_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 135
[DriverInstallx86_50f41558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_50f41558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 50f41558_cfg_pcr

[DriverInstallx86_50f41558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_50f41558;, EventLogService

[DriverServicex86_50f41558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 50f41558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_50f41558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_50f41558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 50f41558_cfg_pcr

[DriverInstallx64_50f41558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_50f41558;, EventLogService

[DriverServicex64_50f41558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 50f41558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[50f41558_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[50f41558_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,00,fe,02,0f,02,0e,\
                                                      00,00,00,a8,04,00,04,00,00,00,02,34,ff,ff,10,01,00,00,02,36,ff,ff,10,01,00,00,03,f4,00,0f,00,0a,\
                                                      00,00,02,48,00,0f,00,0a,00,00,00,90,01,03,01,03,00,00,03,e6,01,00,00,00,00,00,03,e2,00,01,00,00


;cfg idx 136
[DriverInstallx86_50c51558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_50c51558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 50c51558_cfg_pcr

[DriverInstallx86_50c51558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_50c51558;, EventLogService

[DriverServicex86_50c51558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 50c51558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_50c51558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_50c51558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 50c51558_cfg_pcr

[DriverInstallx64_50c51558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_50c51558;, EventLogService

[DriverServicex64_50c51558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 50c51558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[50c51558_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[50c51558_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 137
[DriverInstallx86_51a11558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_51a11558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 51a11558_cfg_pcr

[DriverInstallx86_51a11558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_51a11558;, EventLogService

[DriverServicex86_51a11558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 51a11558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_51a11558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_51a11558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 51a11558_cfg_pcr

[DriverInstallx64_51a11558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_51a11558;, EventLogService

[DriverServicex64_51a11558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 51a11558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[51a11558_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[51a11558_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 138
[DriverInstallx86_a5001558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_a5001558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = a5001558_cfg_pcr

[DriverInstallx86_a5001558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_a5001558;, EventLogService

[DriverServicex86_a5001558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = a5001558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_a5001558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_a5001558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = a5001558_cfg_pcr

[DriverInstallx64_a5001558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_a5001558;, EventLogService

[DriverServicex64_a5001558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = a5001558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[a5001558_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[a5001558_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,00,fe,02,0f,02,0e,\
                                                      00,00,00,a8,04,00,04,00,00,00,02,34,ff,ff,10,01,00,00,02,36,ff,ff,10,01,00,00,03,f4,00,0f,00,0a,\
                                                      00,00,02,48,00,0f,00,0a,00,00,00,90,01,03,01,03


;cfg idx 139
[DriverInstallx86_a6001558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_a6001558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = a6001558_cfg_pcr

[DriverInstallx86_a6001558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_a6001558;, EventLogService

[DriverServicex86_a6001558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = a6001558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_a6001558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_a6001558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = a6001558_cfg_pcr

[DriverInstallx64_a6001558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_a6001558;, EventLogService

[DriverServicex64_a6001558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = a6001558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[a6001558_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[a6001558_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,00,fe,02,0f,02,0e,\
                                                      00,00,00,a8,04,00,04,00,00,00,02,34,ff,ff,10,01,00,00,02,36,ff,ff,10,01,00,00,03,f4,00,0f,00,0a,\
                                                      00,00,02,48,00,0f,00,0a,00,00,00,90,01,03,01,03


;cfg idx 140
[DriverInstallx86_40301558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_40301558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 40301558_cfg_pcr

[DriverInstallx86_40301558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_40301558;, EventLogService

[DriverServicex86_40301558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 40301558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_40301558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_40301558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 40301558_cfg_pcr

[DriverInstallx64_40301558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_40301558;, EventLogService

[DriverServicex64_40301558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 40301558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[40301558_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[40301558_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 141
[DriverInstallx86_14A11558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_14A11558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 14A11558_cfg_pcr

[DriverInstallx86_14A11558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_14A11558;, EventLogService

[DriverServicex86_14A11558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 14A11558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_14A11558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_14A11558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 14A11558_cfg_pcr

[DriverInstallx64_14A11558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_14A11558;, EventLogService

[DriverServicex64_14A11558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 14A11558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[14A11558_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[14A11558_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 142
[DriverInstallx86_384f17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_384f17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 384f17aa_cfg_pcr

[DriverInstallx86_384f17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_384f17aa;, EventLogService

[DriverServicex86_384f17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 384f17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_384f17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_384f17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 384f17aa_cfg_pcr

[DriverInstallx64_384f17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_384f17aa;, EventLogService

[DriverServicex64_384f17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 384f17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[384f17aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[384f17aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,00,fe,02,0f,02,0e,\
                                                      00,00,00,a8,04,00,04,00,00,00,02,34,ff,ff,10,01,00,00,02,36,ff,ff,10,01,00,00,03,f4,00,0f,00,0a,\
                                                      00,00,02,48,00,0f,00,0a,00,00,00,90,01,03,01,03


;cfg idx 143
[DriverInstallx86_e2071071.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_e2071071.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = e2071071_cfg_pcr

[DriverInstallx86_e2071071.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_e2071071;, EventLogService

[DriverServicex86_e2071071]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = e2071071_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_e2071071.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_e2071071.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = e2071071_cfg_pcr

[DriverInstallx64_e2071071.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_e2071071;, EventLogService

[DriverServicex64_e2071071]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = e2071071_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[e2071071_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[e2071071_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 144
[DriverInstallx86_a1211071.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_a1211071.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = a1211071_cfg_pcr

[DriverInstallx86_a1211071.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_a1211071;, EventLogService

[DriverServicex86_a1211071]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = a1211071_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_a1211071.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_a1211071.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = a1211071_cfg_pcr

[DriverInstallx64_a1211071.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_a1211071;, EventLogService

[DriverServicex64_a1211071]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = a1211071_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[a1211071_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[a1211071_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 145
[DriverInstallx86_40151071.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_40151071.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 40151071_cfg_pcr

[DriverInstallx86_40151071.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_40151071;, EventLogService

[DriverServicex86_40151071]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 40151071_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_40151071.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_40151071.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 40151071_cfg_pcr

[DriverInstallx64_40151071.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_40151071;, EventLogService

[DriverServicex64_40151071]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 40151071_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[40151071_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[40151071_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 146
[DriverInstallx86_a2521071.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_a2521071.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = a2521071_cfg_pcr

[DriverInstallx86_a2521071.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_a2521071;, EventLogService

[DriverServicex86_a2521071]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = a2521071_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_a2521071.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_a2521071.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = a2521071_cfg_pcr

[DriverInstallx64_a2521071.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_a2521071;, EventLogService

[DriverServicex64_a2521071]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = a2521071_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[a2521071_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[a2521071_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 147
[DriverInstallx86_b3601071.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_b3601071.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = b3601071_cfg_pcr

[DriverInstallx86_b3601071.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_b3601071;, EventLogService

[DriverServicex86_b3601071]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = b3601071_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_b3601071.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_b3601071.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = b3601071_cfg_pcr

[DriverInstallx64_b3601071.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_b3601071;, EventLogService

[DriverServicex64_b3601071]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = b3601071_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[b3601071_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[b3601071_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 148
[DriverInstallx86_e2051071.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_e2051071.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = e2051071_cfg_pcr

[DriverInstallx86_e2051071.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_e2051071;, EventLogService

[DriverServicex86_e2051071]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = e2051071_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_e2051071.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_e2051071.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = e2051071_cfg_pcr

[DriverInstallx64_e2051071.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_e2051071;, EventLogService

[DriverServicex64_e2051071]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = e2051071_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[e2051071_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[e2051071_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 149
[DriverInstallx86_a1201071.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_a1201071.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = a1201071_cfg_pcr

[DriverInstallx86_a1201071.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_a1201071;, EventLogService

[DriverServicex86_a1201071]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = a1201071_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_a1201071.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_a1201071.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = a1201071_cfg_pcr

[DriverInstallx64_a1201071.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_a1201071;, EventLogService

[DriverServicex64_a1201071]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = a1201071_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[a1201071_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[a1201071_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 150
[DriverInstallx86_d3001071.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_d3001071.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = d3001071_cfg_pcr

[DriverInstallx86_d3001071.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_d3001071;, EventLogService

[DriverServicex86_d3001071]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = d3001071_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_d3001071.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_d3001071.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = d3001071_cfg_pcr

[DriverInstallx64_d3001071.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_d3001071;, EventLogService

[DriverServicex64_d3001071]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = d3001071_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[d3001071_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[d3001071_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 151
[DriverInstallx86_d3011071.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_d3011071.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = d3011071_cfg_pcr

[DriverInstallx86_d3011071.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_d3011071;, EventLogService

[DriverServicex86_d3011071]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = d3011071_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_d3011071.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_d3011071.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = d3011071_cfg_pcr

[DriverInstallx64_d3011071.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_d3011071;, EventLogService

[DriverServicex64_d3011071]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = d3011071_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[d3011071_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[d3011071_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 152
[DriverInstallx86_a1901071.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_a1901071.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = a1901071_cfg_pcr

[DriverInstallx86_a1901071.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_a1901071;, EventLogService

[DriverServicex86_a1901071]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = a1901071_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_a1901071.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_a1901071.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = a1901071_cfg_pcr

[DriverInstallx64_a1901071.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_a1901071;, EventLogService

[DriverServicex64_a1901071]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = a1901071_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[a1901071_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[a1901071_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 153
[DriverInstallx86_a1911071.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_a1911071.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = a1911071_cfg_pcr

[DriverInstallx86_a1911071.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_a1911071;, EventLogService

[DriverServicex86_a1911071]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = a1911071_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_a1911071.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_a1911071.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = a1911071_cfg_pcr

[DriverInstallx64_a1911071.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_a1911071;, EventLogService

[DriverServicex64_a1911071]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = a1911071_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[a1911071_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[a1911071_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 154
[DriverInstallx86_96001558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_96001558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 96001558_cfg_pcr

[DriverInstallx86_96001558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_96001558;, EventLogService

[DriverServicex86_96001558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 96001558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_96001558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_96001558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 96001558_cfg_pcr

[DriverInstallx64_96001558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_96001558;, EventLogService

[DriverServicex64_96001558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 96001558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[96001558_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[96001558_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 155
[DriverInstallx86_86861558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_86861558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 86861558_cfg_pcr

[DriverInstallx86_86861558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_86861558;, EventLogService

[DriverServicex86_86861558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 86861558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_86861558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_86861558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 86861558_cfg_pcr

[DriverInstallx64_86861558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_86861558;, EventLogService

[DriverServicex64_86861558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 86861558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[86861558_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[86861558_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 156
[DriverInstallx86_385417aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_385417aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 385417aa_cfg_pcr

[DriverInstallx86_385417aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_385417aa;, EventLogService

[DriverServicex86_385417aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 385417aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_385417aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_385417aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 385417aa_cfg_pcr

[DriverInstallx64_385417aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_385417aa;, EventLogService

[DriverServicex64_385417aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 385417aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[385417aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[385417aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,00,fe,02,0f,02,0e,\
                                                      00,00,00,a8,04,00,04,00,00,00,02,34,ff,ff,10,01,00,00,02,36,ff,ff,10,01,00,00,03,f4,00,0f,00,0a,\
                                                      00,00,02,48,00,0f,00,0a,00,00,00,90,01,03,01,03,00,00,00,e2,f0,00,30,00,00,00,03,0a,00,c0,00,c0


;cfg idx 157
[DriverInstallx86_385317aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_385317aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 385317aa_cfg_pcr

[DriverInstallx86_385317aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_385317aa;, EventLogService

[DriverServicex86_385317aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 385317aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_385317aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_385317aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 385317aa_cfg_pcr

[DriverInstallx64_385317aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_385317aa;, EventLogService

[DriverServicex64_385317aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 385317aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[385317aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[385317aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,00,fe,02,0f,02,0e,\
                                                      00,00,00,a8,04,00,04,00,00,00,02,34,ff,ff,10,01,00,00,02,36,ff,ff,10,01,00,00,03,f4,00,0f,00,0a,\
                                                      00,00,02,48,00,0f,00,0a,00,00,00,90,01,03,01,03,00,00,00,e2,f0,00,30,00,00,00,03,0a,00,c0,00,c0


;cfg idx 158
[DriverInstallx86_385517aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_385517aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 385517aa_cfg_pcr

[DriverInstallx86_385517aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_385517aa;, EventLogService

[DriverServicex86_385517aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 385517aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_385517aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_385517aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 385517aa_cfg_pcr

[DriverInstallx64_385517aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_385517aa;, EventLogService

[DriverServicex64_385517aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 385517aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[385517aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[385517aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 159
[DriverInstallx86_40501558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_40501558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 40501558_cfg_pcr

[DriverInstallx86_40501558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_40501558;, EventLogService

[DriverServicex86_40501558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 40501558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_40501558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_40501558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 40501558_cfg_pcr

[DriverInstallx64_40501558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_40501558;, EventLogService

[DriverServicex64_40501558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 40501558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[40501558_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[40501558_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 160
[DriverInstallx86_86821558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_86821558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 86821558_cfg_pcr

[DriverInstallx86_86821558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_86821558;, EventLogService

[DriverServicex86_86821558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 86821558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_86821558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_86821558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 86821558_cfg_pcr

[DriverInstallx64_86821558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_86821558;, EventLogService

[DriverServicex64_86821558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 86821558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[86821558_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[86821558_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 161
[DriverInstallx86_86831558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_86831558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 86831558_cfg_pcr

[DriverInstallx86_86831558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_86831558;, EventLogService

[DriverServicex86_86831558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 86831558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_86831558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_86831558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 86831558_cfg_pcr

[DriverInstallx64_86831558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_86831558;, EventLogService

[DriverServicex64_86831558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 86831558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[86831558_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[86831558_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 162
[DriverInstallx86_40181558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_40181558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 40181558_cfg_pcr

[DriverInstallx86_40181558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_40181558;, EventLogService

[DriverServicex86_40181558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 40181558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_40181558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_40181558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 40181558_cfg_pcr

[DriverInstallx64_40181558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_40181558;, EventLogService

[DriverServicex64_40181558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 40181558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[40181558_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[40181558_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 163
[DriverInstallx86_31141DC2.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_31141DC2.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 31141DC2_cfg_pcr

[DriverInstallx86_31141DC2.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_31141DC2;, EventLogService

[DriverServicex86_31141DC2]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 31141DC2_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_31141DC2.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_31141DC2.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 31141DC2_cfg_pcr

[DriverInstallx64_31141DC2.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_31141DC2;, EventLogService

[DriverServicex64_31141DC2]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 31141DC2_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[31141DC2_cfg]
HKR,"seaeagle", "driver_item", 0x00010001, 0x8000001a
HKR,"seaeagle", "PSD_MODE", 0x00010001, 0x80040a0a

[31141DC2_cfg_pcr]
HKR,"seaeagle\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,44,00,00,03,04,77,7e,22,58,00,00,03,0a,00,c0,00,c0


;cfg idx 164
[DriverInstallx86_C195144D.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_C195144D.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = C195144D_cfg_pcr

[DriverInstallx86_C195144D.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_C195144D;, EventLogService

[DriverServicex86_C195144D]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = C195144D_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_C195144D.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_C195144D.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = C195144D_cfg_pcr

[DriverInstallx64_C195144D.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_C195144D;, EventLogService

[DriverServicex64_C195144D]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = C195144D_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[C195144D_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[C195144D_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 165
[DriverInstallx86_001C1E26.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_001C1E26.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 001C1E26_cfg_pcr

[DriverInstallx86_001C1E26.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_001C1E26;, EventLogService

[DriverServicex86_001C1E26]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 001C1E26_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_001C1E26.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_001C1E26.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 001C1E26_cfg_pcr

[DriverInstallx64_001C1E26.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_001C1E26;, EventLogService

[DriverServicex64_001C1E26]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 001C1E26_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[001C1E26_cfg]
HKR,"seaeagle", "driver_item", 0x00010001, 0x8000001a
HKR,"seaeagle", "PSD_MODE", 0x00010001, 0x80040a0a

[001C1E26_cfg_pcr]
HKR,"seaeagle\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,44,00,00,03,04,77,7e,22,58,00,00,03,0a,00,c0,00,c0


;cfg idx 166
[DriverInstallx86_202F1043.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_202F1043.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 202F1043_cfg_pcr

[DriverInstallx86_202F1043.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_202F1043;, EventLogService

[DriverServicex86_202F1043]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 202F1043_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_202F1043.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_202F1043.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 202F1043_cfg_pcr

[DriverInstallx64_202F1043.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_202F1043;, EventLogService

[DriverServicex64_202F1043]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 202F1043_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[202F1043_cfg]
HKR,"seaeagle", "driver_item", 0x00010001, 0x8000001a
HKR,"seaeagle", "PSD_MODE", 0x00010001, 0x80040a0a

[202F1043_cfg_pcr]
HKR,"seaeagle\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,44,00,00,03,04,77,7e,22,58,00,00,03,0a,00,c0,00,c0,\
                                                         00,00,00,a8,04,00,04,00,00,00,02,34,ff,ff,10,01,00,00,02,36,ff,ff,10,01,\
                                                         00,00,03,f4,00,0f,00,0a,00,00,02,48,00,0f,00,0a,00,00,00,90,01,03,01,02,\
                                                         00,00,00,fe,00,0f,00,0e


;cfg idx 167
[DriverInstallx86_50ac17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_50ac17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 50ac17aa_cfg_pcr

[DriverInstallx86_50ac17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_50ac17aa;, EventLogService

[DriverServicex86_50ac17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 50ac17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_50ac17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_50ac17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 50ac17aa_cfg_pcr

[DriverInstallx64_50ac17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_50ac17aa;, EventLogService

[DriverServicex64_50ac17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 50ac17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[50ac17aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[50ac17aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 168
[DriverInstallx86_50ad17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_50ad17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 50ad17aa_cfg_pcr

[DriverInstallx86_50ad17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_50ad17aa;, EventLogService

[DriverServicex86_50ad17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 50ad17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_50ad17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_50ad17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 50ad17aa_cfg_pcr

[DriverInstallx64_50ad17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_50ad17aa;, EventLogService

[DriverServicex64_50ad17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 50ad17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[50ad17aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[50ad17aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 169
[DriverInstallx86_30051a58.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_30051a58.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 30051a58_cfg_pcr

[DriverInstallx86_30051a58.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_30051a58;, EventLogService

[DriverServicex86_30051a58]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 30051a58_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_30051a58.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_30051a58.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 30051a58_cfg_pcr

[DriverInstallx64_30051a58.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_30051a58;, EventLogService

[DriverServicex64_30051a58]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 30051a58_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[30051a58_cfg]
HKR,"seaeagle", "driver_item", 0x00010001, 0x8000001a
HKR,"seaeagle", "PSD_MODE", 0x00010001, 0x80040a0a

[30051a58_cfg_pcr]
HKR,"seaeagle\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,44,00,00,03,04,77,7e,22,58,00,00,03,0a,00,c0,00,c0


;cfg idx 170
[DriverInstallx86_201b1a58.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_201b1a58.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 201b1a58_cfg_pcr

[DriverInstallx86_201b1a58.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_201b1a58;, EventLogService

[DriverServicex86_201b1a58]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 201b1a58_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_201b1a58.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_201b1a58.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 201b1a58_cfg_pcr

[DriverInstallx64_201b1a58.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_201b1a58;, EventLogService

[DriverServicex64_201b1a58]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 201b1a58_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[201b1a58_cfg]
HKR,"seaeagle", "driver_item", 0x00010001, 0x8000001a
HKR,"seaeagle", "PSD_MODE", 0x00010001, 0x80040a0a

[201b1a58_cfg_pcr]
HKR,"seaeagle\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,44,00,00,03,04,77,7e,22,58,00,00,03,0a,00,c0,00,c0


;cfg idx 171
[DriverInstallx86_100b1a58.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_100b1a58.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 100b1a58_cfg_pcr

[DriverInstallx86_100b1a58.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_100b1a58;, EventLogService

[DriverServicex86_100b1a58]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 100b1a58_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_100b1a58.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_100b1a58.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 100b1a58_cfg_pcr

[DriverInstallx64_100b1a58.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_100b1a58;, EventLogService

[DriverServicex64_100b1a58]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 100b1a58_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[100b1a58_cfg]
HKR,"seaeagle", "driver_item", 0x00010001, 0x8000001a
HKR,"seaeagle", "PSD_MODE", 0x00010001, 0x80040a0a

[100b1a58_cfg_pcr]
HKR,"seaeagle\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,44,00,00,03,04,77,7e,22,58,00,00,03,0a,00,c0,00,c0


;cfg idx 172
[DriverInstallx86_c1a7144d.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_c1a7144d.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = c1a7144d_cfg_pcr

[DriverInstallx86_c1a7144d.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_c1a7144d;, EventLogService

[DriverServicex86_c1a7144d]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = c1a7144d_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_c1a7144d.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_c1a7144d.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = c1a7144d_cfg_pcr

[DriverInstallx64_c1a7144d.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_c1a7144d;, EventLogService

[DriverServicex64_c1a7144d]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = c1a7144d_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[c1a7144d_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[c1a7144d_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 173
[DriverInstallx86_386117aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_386117aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 386117aa_cfg_pcr

[DriverInstallx86_386117aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_386117aa;, EventLogService

[DriverServicex86_386117aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 386117aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_386117aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_386117aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 386117aa_cfg_pcr

[DriverInstallx64_386117aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_386117aa;, EventLogService

[DriverServicex64_386117aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 386117aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[386117aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[386117aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0,00,00,00,e2,f0,00,30,00,00,00,00,fe,00,0f,00,08,00,00,03,e6,00,08,00,08


;cfg idx 174
[DriverInstallx86_387017aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_387017aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 387017aa_cfg_pcr

[DriverInstallx86_387017aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_387017aa;, EventLogService

[DriverServicex86_387017aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 387017aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_387017aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_387017aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 387017aa_cfg_pcr

[DriverInstallx64_387017aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_387017aa;, EventLogService

[DriverServicex64_387017aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 387017aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[387017aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[387017aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0


;cfg idx 175
[DriverInstallx86_386F17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_386F17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 386F17aa_cfg_pcr

[DriverInstallx86_386F17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_386F17aa;, EventLogService

[DriverServicex86_386F17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 386F17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_386F17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_386F17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 386F17aa_cfg_pcr

[DriverInstallx64_386F17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_386F17aa;, EventLogService

[DriverServicex64_386F17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 386F17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[386F17aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[386F17aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0


;cfg idx 176
[DriverInstallx86_386617aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_386617aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 386617aa_cfg_pcr

[DriverInstallx86_386617aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_386617aa;, EventLogService

[DriverServicex86_386617aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 386617aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_386617aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_386617aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 386617aa_cfg_pcr

[DriverInstallx64_386617aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_386617aa;, EventLogService

[DriverServicex64_386617aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 386617aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[386617aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[386617aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0


;cfg idx 177
[DriverInstallx86_387217aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_387217aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 387217aa_cfg_pcr

[DriverInstallx86_387217aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_387217aa;, EventLogService

[DriverServicex86_387217aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 387217aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_387217aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_387217aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 387217aa_cfg_pcr

[DriverInstallx64_387217aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_387217aa;, EventLogService

[DriverServicex64_387217aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 387217aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[387217aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[387217aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0


;cfg idx 178
[DriverInstallx86_386217aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_386217aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 386217aa_cfg_pcr

[DriverInstallx86_386217aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_386217aa;, EventLogService

[DriverServicex86_386217aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 386217aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_386217aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_386217aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 386217aa_cfg_pcr

[DriverInstallx64_386217aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_386217aa;, EventLogService

[DriverServicex64_386217aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 386217aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[386217aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[386217aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0


;cfg idx 179
[DriverInstallx86_386b17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_386b17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 386b17aa_cfg_pcr

[DriverInstallx86_386b17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_386b17aa;, EventLogService

[DriverServicex86_386b17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 386b17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_386b17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_386b17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 386b17aa_cfg_pcr

[DriverInstallx64_386b17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_386b17aa;, EventLogService

[DriverServicex64_386b17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 386b17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[386b17aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[386b17aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0


;cfg idx 180
[DriverInstallx86_866d1558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_866d1558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 866d1558_cfg_pcr

[DriverInstallx86_866d1558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_866d1558;, EventLogService

[DriverServicex86_866d1558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 866d1558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_866d1558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_866d1558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 866d1558_cfg_pcr

[DriverInstallx64_866d1558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_866d1558;, EventLogService

[DriverServicex64_866d1558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 866d1558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[866d1558_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[866d1558_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0


;cfg idx 181
[DriverInstallx86_51631558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_51631558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 51631558_cfg_pcr

[DriverInstallx86_51631558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_51631558;, EventLogService

[DriverServicex86_51631558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 51631558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_51631558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_51631558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 51631558_cfg_pcr

[DriverInstallx64_51631558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_51631558;, EventLogService

[DriverServicex64_51631558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 51631558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[51631558_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[51631558_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0


;cfg idx 182
[DriverInstallx86_386417aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_386417aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 386417aa_cfg_pcr

[DriverInstallx86_386417aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_386417aa;, EventLogService

[DriverServicex86_386417aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 386417aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_386417aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_386417aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 386417aa_cfg_pcr

[DriverInstallx64_386417aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_386417aa;, EventLogService

[DriverServicex64_386417aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 386417aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[386417aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[386417aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0


;cfg idx 183
[DriverInstallx86_387117aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_387117aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 387117aa_cfg_pcr

[DriverInstallx86_387117aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_387117aa;, EventLogService

[DriverServicex86_387117aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 387117aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_387117aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_387117aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 387117aa_cfg_pcr

[DriverInstallx64_387117aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_387117aa;, EventLogService

[DriverServicex64_387117aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 387117aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[387117aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[387117aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0


;cfg idx 184
[DriverInstallx86_389b17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_389b17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 389b17aa_cfg_pcr

[DriverInstallx86_389b17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_389b17aa;, EventLogService

[DriverServicex86_389b17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 389b17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_389b17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_389b17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 389b17aa_cfg_pcr

[DriverInstallx64_389b17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_389b17aa;, EventLogService

[DriverServicex64_389b17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 389b17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[389b17aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[389b17aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0


;cfg idx 185
[DriverInstallx86_866c1558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_866c1558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 866c1558_cfg_pcr

[DriverInstallx86_866c1558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_866c1558;, EventLogService

[DriverServicex86_866c1558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 866c1558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_866c1558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_866c1558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 866c1558_cfg_pcr

[DriverInstallx64_866c1558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_866c1558;, EventLogService

[DriverServicex64_866c1558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 866c1558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[866c1558_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[866c1558_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0


;cfg idx 186
[DriverInstallx86_50a31558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_50a31558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 50a31558_cfg_pcr

[DriverInstallx86_50a31558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_50a31558;, EventLogService

[DriverServicex86_50a31558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 50a31558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_50a31558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_50a31558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 50a31558_cfg_pcr

[DriverInstallx64_50a31558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_50a31558;, EventLogService

[DriverServicex64_50a31558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 50a31558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[50a31558_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[50a31558_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0


;cfg idx 187
[DriverInstallx86_77161558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_77161558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 77161558_cfg_pcr

[DriverInstallx86_77161558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_77161558;, EventLogService

[DriverServicex86_77161558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 77161558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_77161558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_77161558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 77161558_cfg_pcr

[DriverInstallx64_77161558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_77161558;, EventLogService

[DriverServicex64_77161558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 77161558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[77161558_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[77161558_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0


;cfg idx 188
[DriverInstallx86_77171558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_77171558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 77171558_cfg_pcr

[DriverInstallx86_77171558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_77171558;, EventLogService

[DriverServicex86_77171558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 77171558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_77171558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_77171558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 77171558_cfg_pcr

[DriverInstallx64_77171558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_77171558;, EventLogService

[DriverServicex64_77171558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 77171558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[77171558_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[77171558_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0


;cfg idx 189
[DriverInstallx86_65f51558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_65f51558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 65f51558_cfg_pcr

[DriverInstallx86_65f51558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_65f51558;, EventLogService

[DriverServicex86_65f51558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 65f51558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_65f51558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_65f51558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 65f51558_cfg_pcr

[DriverInstallx64_65f51558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_65f51558;, EventLogService

[DriverServicex64_65f51558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 65f51558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[65f51558_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[65f51558_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0


;cfg idx 190
[DriverInstallx86_387417aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_387417aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 387417aa_cfg_pcr

[DriverInstallx86_387417aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_387417aa;, EventLogService

[DriverServicex86_387417aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 387417aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_387417aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_387417aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 387417aa_cfg_pcr

[DriverInstallx64_387417aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_387417aa;, EventLogService

[DriverServicex64_387417aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 387417aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[387417aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[387417aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0


;cfg idx 191
[DriverInstallx86_387517aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_387517aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 387517aa_cfg_pcr

[DriverInstallx86_387517aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_387517aa;, EventLogService

[DriverServicex86_387517aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 387517aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[DriverInstallx64_387517aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_387517aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 387517aa_cfg_pcr

[DriverInstallx64_387517aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_387517aa;, EventLogService

[DriverServicex64_387517aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 387517aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg_MS

[387517aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[387517aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0


;cfg idx 192
[DriverInstallx86_387717aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_387717aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 387717aa_cfg_pcr

[DriverInstallx86_387717aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_387717aa;, EventLogService

[DriverServicex86_387717aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 387717aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_387717aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_387717aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 387717aa_cfg_pcr

[DriverInstallx64_387717aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_387717aa;, EventLogService

[DriverServicex64_387717aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 387717aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[387717aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[387717aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0


;cfg idx 193
[DriverInstallx86_202F1043_8621.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_202F1043_8621.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 202F1043_8621_cfg_pcr

[DriverInstallx86_202F1043_8621.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_202F1043_8621;, EventLogService

[DriverServicex86_202F1043_8621]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 202F1043_8621_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_202F1043_8621.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_202F1043_8621.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 202F1043_8621_cfg_pcr

[DriverInstallx64_202F1043_8621.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_202F1043_8621;, EventLogService

[DriverServicex64_202F1043_8621]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 202F1043_8621_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[202F1043_8621_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[202F1043_8621_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0


;cfg idx 194
[DriverInstallx86_77181558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_77181558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 77181558_cfg_pcr

[DriverInstallx86_77181558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_77181558;, EventLogService

[DriverServicex86_77181558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 77181558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_77181558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_77181558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 77181558_cfg_pcr

[DriverInstallx64_77181558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_77181558;, EventLogService

[DriverServicex64_77181558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 77181558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[77181558_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[77181558_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0


;cfg idx 195
[DriverInstallx86_c1ad144d.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_c1ad144d.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = c1ad144d_cfg_pcr

[DriverInstallx86_c1ad144d.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_c1ad144d;, EventLogService

[DriverServicex86_c1ad144d]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = c1ad144d_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_c1ad144d.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_c1ad144d.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = c1ad144d_cfg_pcr

[DriverInstallx64_c1ad144d.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_c1ad144d;, EventLogService

[DriverServicex64_c1ad144d]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = c1ad144d_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[c1ad144d_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[c1ad144d_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0


;cfg idx 196
[DriverInstallx86_40b11558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_40b11558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 40b11558_cfg_pcr

[DriverInstallx86_40b11558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_40b11558;, EventLogService

[DriverServicex86_40b11558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 40b11558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_40b11558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_40b11558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 40b11558_cfg_pcr

[DriverInstallx64_40b11558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_40b11558;, EventLogService

[DriverServicex64_40b11558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 40b11558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[40b11558_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0

[40b11558_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0


;cfg idx 197
[DriverInstallx86_40401558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_40401558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 40401558_cfg_pcr

[DriverInstallx86_40401558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_40401558;, EventLogService

[DriverServicex86_40401558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 40401558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_40401558.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_40401558.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 40401558_cfg_pcr

[DriverInstallx64_40401558.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_40401558;, EventLogService

[DriverServicex64_40401558]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 40401558_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[40401558_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000

[40401558_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0


;cfg idx 198
[DriverInstallx86_387d17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_387d17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 387d17aa_cfg_pcr

[DriverInstallx86_387d17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_387d17aa;, EventLogService

[DriverServicex86_387d17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 387d17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_387d17aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_387d17aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 387d17aa_cfg_pcr

[DriverInstallx64_387d17aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_387d17aa;, EventLogService

[DriverServicex64_387d17aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 387d17aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[387d17aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000

[387d17aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0


;cfg idx 199
[DriverInstallx86_00013100.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_00013100.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 00013100_cfg_pcr

[DriverInstallx86_00013100.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_00013100;, EventLogService

[DriverServicex86_00013100]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 00013100_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_00013100.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_00013100.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 00013100_cfg_pcr

[DriverInstallx64_00013100.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_00013100;, EventLogService

[DriverServicex64_00013100]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 00013100_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[00013100_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000

[00013100_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0


;cfg idx 200
[DriverInstallx86_388317aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon

[DriverInstallx86_388317aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
AddReg         = 388317aa_cfg_pcr

[DriverInstallx86_388317aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex86_388317aa;, EventLogService

[DriverServicex86_388317aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 388317aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[DriverInstallx64_388317aa.NT]
CopyFiles = @bhtsddr.sys
CopyFiles = Copybhtv5Icon,Copybhtv5Icon_WoW64

[DriverInstallx64_388317aa.NT.HW]
;Support Runtime D3 in Win8
Include = machine.inf
;Needs = PciD3ColdSupported.HW
;Add MSI support
AddReg = InterruptMgmtValues
DelReg         = cfg_DelReg
AddReg         = 388317aa_cfg_pcr

[DriverInstallx64_388317aa.NT.Services]
AddService = bhtsddr, 0x00000002 , DriverServicex64_388317aa;, EventLogService

[DriverServicex64_388317aa]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\bhtsddr.sys
DelReg         = cfg_DelDiskReg 
;AddReg         = pnpsafe_pci_addreg
DelReg         = cfg_DelReg
AddReg         = 388317aa_cfg
AddReg         = bus_type
AddReg         = autorun_addreg

[388317aa_cfg]
HKR,"seabird", "driver_item", 0x00010001, 0x8000001a
HKR,"seabird", "SD_CARD_MODE_DIS", 0x00010001, 0x80000001
HKR,"seabird", "PSD_MODE", 0x00010001, 0x80040a14 
HKR,"seabird", "MS_SDIO_CTRL", 0x00010001, 0x0
HKR,"seabird", "AUTO_POWEROFF_TIME", 0x00010001, 0x00000000

[388317aa_cfg_pcr]
HKR,"seabird\pcr", "pcr_value", 1, 00,00,03,00,f0,ff,60,55,00,00,03,04,77,7e,22,4a,00,00,03,0a,00,c0,00,c0

;Common cfg
[Copybhtv5Icon]
bhtv5Icon.dll

[Copybhtv5Icon_WoW64]
bhtv5Icon.dll

[InterruptMgmtValues]
HKR, "Interrupt Management",0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties",0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties",MSISupported,0x00010001,1

[EventLogService]
AddReg = EventLogService_AddReg

[EventLogService_AddReg]
HKR,,EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\IoLogMsg.dll"
HKR,,TypesSupported,   0x00010001, 7

[pnpsafe_pci_addreg]
HKR, "Parameters\PnpInterface", "5", 0x00010001, 0x00000001

[bus_type]
HKR,"Parameters", "BusType", 0x00010001, 0x0000000C

[cfg_DelReg]
HKR,"seaeagle"
HKR,"seabird"

[cfg_DelDiskReg]
HKLM,"System\CurrentControlSet\Services\disk","AutoRunAlwaysDisable"

[default_cfg_se]
HKR,"seaeagle", "psd_mode", 0x00010001, 0x80000000

[default_cfg_sb]
HKR,"seabird", "psd_mode", 0x00010001, 0x80000000

[autorun_addreg] 
;HKLM,"System\CurrentControlSet\Services\disk","AutoRunAlwaysDisable", 0x00010008,"SDHC"
;HKLM,"System\CurrentControlSet\Services\disk","AutoRunAlwaysDisable", 0x00010008,"SDXC"
;HKLM,"System\CurrentControlSet\Services\disk","AutoRunAlwaysDisable", 0x00010008,"SD"
;HKLM,"System\CurrentControlSet\Services\disk","AutoRunAlwaysDisable", 0x00010008,"MMC"
HKLM,"System\CurrentControlSet\Services\disk","AutoRunAlwaysDisable", 0x00010000,"Brother RemovableDisk(U)"

[autorun_addreg_MS] 
;Support ModernStandby
;HKLM,"System\CurrentControlSet\Services\disk","AutoRunAlwaysDisable", 0x00010008,"SDHC"
;HKLM,"System\CurrentControlSet\Services\disk","AutoRunAlwaysDisable", 0x00010008,"SDXC"
;HKLM,"System\CurrentControlSet\Services\disk","AutoRunAlwaysDisable", 0x00010008,"SD"
;HKLM,"System\CurrentControlSet\Services\disk","AutoRunAlwaysDisable", 0x00010008,"MMC"
HKLM,"System\CurrentControlSet\Services\disk","AutoRunAlwaysDisable", 0x00010000,"Brother RemovableDisk(U)"

[Strings]
REG_SZ        = 0x00000000
REG_MULTI_SZ  = 0x00010000
REG_EXPAND_SZ = 0x00020000
REG_BINARY    = 0x00000001
REG_DWORD     = 0x00010001
SERVICEROOT   = "System\CurrentControlSet\Services"

BayHubTech          = "BayHubTech"
bhtsddr.DeviceDesc = "BayHubTech Integrated MMC/SD controller"
bhtsddr.DriverDisk = "BayHubTech Integrated MMC/SD controller Driver Disk"
bhtsddr.DeviceDesc_SD = "BayHubTech SD Host controller"
bhtsddr.Generic_DeviceDesc = "BayHubTech Integrated MMC/SD controller(Generic)"