; nas192wm.inf
; Setup information file for NEC AS192WM Monitor
;
; Copyright 2012, NEC Display Solutions, Ltd.
;-------------------------------------------------
[Version]
signature="$CHICAGO$"
Class=Monitor
ClassGuid={4D36E96E-E325-11CE-BFC1-08002BE10318}
Provider=%NECDS%
CatalogFile=nas192wm.cat
DriverVer=08/21/2012,1.12.0821.1026

[ControlFlags]
ExcludeFromSelect.nt=Monitor\NEC68DA

[DestinationDirs]
DefaultDestDir=11
AS192WM.CopyFiles=23

[SourceDisksNames]
1=%Disk1%,,,

[SourceDisksFiles]
nas192wm.icm=1

[Monitor_Service.Install]
DisplayName    = %Monitor.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START
ErrorControl   = 1               ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\monitor.sys

[Manufacturer]
%NECDS%=NECDS,ntamd64

[NECDS]
%AS192WM%=AS192WM.Install, Monitor\NEC68DA

[NECDS.ntamd64]
%AS192WM%=AS192WM.Install.ntamd64, Monitor\NEC68DA

[AS192WM.Install]
DelReg=DEL_CURRENT_REG
AddReg=AS192WM.AddReg, 1440, DPMS
CopyFiles=AS192WM.CopyFiles

[AS192WM.Install.ntamd64]
DelReg=DEL_CURRENT_REG
AddReg=AS192WM.AddReg, 1440, DPMS
CopyFiles=AS192WM.CopyFiles

[AS192WM.Install.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install; install monitor class function driver

[AS192WM.Install.ntamd64.Services]
AddService = monitor, %SPSVCINST_ASSOCSERVICE%,Monitor_Service.Install; install monitor class function driver

[DEL_CURRENT_REG]
HKR,MODES
HKR,,MaxResolution
HKR,,DPMS
HKR,,ICMProfile

[1440]
HKR,,MaxResolution,,"1440,900"

[DPMS]
HKR,,DPMS,,1

[AS192WM.AddReg]
HKR,"MODES\1440,900",Mode1,,"31.0-85.0,56.0-76.0,-,+"
HKR,,ICMProfile,0,"nas192wm.icm"

[AS192WM.CopyFiles]
nas192wm.icm

[Strings]
NECDS="NEC"
Disk1="NEC Monitor Installation Disk"

SPSVCINST_ASSOCSERVICE = 0x00000002
Monitor.SVCDESC = "Microsoft Monitor Class Function Driver Service"

AS192WM="NEC AS192WM"
