; nl208uxp.inf
; Setup information file for NEC MultiSync LCD2080UX+ Monitor
;
; Copyright 2003, NEC-Mitsubishi Electronics Display, Inc.
;-------------------------------------------------
[Version]
signature="$CHICAGO$"
Class=Monitor
ClassGuid={4D36E96E-E325-11CE-BFC1-08002BE10318}
Provider=%NECDS%
CatalogFile=nl208uxp.cat
DriverVer=10/18/2005, 1.05.1018.1021

[ClassInstall32]
AddReg=ClassAddReg32

[ClassAddReg32]
HKR,,,,%MonitorClassName%
HKR,,Icon,,"-1"
HKR,,NoInstallClass,,1

[DestinationDirs]
LCD2080UXPlus.CopyFiles=23
DefaultDestDir=11

[SourceDisksNames]
1=%Disk1%,,,

[SourceDisksFiles]
nl208uxp.icm=1

[Manufacturer]
%NECDS%=NECDS,ntamd64

[NECDS]
%LCD2080UXPlus%=LCD2080UXPlus.Install, Monitor\NEC662B

[NECDS.ntamd64]
%LCD2080UXPlus%=LCD2080UXPlus.Install.ntamd64, Monitor\NEC662B

[LCD2080UXPlus.Install]
DelReg=DEL_CURRENT_REG
AddReg=LCD2080UXPlus.AddReg, 1600, DPMS
CopyFiles=LCD2080UXPlus.CopyFiles

[LCD2080UXPlus.Install.ntamd64]
DelReg=DEL_CURRENT_REG
AddReg=LCD2080UXPlus.AddReg, 1600, DPMS
CopyFiles=LCD2080UXPlus.CopyFiles

[DEL_CURRENT_REG]
HKR,MODES
HKR,,MaxResolution
HKR,,DPMS
HKR,,ICMProfile

[1600]
HKR,,MaxResolution,,"1600,1200"

[DPMS]
HKR,,DPMS,,1

[LCD2080UXPlus.AddReg]
HKR,"MODES\1600,1200",Mode1,,"30.0-96.0,48.0-87.0,+,+"
HKR,,ICMProfile,0,"nl208uxp.icm"

[LCD2080UXPlus.CopyFiles]
nl208uxp.icm

[Strings]
MonitorClassName="Monitor"
NECDS="NEC"
LCD2080UXPlus="NEC MultiSync LCD2080UX+"
Disk1="NEC Monitor Installation Disk"