;
; Android WinUsb driver installation.
;
[Version]
Signature           = "$Windows NT$"
Class               = AndroidUsbDeviceClass
ClassGuid           = {3F966BD9-FA04-4ec5-991C-D326973B5128}
Provider            = %ProviderName%
DriverVer           = 08/01/2013,7.0.0000.00001
CatalogFile.NTx86   = androidwinusb86.cat
CatalogFile.NTamd64 = androidwinusba64.cat

[ClassInstall32]
Addreg = AndroidWinUsbClassReg

[AndroidWinUsbClassReg]
HKR,,,0,%ClassName%
HKR,,Icon,,-1


[Manufacturer]
%ProviderName% = Google, NTx86, NTamd64


[Google.NTx86]
;;;;;;;;;;;;;;;;;;;;;;Lenovo USB history;;;;;;;;;;;;;;;;;;;;;;;;;;;; 
;MT65xx meta mode
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_0005
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_0005&MI_01
;Lenovo ADB Interface
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7437&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7498&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_749B&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_749D&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_74A4&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7437
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7437&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7498
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7498&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_749B
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_749B&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_2006&PID_0C03&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_05c6&PID_9025&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_2006&PID_0005
%CompositeAdbInterface%     = USB_Install, USB\VID_2006&PID_0005&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_D00D
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7495&MI_00
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_74EC&MI_00
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_74F6&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7509&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_750A&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_750D&MI_01
;;;;;;;;;;;;;;;;;;;;;;Lenovo USB history end;;;;;;;;;;;;;;;;;;;;;;;; 


;;;;;;;;;;;;;;;;;;;;;;Lenovo USB generic;;;;;;;;;;;;;;;;;;;;;;;;;;;; 
;generic mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7435&MI_01
;generic mass_storage,adb,acm
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_74ED&MI_01
;generic adb,diag,modem,nmea
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7501&MI_00
;generic adb,diag,modem,nmea,mass_storage
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7513&MI_00
;generic mtp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_74F8&MI_01
;generic ptp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_74F9&MI_01
;generic rndis,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7500&MI_02
;generic bicr,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_750E&MI_01
;generic mtp,adb,mass_storage
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_74EE&MI_01
;generic mtp,mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7718&MI_02
;;;;;;;;;;;;;;;;;;;;;;Lenovo USB generic end;;;;;;;;;;;;;;;;;;;;;;;;; 
      
;;;;;;;;;;;;;;;;;;;;;;Lenovo USB Project ;;;;;;;;;;;;;;;;;;;;;;;;;;;
; S6000L mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_75E0&MI_01
; S6000L ptp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_75E6&MI_01
; S6000L rndis,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_75EA&MI_02
; S6000L mtp,mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_75E4&MI_02
; S6000L bicr,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7629&MI_01
; S6000L mtp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_75E2&MI_01

; S5000 mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76E5&MI_01
; S5000 ptp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76EB&MI_01
; S5000 rndis,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76ED&MI_02
; S5000 mtp,mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76E9&MI_02
; S5000 bicr,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76EF&MI_01
; S5000 mtp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76E7&MI_01

; S960 mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7709&MI_01
; S960 ptp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_770D&MI_01
; S960 rndis,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_770F&MI_02
; S960 mtp,mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_770B&MI_02

; K910 adb,diag,modem,nmea,mass_storage
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7710&MI_00
; K910 ptp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7715&MI_01
; K910 rndis,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7717&MI_02
; K910 mtp,mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7713&MI_02

; BLADE8 mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76F1&MI_01
; BLADE8 mtp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76F3&MI_01
; BLADE8 mtp,mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76F5&MI_02
; BLADE8 ptp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76F7&MI_01
; BLADE8 rndis,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76F9&MI_02
; BLADE8 bicr,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76FB&MI_01

; BLADE10 mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76FD&MI_01
; BLADE10 mtp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76FF&MI_01
; BLADE10 mtp,mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7701&MI_02
; BLADE10 ptp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7703&MI_01
; BLADE10 rndis,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7705&MI_02
; BLADE10 bicr,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7707&MI_01
;;;;;;;;;;;;;;;;;;;;;;Lenovo USB Project end;;;;;;;;;;;;;;;;;;;;;;;;;;;

[Google.NTamd64]
;;;;;;;;;;;;;;;;;;;;;;Lenovo USB history;;;;;;;;;;;;;;;;;;;;;;;;;;;; 
;MT65xx meta mode
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_0005
%CompositeAdbInterface%     = USB_Install, USB\VID_0BB4&PID_0005&MI_01
;Lenovo ADB Interface
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7437&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7498&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_749B&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_749D&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_74A4&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7437
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7437&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7498
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7498&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_749B
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_749B&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_2006&PID_0C03&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_05c6&PID_9025&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_2006&PID_0005
%CompositeAdbInterface%     = USB_Install, USB\VID_2006&PID_0005&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_D00D
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7495&MI_00
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_74EC&MI_00
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_74F6&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7509&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_750A&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_750D&MI_01
;;;;;;;;;;;;;;;;;;;;;;Lenovo USB history end;;;;;;;;;;;;;;;;;;;;;;;; 


;;;;;;;;;;;;;;;;;;;;;;Lenovo USB generic;;;;;;;;;;;;;;;;;;;;;;;;;;;; 
;generic mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7435&MI_01
;generic mass_storage,adb,acm
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_74ED&MI_01
;generic adb,diag,modem,nmea
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7501&MI_00
;generic adb,diag,modem,nmea,mass_storage
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7513&MI_00
;generic mtp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_74F8&MI_01
;generic ptp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_74F9&MI_01
;generic rndis,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7500&MI_02
;generic bicr,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_750E&MI_01
;generic mtp,adb,mass_storage
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_74EE&MI_01
;generic mtp,mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7718&MI_02
;;;;;;;;;;;;;;;;;;;;;;Lenovo USB generic end;;;;;;;;;;;;;;;;;;;;;;;;; 
      
;;;;;;;;;;;;;;;;;;;;;;Lenovo USB Project ;;;;;;;;;;;;;;;;;;;;;;;;;;;
; S6000L mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_75E0&MI_01
; S6000L ptp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_75E6&MI_01
; S6000L rndis,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_75EA&MI_02
; S6000L mtp,mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_75E4&MI_02
; S6000L bicr,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7629&MI_01
; S6000L mtp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_75E2&MI_01

; S5000 mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76E5&MI_01
; S5000 ptp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76EB&MI_01
; S5000 rndis,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76ED&MI_02
; S5000 mtp,mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76E9&MI_02
; S5000 bicr,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76EF&MI_01
; S5000 mtp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76E7&MI_01

; S960 mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7709&MI_01
; S960 ptp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_770D&MI_01
; S960 rndis,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_770F&MI_02
; S960 mtp,mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_770B&MI_02

; K910 adb,diag,modem,nmea,mass_storage
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7710&MI_00
; K910 ptp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7715&MI_01
; K910 rndis,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7717&MI_02
; K910 mtp,mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7713&MI_02

; BLADE8 mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76F1&MI_01
; BLADE8 mtp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76F3&MI_01
; BLADE8 mtp,mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76F5&MI_02
; BLADE8 ptp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76F7&MI_01
; BLADE8 rndis,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76F9&MI_02
; BLADE8 bicr,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76FB&MI_01

; BLADE10 mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76FD&MI_01
; BLADE10 mtp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_76FF&MI_01
; BLADE10 mtp,mass_storage,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7701&MI_02
; BLADE10 ptp,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7703&MI_01
; BLADE10 rndis,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7705&MI_02
; BLADE10 bicr,adb
%CompositeAdbInterface%     = USB_Install, USB\VID_17EF&PID_7707&MI_01

;;;;;;;;;;;;;;;;;;;;;;Lenovo USB Project end;;;;;;;;;;;;;;;;;;;;;;;;;;;

[USB_Install]
Include = winusb.inf
Needs   = WINUSB.NT

[USB_Install.Services]
Include     = winusb.inf
AddService  = WinUSB,0x00000002,WinUSB_ServiceInstall

[WinUSB_ServiceInstall]
DisplayName     = %WinUSB_SvcDesc%
ServiceType     = 1
StartType       = 3
ErrorControl    = 1
ServiceBinary   = %12%\WinUSB.sys

[USB_Install.Wdf]
KmdfService = WINUSB, WinUSB_Install

[WinUSB_Install]
KmdfLibraryVersion  = 1.9

[USB_Install.HW]
AddReg  = Dev_AddReg

[Dev_AddReg]
HKR,,DeviceInterfaceGUIDs,0x10000,"{F72FE0D4-CBCB-407d-8814-9ED673D0DD6B}"

[USB_Install.CoInstallers]
AddReg    = CoInstallers_AddReg
CopyFiles = CoInstallers_CopyFiles

[CoInstallers_AddReg]
HKR,,CoInstallers32,0x00010000,"WdfCoInstaller01009.dll,WdfCoInstaller","WinUSBCoInstaller2.dll"

[CoInstallers_CopyFiles]
WinUSBCoInstaller2.dll
WdfCoInstaller01009.dll

[DestinationDirs]
CoInstallers_CopyFiles=11

[SourceDisksNames]
1 = %DISK_NAME%,,,\i386
2 = %DISK_NAME%,,,\amd64

[SourceDisksFiles.x86]
WinUSBCoInstaller2.dll  = 1
WdfCoInstaller01009.dll = 1

[SourceDisksFiles.amd64]
WinUSBCoInstaller2.dll  = 2
WdfCoInstaller01009.dll = 2

[Strings]
ProviderName                = "Lenovo Inc."
SingleAdbInterface          = "Lenovo ADB Interface"
CompositeAdbInterface       = "Lenovo Composite ADB Interface"
SingleBootLoaderInterface   = "Lenovo Bootloader Interface"
WinUSB_SvcDesc              = "Lenovo USB Driver"
DISK_NAME                   = "Lenovo WinUsb installation disk"
ClassName                   = "Lenovo ADB Device"