;
; Android WinUsb driver installation.
;
[Version]
Signature           = "$Windows NT$"
Class               = AndroidUsbDeviceClass
ClassGuid           = {3F966BD9-FA04-4ec5-991C-D326973B5128}
Provider            = %ProviderName%
DriverVer           = 11/17/2014,10.0.0000.00000
CatalogFile         = androidwinusb.cat

[ClassInstall32]
Addreg = AndroidWinUsbClassReg

[AndroidWinUsbClassReg]
HKR,,,0,%ClassName%
HKR,,Icon,,-1


[Manufacturer]
%ProviderName% = Google, NTx86, NTamd64


[Google.NTx86]

;Google Nexus One
%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_0D02
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_0D02&MI_01
%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_4E11
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4E12&MI_01

;Google Nexus S
%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_4E21
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4E22&MI_01
%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_4E23
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4E24&MI_01

;Google Nexus 7
%SingleBootLoaderInterface% = USB_Install, USB\VID_18D1&PID_4E40
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4E42&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4E44&MI_01

;Google Nexus Q
%SingleBootLoaderInterface% = USB_Install, USB\VID_18D1&PID_2C10
%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_2C11

;Google Nexus (generic)
%SingleBootLoaderInterface% = USB_Install, USB\VID_18D1&PID_4EE0
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4EE2&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4EE4&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4EE6&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4EE7

;Google Glass
%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_9001
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_9001&MI_01

;FUJITSU SP(GLF)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1560&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1561&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1562&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1563&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1564&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1565&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1566&MI_02

;FUJITSU SP(SLV)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1536&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1537&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1538&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1567&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1539&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_153A&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_153B&MI_02

;FUJITSU SP(SQM)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_154E&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_154F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1550&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1551&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1552&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1553&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1554&MI_02

;FUJITSU SP(LAM)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1547&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1548&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1549&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_154A&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_154B&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_154C&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_154D&MI_02

;FUJITSU SP(SQD)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1530&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1531&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1532&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1546&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1533&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1534&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1535&MI_02

;FUJITSU SP(LAT)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_152A&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_152B&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_152C&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1545&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_152D&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_152E&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_152F&MI_02

;FUJITSU SP(FJB)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1510&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1511&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1512&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1513&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1514&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1515&MI_02

;FUJITSU SP(TNM)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1505&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1506&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1507&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1508&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1509&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_150A&MI_02

;FUJITSU SP(CGM)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14FF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1500&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1501&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1502&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1503&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1504&MI_02

;FUJITSU SP(CGD)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14F9&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14FA&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14FB&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14FC&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14FD&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14FE&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1544&MI_02

;FUJITSU SP(DTM)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14F3&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14F4&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14F5&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14F6&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14F7&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14F8&MI_02

;FUJITSU SP(DTD)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14D4&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14D5&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14D6&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14D7&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14D8&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14D9&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1543&MI_02

;FUJITSU SP(RGB)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14CE&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14CF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14D0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14D1&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14D2&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14D3&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1542&MI_02

;FUJITSU SP(HDA)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14C7&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14C8&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14C9&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14CA&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14CB&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14CC&MI_02

;FUJITSU SP(BRMJ)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_149D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_149E&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_149F&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14A0&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14A1&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14A2&MI_02

;FUJITSU SP(BRM)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1497&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1498&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1499&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_149A&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_149B&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_149C&MI_02

;FUJITSU SP(BRG)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1491&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1492&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1493&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1494&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1495&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1496&MI_02

;FUJITSU SP(BAL)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_148B&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_148C&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_148D&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_148E&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_148F&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1490&MI_02

;FUJITSU SP(SHC)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1482&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1483&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1484&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1485&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1486&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1487&MI_02

;FUJITSU SP(VOL)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_147C&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_147D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_147E&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_147F&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1480&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1481&MI_02

;FUJITSU SP(ASA)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1457&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1458&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1459&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_145A&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_145B&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_145C&MI_02

;FUJITSU SP(SQU)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_144B&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_144C&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_144D&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_144E&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_144F&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1450&MI_02

;FUJITSU SP(ARG)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1429&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_142A&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_142B&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_142C&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_142D&MI_02

;FUJITSU SP(SPD)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1423&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1424&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1425&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1427&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1428&MI_02

;FUJITSU SP(KJK)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1414&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1415&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1416&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1417&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1418&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1444&MI_03

;FUJITSU SP(DRA)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1419&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_141A&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_141B&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_141D&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_141E&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1442&MI_03

;FUJITSU SP(KJD)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13FB&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13FC&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13FD&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13FE&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13E8&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1420&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1443&MI_03

;FUJITSU SP(HUD)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1403&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1404&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1405&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1406&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1407&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13EA&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1441&MI_03

;FUJITSU SP(CAS)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13FF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1400&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1401&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1402&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13E9&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1421&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1440&MI_03

;FUJITSU SP(LUG)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13F5&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13F6&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13F7&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13F9&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13E7&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_141F&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_143F&MI_03

;FUJITSU SP(HIM)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13D2&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13D3&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13D4&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13D6&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13D1&MI_02

;FUJITSU SP(CAN)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13BE&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13BF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13C0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13C2&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13C3&MI_02

;FUJITSU SP(TMS)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13DD&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13DE&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13DF&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13E0&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13E1&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13E2&MI_02

;FUJITSU SP(LPN)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13CB&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13CC&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13CD&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13CF&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13D0&MI_02

;FUJITSU SP(NAE)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_140E&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_140F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1410&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1411&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1412&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1413&MI_02

;FUJITSU SP(BRK)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_136E&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_136F&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1370&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1371&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1372&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1373&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1374&MI_02

;FUJITSU SP(NAS)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1384&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1385&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1386&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1388&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1389&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1387&MI_04

;FUJITSU SP(BOD)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1378&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1379&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_137A&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_137C&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_137E&MI_01

;FUJITSU SP(NAD)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_137F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1380&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1381&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1383&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1399&MI_01

;FUJITSU SP(IRU)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_138E&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_138F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1390&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1392&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1394&MI_01

;FUJITSU SP(IRUJW)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1395&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1396&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1397&MI_02

;FUJITSU SP(LY)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_139E&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_139F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13A0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13A2&MI_03

;FUJITSU SP(TA)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1314&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1315&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_131A&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_131B&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1340&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1340&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1341&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1341&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1317&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1318&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1352&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1353&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1111&MI_02

;FUJITSU SP(AR)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1321&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1322&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1325&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1326&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_133F&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1355&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_136D&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1331&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1332&MI_06
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1333&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_133E&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1324&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_133D&MI_01

;FUJITSU SP(AC)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1342&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1343&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1344&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1346&MI_04

;FUJITSU SP(QFAC)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1112&MI_01

;FUJITSU SP(NDS)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1356&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1357&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1358&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_135A&MI_04

;FUJITSU SP(BGB)
%CompositeAdbInterface%     = USB_Install, USB\VID_04c5&PID_12C8&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04c5&PID_12C9&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04c5&PID_12CA&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04c5&PID_12CB&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04c5&PID_12CC&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04c5&PID_12CD&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04c5&PID_12D8&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04c5&PID_12E4&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_04c5&PID_1337&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04c5&PID_1338&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04c5&PID_1367&MI_01

;FUJITSU SP(SW)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_135E&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_135F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1360&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1362&MI_03

;FUJITSU SP(SHD)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12B4&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12B5&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12E6&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1335&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1365&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1350&MI_01

;FUJITSU SP(ELL)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_131D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_131E&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_131F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_139B&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_139C&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_139D&MI_01

;FUJITSU SP(TRI)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12EF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12F0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12F2&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1336&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1351&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1366&MI_01

;FUJITSU SP(APOK)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12F9&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12FA&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12FB&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12FB&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12FC&MI_06
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12FD&MI_01

;FUJITSU SP(APOD)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12F3&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12F4&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12F5&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_135C&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_135D&MI_01

;FUJITSU SP(SKY)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12E8&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12E9&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12EA&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12EA&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12EB&MI_07
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12EC&MI_01

;FUJITSU SP(BAC)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12B0&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12AF&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12C5&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12C6&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1334&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1364&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_134F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_131C&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13AF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13B0&MI_01

;FUJITSU SP(EIF)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12AB&MI_01

;TOSHIBA T-01C
%CompositeAdbInterface%     = USB_Install, USB\VID_0930&PID_0D85&MI_01
;
;TOSHIBA IS04
%CompositeAdbInterface%     = USB_Install, USB\VID_0930&PID_0D8D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0930&PID_0D8C&MI_01


[Google.NTamd64]

;Google Nexus One
%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_0D02
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_0D02&MI_01
%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_4E11
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4E12&MI_01

;Google Nexus S
%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_4E21
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4E22&MI_01
%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_4E23
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4E24&MI_01

;Google Nexus 7
%SingleBootLoaderInterface% = USB_Install, USB\VID_18D1&PID_4E40
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4E42&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4E44&MI_01

;Google Nexus Q
%SingleBootLoaderInterface% = USB_Install, USB\VID_18D1&PID_2C10
%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_2C11

;Google Nexus (generic)
%SingleBootLoaderInterface% = USB_Install, USB\VID_18D1&PID_4EE0
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4EE2&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4EE4&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4EE6&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4EE7

;Google Glass
%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_9001
%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_9001&MI_01

;FUJITSU SP(GLF)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1560&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1561&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1562&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1563&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1564&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1565&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1566&MI_02

;FUJITSU SP(SLV)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1536&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1537&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1538&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1567&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1539&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_153A&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_153B&MI_02

;FUJITSU SP(SQM)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_154E&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_154F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1550&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1551&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1552&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1553&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1554&MI_02

;FUJITSU SP(LAM)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1547&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1548&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1549&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_154A&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_154B&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_154C&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_154D&MI_02

;FUJITSU SP(SQD)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1530&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1531&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1532&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1546&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1533&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1534&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1535&MI_02

;FUJITSU SP(LAT)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_152A&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_152B&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_152C&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1545&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_152D&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_152E&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_152F&MI_02

;FUJITSU SP(FJB)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1510&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1511&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1512&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1513&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1514&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1515&MI_02

;FUJITSU SP(TNM)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1505&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1506&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1507&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1508&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1509&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_150A&MI_02

;FUJITSU SP(CGM)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14FF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1500&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1501&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1502&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1503&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1504&MI_02

;FUJITSU SP(CGD)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14F9&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14FA&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14FB&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14FC&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14FD&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14FE&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1544&MI_02

;FUJITSU SP(DTM)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14F3&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14F4&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14F5&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14F6&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14F7&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14F8&MI_02

;FUJITSU SP(DTD)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14D4&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14D5&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14D6&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14D7&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14D8&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14D9&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1543&MI_02

;FUJITSU SP(RGB)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14CE&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14CF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14D0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14D1&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14D2&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14D3&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1542&MI_02

;FUJITSU SP(HDA)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14C7&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14C8&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14C9&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14CA&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14CB&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14CC&MI_02

;FUJITSU SP(BRMJ)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_149D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_149E&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_149F&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14A0&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14A1&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_14A2&MI_02

;FUJITSU SP(BRM)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1497&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1498&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1499&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_149A&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_149B&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_149C&MI_02

;FUJITSU SP(BRG)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1491&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1492&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1493&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1494&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1495&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1496&MI_02

;FUJITSU SP(BAL)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_148B&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_148C&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_148D&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_148E&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_148F&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1490&MI_02

;FUJITSU SP(SHC)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1482&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1483&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1484&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1485&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1486&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1487&MI_02

;FUJITSU SP(VOL)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_147C&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_147D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_147E&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_147F&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1480&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1481&MI_02

;FUJITSU SP(ASA)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1457&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1458&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1459&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_145A&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_145B&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_145C&MI_02

;FUJITSU SP(SQU)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_144B&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_144C&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_144D&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_144E&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_144F&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1450&MI_02

;FUJITSU SP(ARG)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1429&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_142A&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_142B&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_142C&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_142D&MI_02

;FUJITSU SP(SPD)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1423&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1424&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1425&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1427&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1428&MI_02

;FUJITSU SP(KJK)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1414&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1415&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1416&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1417&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1418&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1444&MI_03

;FUJITSU SP(DRA)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1419&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_141A&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_141B&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_141D&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_141E&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1442&MI_03

;FUJITSU SP(KJD)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13FB&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13FC&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13FD&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13FE&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13E8&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1420&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1443&MI_03

;FUJITSU SP(HUD)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1403&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1404&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1405&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1406&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1407&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13EA&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1441&MI_03

;FUJITSU SP(CAS)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13FF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1400&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1401&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1402&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13E9&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1421&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1440&MI_03

;FUJITSU SP(LUG)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13F5&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13F6&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13F7&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13F9&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13E7&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_141F&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_143F&MI_03

;FUJITSU SP(HIM)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13D2&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13D3&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13D4&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13D6&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13D1&MI_02

;FUJITSU SP(CAN)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13BE&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13BF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13C0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13C2&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13C3&MI_02

;FUJITSU SP(TMS)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13DD&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13DE&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13DF&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13E0&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13E1&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13E2&MI_02

;FUJITSU SP(LPN)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13CB&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13CC&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13CD&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13CF&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13D0&MI_02

;FUJITSU SP(NAE)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_140E&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_140F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1410&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1411&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1412&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1413&MI_02

;FUJITSU SP(BRK)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_136E&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_136F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1370&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1371&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1372&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1373&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1374&MI_02

;FUJITSU SP(NAS)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1384&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1385&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1386&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1388&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1389&MI_02

;FUJITSU SP(BOD)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1378&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1379&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_137A&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_137C&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_137E&MI_01

;FUJITSU SP(NAD)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_137F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1380&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1381&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1383&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1399&MI_01

;FUJITSU SP(IRUD)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_138E&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_138F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1390&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1392&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1394&MI_01

;FUJITSU SP(IRUJW)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1395&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1396&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1397&MI_02

;FUJITSU SP(LY)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_139E&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_139F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13A0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13A2&MI_03


;FUJITSU SP(TA)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1314&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1315&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_131A&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_131B&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1340&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1340&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1341&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1341&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1317&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1318&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1352&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1353&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1111&MI_02

;FUJITSU SP(AR)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1321&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1322&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1325&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1326&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_133F&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1355&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_136D&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1331&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1332&MI_06
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1333&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_133E&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1324&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_133D&MI_01

;FUJITSU SP(AC)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1342&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1343&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1344&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1346&MI_04

;FUJITSU SP(QFAC)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1112&MI_01

;FUJITSU SP(NDS)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1356&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1357&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1358&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_135A&MI_04

;FUJITSU SP(BGB)
%CompositeAdbInterface%     = USB_Install, USB\VID_04c5&PID_12C8&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04c5&PID_12C9&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04c5&PID_12CA&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04c5&PID_12CB&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04c5&PID_12CC&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04c5&PID_12CD&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04c5&PID_12D8&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04c5&PID_12E4&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_04c5&PID_1337&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04c5&PID_1338&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04c5&PID_1367&MI_01

;FUJITSU SP(SW)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_135E&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_135F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1360&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1362&MI_03

;FUJITSU SP(SHD)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12B4&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12B5&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12E6&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1335&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1365&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1350&MI_01

;FUJITSU SP(ELL)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_131D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_131E&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_131F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_139B&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_139C&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_139D&MI_01

;FUJITSU SP(TRI)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12EF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12F0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12F2&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1336&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1351&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1366&MI_01

;FUJITSU SP(APOK)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12F9&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12FA&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12FB&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12FB&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12FC&MI_06
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12FD&MI_01

;FUJITSU SP(APOD)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12F3&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12F4&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12F5&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_135C&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_135D&MI_01

;FUJITSU SP(SKY)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12E8&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12E9&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12EA&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12EA&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12EB&MI_07
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12EC&MI_01

;FUJITSU SP(BAC)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12B0&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12AF&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12C5&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12C6&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1334&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_1364&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_134F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_131C&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13AF&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_13B0&MI_01

;FUJITSU SP(EIF)
%CompositeAdbInterface%     = USB_Install, USB\VID_04C5&PID_12AB&MI_01

;TOSHIBA T-01C
%CompositeAdbInterface%     = USB_Install, USB\VID_0930&PID_0D85&MI_01
;
;TOSHIBA IS04
%CompositeAdbInterface%     = USB_Install, USB\VID_0930&PID_0D8D&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0930&PID_0D8C&MI_01


[USB_Install]
Include = winusb.inf
Needs   = WINUSB.NT

[USB_Install.Services]
Include     = winusb.inf
AddService  = WinUSB,0x00000002,WinUSB_ServiceInstall

[WinUSB_ServiceInstall]
DisplayName     = %WinUSB_SvcDesc%
ServiceType     = 1
StartType       = 3
ErrorControl    = 1
ServiceBinary   = %12%\WinUSB.sys

[USB_Install.Wdf]
KmdfService = WINUSB, WinUSB_Install

[WinUSB_Install]
KmdfLibraryVersion  = 1.9

[USB_Install.HW]
AddReg  = Dev_AddReg

[Dev_AddReg]
HKR,,DeviceInterfaceGUIDs,0x10000,"{F72FE0D4-CBCB-407d-8814-9ED673D0DD6B}"

[USB_Install.CoInstallers]
AddReg    = CoInstallers_AddReg
CopyFiles = CoInstallers_CopyFiles

[CoInstallers_AddReg]
HKR,,CoInstallers32,0x00010000,"WdfCoInstaller01009.dll,WdfCoInstaller","WinUSBCoInstaller2.dll"

[CoInstallers_CopyFiles]
WinUSBCoInstaller2.dll
WdfCoInstaller01009.dll

[DestinationDirs]
CoInstallers_CopyFiles=11

[SourceDisksNames]
1 = %DISK_NAME%,,,\i386
2 = %DISK_NAME%,,,\amd64

[SourceDisksFiles.x86]
WinUSBCoInstaller2.dll  = 1
WdfCoInstaller01009.dll = 1

[SourceDisksFiles.amd64]
WinUSBCoInstaller2.dll  = 2
WdfCoInstaller01009.dll = 2

[Strings]
ProviderName                = "Google, Inc."
SingleAdbInterface          = "Android ADB Interface"
CompositeAdbInterface       = "Android Composite ADB Interface"
SingleBootLoaderInterface   = "Android Bootloader Interface"
WinUSB_SvcDesc              = "Android USB Driver"
DISK_NAME                   = "Android WinUsb installation disk"
ClassName                   = "Android Device"
