;*********************************************************************************************
; Windows USB Composite Setup File for Intel Android Smartphones
;
; Copyright (c) 2012 Intel Corporation 
;
; For use only on Windows operating systems.
;*********************************************************************************************
[Version] 
Signature 			= "$WINDOWS NT$" 
Class 				= USB 
ClassGUID 			= {36fc9e60-c465-11cf-8056-444553540000} 
Provider 			= %ProviderName% 
DriverVer			= 04/30/2012,1.2.0.0
CatalogFile.NTx86  	= intc_usbcompx86.cat
CatalogFile.NTAMD64 = intc_usbcompamd64.cat

[Manufacturer] 
%ProviderName% 	=	Generic,NTx86,NTamd64
 
[Generic.NTx86]
; Intel Clovertrail Android ICS
%USBCompositeDevice% = Composite.Device,USB\VID_8087&PID_0A16 ; MTP+ADB
%USBCompositeDevice% = Composite.Device,USB\VID_8087&PID_0A18 ; PTP+ADB
%USBCompositeDevice% = Composite.Device,USB\VID_8087&PID_0A1A ; RNDIS+ADB
%USBCompositeDevice% = Composite.Device,USB\VID_8087&PID_0A1B ; RNDIS+ACM+ADB

; Intel Medfield Android ICS
%USBCompositeDevice% = Composite.Device,USB\VID_8087&PID_09FC ; MTP+ADB
%USBCompositeDevice% = Composite.Device,USB\VID_8087&PID_09FE ; PTP+ADB
%USBCompositeDevice% = Composite.Device,USB\VID_8087&PID_09F4 ; RNDIS+ADB
%USBCompositeDevice% = Composite.Device,USB\VID_8087&PID_09F8 ; RNDIS+ACM+ADB

; Intel Medfield Android GB
%USBCompositeDevice% = Composite.Device,USB\VID_8087&PID_09f2 
%USBCompositeDevice% = Composite.Device,USB\VID_8087&PID_09f1 
%USBCompositeDevice% = Composite.Device,USB\VID_8087&PID_09f3 
%USBCompositeDevice% = Composite.Device,USB\VID_8087&PID_09f4 
%USBCompositeDevice% = Composite.Device,USB\VID_8087&PID_09f6

[Generic.NTamd64]
; Intel Clovertrail Android ICS
%USBCompositeDevice% = Composite.Device,USB\VID_8087&PID_0A16 ; MTP+ADB
%USBCompositeDevice% = Composite.Device,USB\VID_8087&PID_0A18 ; PTP+ADB
%USBCompositeDevice% = Composite.Device,USB\VID_8087&PID_0A1A ; RNDIS+ADB
%USBCompositeDevice% = Composite.Device,USB\VID_8087&PID_0A1B ; RNDIS+ACM+ADB

; Intel Medfield Android ICS
%USBCompositeDevice% = Composite.Device,USB\VID_8087&PID_09FC ; MTP+ADB
%USBCompositeDevice% = Composite.Device,USB\VID_8087&PID_09FE ; PTP+ADB
%USBCompositeDevice% = Composite.Device,USB\VID_8087&PID_09F4 ; RNDIS+ADB
%USBCompositeDevice% = Composite.Device,USB\VID_8087&PID_09F8 ; RNDIS+ACM+ADB

; Intel Medfield Android GB
%USBCompositeDevice% = Composite.Device,USB\VID_8087&PID_09f2 
%USBCompositeDevice% = Composite.Device,USB\VID_8087&PID_09f1 
%USBCompositeDevice% = Composite.Device,USB\VID_8087&PID_09f3 
%USBCompositeDevice% = Composite.Device,USB\VID_8087&PID_09f4 
%USBCompositeDevice% = Composite.Device,USB\VID_8087&PID_09f6

[ControlFlags] 
ExcludeFromSelect=* 
 
; Common Class Generic Parent for root ID 
[Composite.Device] 
Include=usb.inf 
Needs=Composite.Dev.NT 
 
[Composite.Device.Services] 
Include=usb.inf 
Needs=Composite.Dev.NT.Services 
 
[SourceDisksNames] 
1=%SourceDisk%,,1 
 
[Strings]
ProviderName 		= "Intel Corporation"
ServiceDisplayName	= "Intel Android USB Composite Device Driver" 
USBCompositeDevice	= "Intel Android USB Composite Device" 
SourceDisk 			= "Intel Android USB Composite Device Install Disk" 
