; Windows Virtual Serial Port Setup File
; Copyright (c) 2009 HTC Corp.
; Manufacturer: HTC Corp.

[Version]
  signature  = "$WINDOWS NT$"
  Class      = Ports
  Provider   = %OEM%
  ClassGuid  = {4D36E978-E325-11CE-BFC1-08002BE10318}
  DriverVer  = 03/02/2009,5.0.0.3
  Catalogfile.NTamd64=HtcVComV64.cat

[Strings]
  OEM                 = "HTC Corporation"
  OEMSRCDISK          = "HTC USB Driver Disk"
  OEMDevice00         = "HTC Diagnostic Interface"
  OEMDevice01         = "HTC Diagnostic Interface"
  OEMDevice02         = "HTC Diagnostic Interface"
  OEMSerialPortName00 = "HTC Diagnostic Port"

[Manufacturer]
  %OEM% = Models, NTamd64

[Models.NTamd64]
%OEMDevice00% = OEMPort00, USB\VID_0BB4&PID_0EFE
%OEMDevice01% = OEMPort00, USB\VID_0BB4&PID_0E01&MI_00
%OEMDevice02% = OEMPort00, USB\VID_0BB4&PID_0E02&MI_00

[SourceDisksNames]
  1000 = %OEMSRCDISK%,"",,

[SourceDisksFiles]
  HtcVComV64.sys = 1000

[ControlFlags]
  ExcludeFromSelect = *

[OEMPort00.NTamd64]
  CopyFiles = FakePortCopyFileSection00
  AddReg = All00, AddReg.NTamd64

[FakePortCopyFileSection00]
  HtcVComV64.sys,,,0x20

[DestinationDirs]
  DefaultDestDir = 12

[OEMPort00.NTamd64.Services]
  AddService = HtcVCom32,  0x00000002, OEMPort_Service_Inst00

[AddReg.NTamd64]
  HKR,,PortSubClass,1,01
  HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"

[All00]
  HKR,,NTMPDriver,,HtcVComV64.sys

[OEMPort_Service_Inst00]
  DisplayName   = %OEMSerialPortName00%
  ServiceType   = 1
  StartType     = 3
  ErrorControl  = 1
  ServiceBinary = %12%\HtcVComV64.sys



