Instruction manual

The configurator is intended to disable unnecessary functions of the HDD and enable previously turned off.

Step 1: Identify
Getting factory HDD configuration. In this case, those items that can be controlled appear.

Step 2: Restore
Before each configuration change, reset the previous Restore button.

Step 3: Set or remove the necessary checkbox-options HDD.

Step 4: Apply - apply settings.
The drive can return an error if you apply an unchanged configuration, apply the configuration without resetting the previous, or restoring the HDD with a configuration that does not differ from the default.

To disable SMART through DCO, you must first disable it through ATA.

Between receiving the configuration and its application - other operations are not allowed (for example, get HDD passport), because shared data buffer is used.

Freeze blocks DCO operation until the power is turned off.

For more details, see hdd.by